earthworks-itp-template | Inspection and Test Plan
[Fill: project name] | Earthworks and excavation inspection and test plan template — free editable baseline | [Fill: Australian state/territory] | Rev 00 | 2026-10-06 | For review
Contractor: [Fill: contractor]    Client: [Fill: client]
Scope: Reusable baseline for site clearing, bulk cut/fill, foundation excavation, subgrade and trench backfill as applicable. Split the plan by material/use zone and identify geotechnical release interfaces. Excludes deep foundations, contaminated-land remediation, blasting, ground improvement and pavement-specific acceptance unless expressly included. This is a free, editable, proposed baseline and is not tailored to a project, approved by a client, or evidence of completed inspection. Before use, complete the scope questions and bracketed fields, confirm every criterion and control against current project documents, and remove non-applicable rows.
Exclusions: Confirm exclusions for this project; use the scope notes above.
	ID
	Stage
	Inspection / test
	Method
	Acceptance requirement
	Reference
	Frequency
	Responsible role
	Point
	Approval / witness party
	Notice / release
	Record
	Remarks

	EAR-01
	Planning and geotechnical basis
	Proposed: baseline — Confirm earthworks zones, cut/fill limits, geotechnical design, material classes, lot/testing rules and service constraints.
	Proposed: baseline — Review current drawings, geotechnical report, specification, survey control, services information and approved work method.
	Proposed: baseline — Current documents define [Fill: Scope / earthworks zones], [Fill: Material classification / acceptance], [Fill: Compaction criteria], [Fill: Lot size / test frequency] and [Fill: Design geometry, survey tolerances and deliverables]; identify conflicts and missing geotechnical dispositions.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS04, HUTCHIES-SUITE
	Proposed: Before clearing, excavation or fill placement.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Earthworks document and lot plan
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	EAR-02
	Survey control and set-out
	Proposed: baseline — Verify survey control, limits, formation levels and service/set-out references before disturbance.
	Proposed: baseline — Check control marks and survey set-out against approved drawings and survey plan.
	Proposed: baseline — Control points are current and protected; limits and levels match [Fill: Set-out / tolerances]; conflicts with services or boundaries are resolved before excavation.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS04, HUTCHIES-SUITE
	Proposed: Before starting each area and after control disturbance.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Survey control and set-out record
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	EAR-03
	Service clearance and permits
	Proposed: baseline — Confirm service searches, locating, permits and protection/diversion arrangements for the planned excavation.
	Proposed: baseline — Review current service plans and clearance permits; record field locating/marking and required authority releases.
	Proposed: baseline — Required services are located/protected and permits/clearances for [Fill: Earthworks activity and physical boundaries] are current before excavation; unknown services stop affected work for instruction.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS04, HUTCHIES-SUITE
	Proposed: Before ground penetration in each work area.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Services clearance / excavation permit
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	EAR-04
	Clearing and topsoil stripping
	Proposed: baseline — Check clearing boundaries, topsoil/vegetation stripping, salvage and stockpile locations.
	Proposed: baseline — Observe limits and compare stripped material handling with environmental and earthworks requirements.
	Proposed: baseline — Work remains within [Fill: Clearing / topsoil handling limits]; topsoil and unsuitable material are segregated, identified and stored/disposed as specified.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS04
	Proposed: Each clearing/stripping area before bulk excavation or fill.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Clearing and stripping checklist
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	EAR-05
	Unsuitable material and groundwater
	Proposed: baseline — Identify soft, wet, contaminated or otherwise unsuitable material and unexpected groundwater during excavation.
	Proposed: baseline — Visual inspection and geotechnical review where required; record extent, photographs, removal and replacement instructions.
	Proposed: baseline — Unexpected conditions are referred under [Fill: Geotechnical referral and release process]; removal limits and replacement material are documented before covering.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS04, HUTCHIES-SUITE
	Proposed: Continuously as excavation exposes changed ground; before replacement.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Unsuitable material / geotechnical disposition record
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	EAR-06
	Excavation dimensions and formation
	Proposed: baseline — Check excavation limits, lines, levels, stability and formation against drawings/geotechnical requirements.
	Proposed: baseline — Measure/survey formation and inspect condition; involve geotechnical engineer where specified.
	Proposed: baseline — Excavation geometry matches [Fill: Excavation geometry / level criteria] and founding condition meets documented [Fill: Founding condition / bearing criteria]; changed conditions receive written disposition before blinding/fill/structure.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS04, HUTCHIES-SUITE
	Proposed: Each foundation/formation area before covering or placing over.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Excavation and formation release
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	EAR-07
	Fill source and material approval
	Proposed: baseline — Verify source, classification, sampling and approval for each proposed fill material.
	Proposed: baseline — Review source approval and lab classification/test certificates; reconcile delivered material with approved source/material ID.
	Proposed: baseline — Material is approved for [Fill: Fill use / zone] and meets [Fill: Required material properties]; any source or material change is approved and tested before placement.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS04, HUTCHIES-SUITE
	Proposed: Each source/material type and source change before use.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Fill material approval register
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	EAR-08
	Subgrade preparation and proof condition
	Proposed: baseline — Check exposed subgrade is trimmed, drained and free from unacceptable disturbance before placing fill or pavement layers.
	Proposed: baseline — Visual walkover and specified proof roll or geotechnical inspection; record soft spots and remediation.
	Proposed: baseline — Subgrade matches [Fill: Subgrade condition / proof criteria] and any required proof/engineer release is documented; remedial areas are retested or re-released.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS04, HUTCHIES-SUITE
	Proposed: Each work area before first fill/pavement layer.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Subgrade inspection and release
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	EAR-09
	Fill placement layer controls
	Proposed: baseline — Check placed material type, placement area, loose layer thickness and segregation before compaction.
	Proposed: baseline — Observe placement; measure layer thickness and compare material and equipment/work method with approved trial or specification.
	Proposed: baseline — Material matches approved source; layer and method comply with [Fill: Layer thickness / method criteria] and project/geotechnical requirements.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS04, HUTCHIES-SUITE
	Proposed: Each layer, area and material change before compaction.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Layer placement log
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	EAR-10
	Moisture conditioning and compaction
	Proposed: baseline — Verify moisture conditioning and compaction method are appropriate to approved material and project requirement.
	Proposed: baseline — Observe water addition/aeration and compaction passes/equipment; record method where required by project.
	Proposed: baseline — Conditioning and compaction follow [Fill: Compaction / moisture conditioning method] for the approved material; do not infer target moisture or density.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS04, HUTCHIES-SUITE
	Proposed: Each layer and material/condition change.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Compaction process log
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	EAR-11
	In-situ density and material testing
	Proposed: baseline — Arrange specified field/lab testing and link each result to the correct lot, layer, location and material.
	Proposed: baseline — Use project-nominated methods and qualified/lab personnel; map test locations and compare results with exact project limits.
	Proposed: baseline — Test method, rate, lot coverage and acceptance match [Fill: Density / compaction limits] and [Fill: Lot/test frequency]; failed/invalid tests trigger documented rework and retest.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS04, HUTCHIES-SUITE
	Proposed: At project-defined rate for each applicable lot/layer/material.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Earthworks lot and test register
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	EAR-12
	Nonconformance, rework and retest
	Proposed: baseline — Track failed tests, unsuitable areas and corrective work through acceptable retest or written disposition.
	Proposed: baseline — Review test/NCR records, identify affected lot and layer, verify rework boundaries and retest.
	Proposed: baseline — Affected work is not covered or released until retest meets [Fill: Compaction acceptance values and test methods by zone/material] or a documented authorised disposition is issued; preserve test-to-lot traceability.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS04
	Proposed: For each failure/deviation before covering subsequent layer.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Earthworks NCR and retest register
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	EAR-13
	Trench backfill and reinstatement
	Proposed: baseline — Check bedding, haunch/side support, pipe protection and backfill material/layers for trench works.
	Proposed: baseline — Inspect before concealment and record material, layer placement, specified compaction tests and surface reinstatement.
	Proposed: baseline — Trench components and backfill comply with [Fill: Trench zone materials / compaction / cover criteria]; record service owner/inspection release and test evidence before cover.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS04, HUTCHIES-SUITE
	Proposed: Each trench section before cover and at specified compaction lot stages.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Trench backfill and pre-cover record
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	EAR-14
	Drainage, erosion and water management
	Proposed: baseline — Check temporary drainage, dewatering, erosion/sediment controls and protection of completed formation/fill.
	Proposed: baseline — Inspect controls before and during work and after rainfall/change events against approved environmental/site plans.
	Proposed: baseline — Controls and discharge arrangements match [Fill: Water / erosion control requirements]; erosion, contamination or softening is corrected and affected work reassessed before acceptance.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS04, HUTCHIES-SUITE
	Proposed: Before disturbance, during active work and after triggering weather/events as project specifies.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Water and erosion control inspection log
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	EAR-15
	Final levels, geometry and closeout
	Proposed: baseline — Survey completed surfaces, batters, slopes, formation and interfaces; compile material, lot and test records.
	Proposed: baseline — Survey/measure against final design and compare register for all lots, nonconformances and geotechnical releases.
	Proposed: baseline — Final geometry meets [Fill: As-built tolerances / survey coverage]; every lot has linked test/acceptance evidence and open deviations have approved disposition before handover.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS04, HUTCHIES-SUITE
	Proposed: Each completed zone before subsequent work / package closeout.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Earthworks as-built survey and lot closeout register
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.



Inspection point key
Inspection point key: H = Proposed Hold Point - use only if assigned in the contract | W = Proposed Witness Point - use only if assigned in the contract | R = Proposed Review | S = Proposed Surveillance | TBC = To be confirmed | N/A = Not applicable. External H/W rights and whether work may proceed are governed by the project contract and approved process; proposed points require agreement.


Blank Inspection Record Forms
[Fill: project name] | earthworks-itp-template | Record actual observations during the work. No results or signatures are pre-filled.
	ITP ID / Stage
	Inspection / method / acceptance
	Location / lot
	Date and result
	Evidence / record ref.
	Performed by / signature
	Reviewed by / signature

	EAR-01 | Planning and geotechnical basis
	Proposed: baseline — Confirm earthworks zones, cut/fill limits, geotechnical design, material classes, lot/testing rules and service constraints.
Method: Proposed: baseline — Review current drawings, geotechnical report, specification, survey control, services information and approved work method.
Accept when: Proposed: baseline — Current documents define [Fill: Scope / earthworks zones], [Fill: Material classification / acceptance], [Fill: Compaction criteria], [Fill: Lot size / test frequency] and [Fill: Design geometry, survey tolerances and deliverables]; identify conflicts and missing geotechnical dispositions.
Record: Earthworks document and lot plan
	
	Date: __________
Document title / number: __________
Revision / issue date: __________
Geotechnical report reference: __________
Lot/testing plan reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	EAR-02 | Survey control and set-out
	Proposed: baseline — Verify survey control, limits, formation levels and service/set-out references before disturbance.
Method: Proposed: baseline — Check control marks and survey set-out against approved drawings and survey plan.
Accept when: Proposed: baseline — Control points are current and protected; limits and levels match [Fill: Set-out / tolerances]; conflicts with services or boundaries are resolved before excavation.
Record: Survey control and set-out record
	
	Date: __________
Area / chainage: __________
Control mark ID: __________
Design level (m): __________
Set-out level (m): __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	EAR-03 | Service clearance and permits
	Proposed: baseline — Confirm service searches, locating, permits and protection/diversion arrangements for the planned excavation.
Method: Proposed: baseline — Review current service plans and clearance permits; record field locating/marking and required authority releases.
Accept when: Proposed: baseline — Required services are located/protected and permits/clearances for [Fill: Earthworks activity and physical boundaries] are current before excavation; unknown services stop affected work for instruction.
Record: Services clearance / excavation permit
	
	Date: __________
Service type / owner: __________
Marked location: __________
Permit / clearance ref: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	EAR-04 | Clearing and topsoil stripping
	Proposed: baseline — Check clearing boundaries, topsoil/vegetation stripping, salvage and stockpile locations.
Method: Proposed: baseline — Observe limits and compare stripped material handling with environmental and earthworks requirements.
Accept when: Proposed: baseline — Work remains within [Fill: Clearing / topsoil handling limits]; topsoil and unsuitable material are segregated, identified and stored/disposed as specified.
Record: Clearing and stripping checklist
	
	Date: __________
Area / chainage: __________
Stripped depth (mm): __________
Stockpile ID/location: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	EAR-05 | Unsuitable material and groundwater
	Proposed: baseline — Identify soft, wet, contaminated or otherwise unsuitable material and unexpected groundwater during excavation.
Method: Proposed: baseline — Visual inspection and geotechnical review where required; record extent, photographs, removal and replacement instructions.
Accept when: Proposed: baseline — Unexpected conditions are referred under [Fill: Geotechnical referral and release process]; removal limits and replacement material are documented before covering.
Record: Unsuitable material / geotechnical disposition record
	
	Date: __________
Location / depth: __________
Extent / volume (m³): __________
Observed condition: __________
Geotechnical instruction ref: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	EAR-06 | Excavation dimensions and formation
	Proposed: baseline — Check excavation limits, lines, levels, stability and formation against drawings/geotechnical requirements.
Method: Proposed: baseline — Measure/survey formation and inspect condition; involve geotechnical engineer where specified.
Accept when: Proposed: baseline — Excavation geometry matches [Fill: Excavation geometry / level criteria] and founding condition meets documented [Fill: Founding condition / bearing criteria]; changed conditions receive written disposition before blinding/fill/structure.
Record: Excavation and formation release
	
	Date: __________
Area / footing ID: __________
Formation level (m): __________
Depth (m): __________
Geotechnical release ref: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	EAR-07 | Fill source and material approval
	Proposed: baseline — Verify source, classification, sampling and approval for each proposed fill material.
Method: Proposed: baseline — Review source approval and lab classification/test certificates; reconcile delivered material with approved source/material ID.
Accept when: Proposed: baseline — Material is approved for [Fill: Fill use / zone] and meets [Fill: Required material properties]; any source or material change is approved and tested before placement.
Record: Fill material approval register
	
	Date: __________
Source / quarry: __________
Material / class: __________
Sample / report ID: __________
Approval reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	EAR-08 | Subgrade preparation and proof condition
	Proposed: baseline — Check exposed subgrade is trimmed, drained and free from unacceptable disturbance before placing fill or pavement layers.
Method: Proposed: baseline — Visual walkover and specified proof roll or geotechnical inspection; record soft spots and remediation.
Accept when: Proposed: baseline — Subgrade matches [Fill: Subgrade condition / proof criteria] and any required proof/engineer release is documented; remedial areas are retested or re-released.
Record: Subgrade inspection and release
	
	Date: __________
Area / chainage: __________
Proof method: __________
Soft spot / treatment: __________
Release reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	EAR-09 | Fill placement layer controls
	Proposed: baseline — Check placed material type, placement area, loose layer thickness and segregation before compaction.
Method: Proposed: baseline — Observe placement; measure layer thickness and compare material and equipment/work method with approved trial or specification.
Accept when: Proposed: baseline — Material matches approved source; layer and method comply with [Fill: Layer thickness / method criteria] and project/geotechnical requirements.
Record: Layer placement log
	
	Date: __________
Lot ID: __________
Layer number: __________
Material ID: __________
Loose thickness (mm): __________
Compaction plant: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	EAR-10 | Moisture conditioning and compaction
	Proposed: baseline — Verify moisture conditioning and compaction method are appropriate to approved material and project requirement.
Method: Proposed: baseline — Observe water addition/aeration and compaction passes/equipment; record method where required by project.
Accept when: Proposed: baseline — Conditioning and compaction follow [Fill: Compaction / moisture conditioning method] for the approved material; do not infer target moisture or density.
Record: Compaction process log
	
	Date: __________
Lot ID: __________
Layer number: __________
Conditioning action: __________
Plant / passes: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	EAR-11 | In-situ density and material testing
	Proposed: baseline — Arrange specified field/lab testing and link each result to the correct lot, layer, location and material.
Method: Proposed: baseline — Use project-nominated methods and qualified/lab personnel; map test locations and compare results with exact project limits.
Accept when: Proposed: baseline — Test method, rate, lot coverage and acceptance match [Fill: Density / compaction limits] and [Fill: Lot/test frequency]; failed/invalid tests trigger documented rework and retest.
Record: Earthworks lot and test register
	
	Date: __________
Lot ID: __________
Layer number: __________
Test location / coordinates: __________
Test method: __________
Measured result: __________
Applicable criterion: __________
Lab report ID: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	EAR-12 | Nonconformance, rework and retest
	Proposed: baseline — Track failed tests, unsuitable areas and corrective work through acceptable retest or written disposition.
Method: Proposed: baseline — Review test/NCR records, identify affected lot and layer, verify rework boundaries and retest.
Accept when: Proposed: baseline — Affected work is not covered or released until retest meets [Fill: Compaction acceptance values and test methods by zone/material] or a documented authorised disposition is issued; preserve test-to-lot traceability.
Record: Earthworks NCR and retest register
	
	Date: __________
NCR ID: __________
Affected lot/layer: __________
Rework performed: __________
Retest report / result: __________
Approval reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	EAR-13 | Trench backfill and reinstatement
	Proposed: baseline — Check bedding, haunch/side support, pipe protection and backfill material/layers for trench works.
Method: Proposed: baseline — Inspect before concealment and record material, layer placement, specified compaction tests and surface reinstatement.
Accept when: Proposed: baseline — Trench components and backfill comply with [Fill: Trench zone materials / compaction / cover criteria]; record service owner/inspection release and test evidence before cover.
Record: Trench backfill and pre-cover record
	
	Date: __________
Chainage / section: __________
Bedding material / thickness: __________
Cover / level: __________
Density test report / result: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	EAR-14 | Drainage, erosion and water management
	Proposed: baseline — Check temporary drainage, dewatering, erosion/sediment controls and protection of completed formation/fill.
Method: Proposed: baseline — Inspect controls before and during work and after rainfall/change events against approved environmental/site plans.
Accept when: Proposed: baseline — Controls and discharge arrangements match [Fill: Water / erosion control requirements]; erosion, contamination or softening is corrected and affected work reassessed before acceptance.
Record: Water and erosion control inspection log
	
	Date: __________
Area: __________
Control inspected: __________
Rain/event/time: __________
Action / closeout: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	EAR-15 | Final levels, geometry and closeout
	Proposed: baseline — Survey completed surfaces, batters, slopes, formation and interfaces; compile material, lot and test records.
Method: Proposed: baseline — Survey/measure against final design and compare register for all lots, nonconformances and geotechnical releases.
Accept when: Proposed: baseline — Final geometry meets [Fill: As-built tolerances / survey coverage]; every lot has linked test/acceptance evidence and open deviations have approved disposition before handover.
Record: Earthworks as-built survey and lot closeout register
	
	Date: __________
Zone / chainage: __________
Design level (m): __________
As-built level (m): __________
Survey report ref: __________
Lot closeout ref: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	





Source Register
	Source ID
	Title / filename
	Revision
	Type
	Path / URL

	NSW-QMG
	NSW Government Quality Management Guidelines for Construction, Appendix D (ITP guidance)
	See linked source; verify current edition and project adoption
	guidance
	https://www.info.buy.nsw.gov.au/resources/construction/quality-management-guidelines-for-construction

	TMR-MRTS04
	Queensland TMR MRTS04 General Earthworks (March 2025)
	See linked source; verify current edition and project adoption
	guidance
	https://www.tmr.qld.gov.au/_/media/busind/techstdpubs/specifications-and-drawings/specifications/3-roadworks-drainage-culverts-and-geotechnical/mrts04.pdf?extension=pdf&hash=840B4677F54FF4F65E5C80A7EF563206&rev=d832abe7f4fb4ca1bb13425291c3faca&sc_lang=en&size=2763810

	HUTCHIES-SUITE
	Hutchinson Builders, Construction ITPs and Reports suite (downloadable Word examples)
	See linked source; verify current edition and project adoption
	guidance
	https://subbies.hutchies.com.au/resources/videos/safety-and-quality-planning



Open Confirmations
	Issue ID
	Priority
	ITP rows
	Open item
	Action needed

	CONF-001
	confirmation
	EAR-01
	EAR-01: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-002
	confirmation
	EAR-02
	EAR-02: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-003
	confirmation
	EAR-03
	EAR-03: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-004
	confirmation
	EAR-04
	EAR-04: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-005
	confirmation
	EAR-05
	EAR-05: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-006
	confirmation
	EAR-06
	EAR-06: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-007
	confirmation
	EAR-07
	EAR-07: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-008
	confirmation
	EAR-08
	EAR-08: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-009
	confirmation
	EAR-09
	EAR-09: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-010
	confirmation
	EAR-10
	EAR-10: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-011
	confirmation
	EAR-11
	EAR-11: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-012
	confirmation
	EAR-12
	EAR-12: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-013
	confirmation
	EAR-13
	EAR-13: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-014
	confirmation
	EAR-14
	EAR-14: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-015
	confirmation
	EAR-15
	EAR-15: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.







