CAVOREN  |  FIELD RECORD
Electrical Rough-In Inspection Record
Blank project field record  |  Complete from current approved documents and site observations
Scope
Included: Visual and document checks of identified ordinary low-voltage rough-in work while accessible: route and circuit identity, support/protection, separation and interfaces, penetrations/fire-stopping coordination, enclosure condition and concealment evidence.
Excluded: Electrical design; conductor or protective-device selection/sizing; testing, commissioning, energisation or certification; high voltage, hazardous areas, PV/battery or specialist installations; and universal spacing, support interval, depth, separation or fire-rating values.
Use and project setup
Project field: Project / jurisdiction / contractor  ______________________________________________
Project field: Area / level / room / grid  ______________________________________________
Project field: Drawing / revision / circuit schedule ref  ______________________________________________
Project field: Circuit / cable / containment identity  ______________________________________________
Project field: Origin and destination / board reference  ______________________________________________
Project field: Concealment stage / inspection notice  ______________________________________________
Project field: Penetration / fire compartment / interface refs  ______________________________________________
Project field: Photo / NCR / RFI / disposition refs  ______________________________________________
Before inspection: Approved electrical drawings, schedules and specifications — Identify design intent, routes, circuits, cable and containment requirements and revision.
Before inspection: Current coordination and fire-compartment details — Locate interfaces, penetrations, separation and required fire-stopping detail.
Before inspection: Project inspection and concealment schedule — Identify notice, witness and release roles before work becomes inaccessible.
Before inspection: Product approvals and installation instructions — Verify installed cable, containment, supports and protection against accepted submittals.
Before inspection: Electrical contractor work method and risk controls — Define qualified personnel, access controls and safe inspection arrangements.
How to use
1. Identify jurisdiction, exact installation/work boundary and current controlled drawing revision.
2. Enter applicable project acceptance references, methods, limits, witness points and responsible roles from approved project documents; no defaults are supplied.
3. Record actual observations/results only from contemporaneous work or issued reports, retaining units, report IDs and revisions.
4. Maintain a dated, attributable event trail for defects, repair, retest and disposition; preserve earlier entries.
5. Keep project release, statutory certificate, inspector sign-off or connection authorisation as separate evidence linked by reference.
Important: Blank field record for ordinary building low-voltage electrical work only. Project documents and applicable state or territory requirements control. This record is neither a statutory certificate, electrical test certification, inspector approval nor authorisation to connect or energise. Do not perform electrical work or tests unless appropriately licensed/authorised. Actual results, dates, decisions and signatures remain blank until contemporaneous evidence is entered by the responsible person.


Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	RIR-01  Area, circuit and drawing identity


	What to observe
	Area, level, circuit or cable ID, origin/destination and current drawing/schedule revision.

	How to check
	Trace visible work to approved drawing and circuit schedule; note deviations for disposition.

	Acceptance basis
	Installed extent is identifiable and checked against current approved design documents.

	Reference to verify
	Approved project electrical specification, jurisdictional rules, drawings and controlled test/inspection plan; record exact revision/clause.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Area / circuit
	



	Drawing revision
	



	Origin / destination
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	RIR-02  Route, supports and mechanical protection


	What to observe
	Visible route, containment type, support arrangement, edge protection and exposure to damage.

	How to check
	Compare installed arrangement to project details and approved product instructions; record locations without generic intervals.

	Acceptance basis
	Project-specified support and protection are evidenced for this route.

	Reference to verify
	Approved project electrical specification, jurisdictional rules, drawings and controlled test/inspection plan; record exact revision/clause.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Route / containment
	



	Support / protection detail
	



	Photo / deviation ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	RIR-03  Segregation and service interfaces


	What to observe
	Proximity/crossings with other services, incompatible systems, access zones and later trade interfaces.

	How to check
	Compare interface to coordinated approved drawings and project requirements; document unresolved crossings.

	Acceptance basis
	Required project separation and interface treatment are traceable.

	Reference to verify
	Approved project electrical specification, jurisdictional rules, drawings and controlled test/inspection plan; record exact revision/clause.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Crossing / interface
	



	Coordination drawing
	



	Disposition ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	RIR-04  Penetrations and fire-compartment interfaces


	What to observe
	Penetration location, affected barrier identity and specified fire-stopping system/status.

	How to check
	Match penetration to current fire strategy/detail and approved system submittal; record fire-stop evidence separately.

	Acceptance basis
	Penetration treatment is traceable to approved project documents.

	Reference to verify
	Approved project electrical specification, jurisdictional rules, drawings and controlled test/inspection plan; record exact revision/clause.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Penetration ID
	



	Barrier/detail ref
	



	Fire-stop submittal
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	RIR-05  Cable / enclosure condition and ends


	What to observe
	Visible damage, contamination, open ends, identification and protection at exposed terminations.

	How to check
	Visually inspect accessible work and compare identification/protection to project requirements; no electrical testing implied.

	Acceptance basis
	No unresolved visible damage or identification issue remains for this extent.

	Reference to verify
	Approved project electrical specification, jurisdictional rules, drawings and controlled test/inspection plan; record exact revision/clause.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Cable / enclosure ID
	



	Observed defect
	



	Repair ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	RIR-06  Concealment notice and evidence handover


	What to observe
	Inspection request, witness requirement, open issues, photo coverage and authorised project release reference.

	How to check
	Reconcile notice and required witness with project inspection plan; record release evidence from assigned role.

	Acceptance basis
	Project-required pre-cover evidence and decisions are linked before concealment.

	Reference to verify
	Approved project electrical specification, jurisdictional rules, drawings and controlled test/inspection plan; record exact revision/clause.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Notice / witness ref
	



	Open items
	



	Release decision ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Electrical Rough-In Inspection Record event log
Use one row per defined area/circuit/check event. Keep project criteria separate from actual observations and reported results. Preserve failed and superseded entries; link every decision to its authorised role and separate evidence. This log does not certify work or authorise connection.
Project / contract: ______________________________    Element / pour / lot: ______________________________    Date / shift: ____________________
Location / area: ______________________________    Record reference / revision: ______________________________
	Date / event
	Area / board / circuit
	Drawing / revision
	Check / test category
	Project method / criterion ref
	Actual result / unit or observation
	Report / photo / NCR ref
	Action / retest / disposition
	Role / reviewer / authority ref
	Status / handover ref

	 
	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 
	 




Issues and corrective action
Project: _____________________  Location / room / element: _____________________  Inspection date: _____________________
	Item / date
	Issue and immediate action
	Disposition / corrective instruction
	Recheck evidence / date
	Responsible role / reference

	


	


	


	


	



	


	


	


	


	



	


	


	


	


	



	


	


	


	


	



	


	


	


	


	




Unresolved items: identify affected area, status, person notified, instruction / NCR reference and any condition before concealment or next work.


Electrical work evidence handover
Project: _____________________  Location / room / element: _____________________  Date: _____________________
Record evidence status
[  ] Evidence linked for assigned reviewer
[  ] Defect / required test / report remains open
[  ] Separate statutory, inspector, network or project decision required
This field record preserves inspection and document references. It is not a statutory certificate, test certification, inspector sign-off, project release or authority to connect/energise.
Handover roles and references
Installer / authorised electrical worker / scope and date  ______________________________________________
Field recorder / role / evidence reference  ______________________________________________
Electrical contractor responsible person / licence or authorisation ref  ______________________________________________
Inspector / regulator / network approval reference where applicable  ______________________________________________
Project reviewer / disposition reference  ______________________________________________
Open defects / retest / as-built references  ______________________________________________
Signatures record the named person’s stated role and entry only. They do not by themselves approve design, certify compliance, release a contractual control point or authorize the next activity.


Source notes
These references explain topic and record design. They do not supply universal project acceptance values. Confirm the contract documents, applicable jurisdiction and approved product/system before use.
Queensland Electrical Safety Office, Guidelines for testing low voltage electrical installations (2026)
Role: Queensland technical guidance; it does not set project criteria or authorise unqualified persons to test.
Locator: 2026 guide, visual inspection before mandatory tests and verification sections. Used for evidence categories and sequence context only.
Source URL: https://www.worksafe.qld.gov.au/__data/assets/pdf_file/0026/158525/guide-for-testing-low-voltage-electrical-installations.pdf
WorkSafe Queensland, Electrical safety in the construction industry
Role: Queensland jurisdictional guidance informing role and construction context.
Locator: Construction electrical safety: electrical work by licensed/authorised persons; construction wiring inspection/testing by a qualified person before use.
Source URL: https://www.worksafe.qld.gov.au/safety-and-prevention/hazards/electricity/industry-specific-electrical-hazards/electrical-safety-in-the-construction-industry
WorkSafe Queensland, Issuing certificates of compliance
Role: State-specific statutory certificate context. This record is expressly not that certificate.
Locator: Certificate of testing and compliance requirements for installation work and responsible issuer under Queensland rules.
Source URL: https://www.worksafe.qld.gov.au/laws-and-compliance/electrical-safety-laws/issuing-certificates-of-compliance
Energy Safe Victoria, Electrical installation FAQ
Role: Victoria-specific process example, subject to jurisdiction and work classification.
Locator: Testing and inspection; prescribed work inspection before connection, including main switchboard example.
Source URL: https://www.energysafe.vic.gov.au/industry-guidance/electrical/frequently-asked-questions/electrical-installation
Energy Safe Victoria, Prescribed and non-prescribed work
Role: Victoria-specific statutory boundary; not generalized to other jurisdictions.
Locator: Prescribed installation work inspection, including consumer mains, main earthing and relevant main switchboard components.
Source URL: https://www.energysafe.vic.gov.au/certificates-electrical-safety/obligations-and-guidelines/prescribed-and-non-prescribed-work
https://itp.cavoren.net/checklists/electrical-rough-in/  |  Project: __________________________  |  Page 




