CAVOREN  |  FIELD RECORD
Formwork Inspection Checklist
Blank project field record  |  Complete from current approved documents and site observations
Scope
Included: Installed formwork and associated falsework for ordinary cast-in-place slabs, pad footings and strip footings, before loading/concrete placement against project temporary-works documents.
Excluded: Temporary-works design/capacity calculations, independent design certification, complex suspended falsework, bridges/highways special provisions, jump/slip/travelling forms, major lift design, prestressing, demolition/stripping/load release and whole-pour release.
Use and project setup
Project field: Project / contractor  ______________________________________________
Project field: Element / formwork zone  ______________________________________________
Project field: Pour or lot reference  ______________________________________________
Project field: Inspection date  ______________________________________________
Project field: Temporary-works drawing / revision  ______________________________________________
Project field: Formwork system identifier  ______________________________________________
Before inspection: Element, formwork zone, pour/lot and system identifier — Makes the inspected assembly/configuration traceable.
Before inspection: Approved temporary-works drawings, system details and revision — Defines installed arrangement and inspection basis.
Before inspection: Design assumptions, support evidence and required independent check records — Allows checking that documents match visible conditions without recalculating capacity.
Before inspection: Structural/formwork geometry and project dimensional criteria — Provides project dimensions and tolerances for measurements.
Before inspection: Current pour method, access/SWMS and change-control procedure — Connects inspection to placement, loads, safe access and field-change escalation.
How to use
1. Define assembly boundary and gather controlled drawings, system instructions, structural interfaces, pour method and safety plan.
2. Inspect installed configuration and interfaces at work location; record component IDs and measurements against cited documents.
3. Keep design/check evidence separate from observations; do not infer capacity visually.
4. If system, support, loading, geometry or access differs from documents, identify change and refer under project change control.
5. Transfer any release decision to assigned authority and contractual ITP; this checklist does not authorize stripping.
Important: Blank field checklist for project adaptation. Use actual approved documents and project acceptance criteria. Record only observations made. This is not design approval, a temporary-works certificate, contractual Hold/Witness Point release, or permission to place, strip or load.


Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	FW-01  Work package documents and design-check status


	What to observe
	Identify element/boundary, current temporary-works drawings, design revision, erection sequence and required independent check/submission records.

	How to check
	Compare work area with controlled document register; verify status and that check records apply to actual system/configuration.

	Acceptance basis
	Use project temporary-works procedure, approved drawings, specification and contract points; cite design/check status without treating field inspection as design approval.

	Reference to verify
	Controlled temporary-works register, approved drawings, project procedure and required design/check records.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	element / formwork zone
	



	drawing / rev
	



	design-check record ref
	



	open query / response
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	FW-02  System components and visible condition


	What to observe
	Observe form face/framing, proprietary components, ties/connectors and reused parts for damage, deformation, corrosion, omissions or unapproved mixed systems.

	How to check
	Walk accessible faces and compare system identifiers/components with approved drawings, supplier details and inspection points.

	Acceptance basis
	Use approved project system/component schedule; damaged/reused component criteria come from project designer/manufacturer.

	Reference to verify
	Approved system/component schedule, manufacturer instructions and project condition/disposition criteria.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	system / component ID
	



	location / condition
	



	detail / drawing ref
	



	photo / disposition ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	FW-03  Bearing, support and founding interface


	What to observe
	Observe base plates, sole plates, bearers, props and actual ground/slab contact, including settlement, voids, disturbance or unplanned load transfer.

	How to check
	Inspect support points against approved details and project ground/floor information; record location and movement signs.

	Acceptance basis
	Use project design assumptions, approved support/founding detail and required ground/slab verification; no bearing capacity or prop load is set.

	Reference to verify
	Approved support/founding details, design assumptions and project ground/slab verification.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	support ID / location
	



	bearing detail ref
	



	contact / movement
	



	verification / direction ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	FW-04  Line, level, dimensions and formed profile


	What to observe
	Check installed form surface/edges against element geometry and setting-out information, including openings/steps in this package.

	How to check
	Measure project-designated points with identified instruments; record readings, grid/offset and drawing/detail.

	Acceptance basis
	Use approved structural/formwork drawings and project tolerances; do not use generic dimensional limits.

	Reference to verify
	Approved structural and formwork drawings and project dimensional criteria.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	grid / point
	



	criterion / drawing ref
	



	instrument / method
	



	actual / unit / recheck
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	FW-05  Joints, sealing and concrete-loss paths


	What to observe
	Inspect panel joints, corners, stop-ends, kickers, penetrations and closures for gaps, movement paths and sealing per approved detail/method.

	How to check
	Visually inspect joints and compare materials/detail with temporary-works drawings and pour method; photograph suspected leakage paths.

	Acceptance basis
	Use approved project joint/sealing detail and placement method; no generic gap limit or sealant prescription applies.

	Reference to verify
	Approved joint/sealing details and concrete placement method.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	joint / location
	



	detail / material ref
	



	seal condition
	



	repair / recheck ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	FW-06  Bracing, ties, connections and restraint fit


	What to observe
	Observe braces, ties, wedges, pins, clamps and connections for presence, orientation/engagement and visible damage against approved arrangement.

	How to check
	Inspect drawing-identified points; compare component and installation with system instructions/project erection details.

	Acceptance basis
	Use approved temporary-works design and manufacturer/project details; do not infer spacing, torque, capacity or allowable deflection.

	Reference to verify
	Approved bracing/tie/connection details and applicable system installation instructions.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	connection / location
	



	system detail ref
	



	engagement / defect
	



	direction / recheck ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	FW-07  Cast-in openings and interface coordination


	What to observe
	Check voids, block-outs, stop-ends or form interfaces shown on coordinated project drawings and within formwork package.

	How to check
	Compare with current structural/coordination details; verify secure fixing and no unapproved cuts/alterations to system.

	Acceptance basis
	Use approved coordinated drawings and temporary-works details; field-cut penetrations require approvals set by project design process.

	Reference to verify
	Approved coordination/opening drawings and temporary-works alteration details.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	opening / grid
	



	coordination drawing ref
	



	position / dimensions
	



	response / recheck ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	FW-08  Access, edge protection and work-stage safety interface


	What to observe
	Observe access route, working platform, edge/opening protection and safe arrangement relevant to inspecting/placing concrete.

	How to check
	Compare visible access/protection with project SWMS, work-at-height and temporary-works plans; refer hazards to site safety process.

	Acceptance basis
	Apply site safety plan and jurisdictional WHS requirements; checklist does not certify a platform, edge protection or SWMS.

	Reference to verify
	Site SWMS, access/work-at-height plans and applicable jurisdictional WHS requirements.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	zone / access point
	



	SWMS / plan ref
	



	hazard / reported role
	



	correction evidence
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	FW-09  Placement-stage loads, access and change control


	What to observe
	Confirm planned placement sequence, access and equipment are covered by current approved temporary-works/method documents; identify field changes.

	How to check
	Review method with responsible site role and compare planned sequence/equipment/configuration to documented design assumptions.

	Acceptance basis
	Use approved sequence and assumptions; no allowable load, pour rate, concrete pressure or vibration criterion is supplied.

	Reference to verify
	Approved placement method, temporary-works assumptions and written change review.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	method revision
	



	design assumption ref
	



	equipment / sequence
	



	change approval ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Issues and corrective action
Project: _____________________  Location / room / element: _____________________  Inspection date: _____________________
	Item / date
	Issue and immediate action
	Disposition / corrective instruction
	Recheck evidence / date
	Responsible role / reference

	


	


	


	


	



	


	


	


	


	



	


	


	


	


	



	


	


	


	


	



	


	


	


	


	




Unresolved items: identify affected area, status, person notified, instruction / NCR reference and any condition before concealment or next work.


Formwork inspection handover
Project: _____________________  Location / room / element: _____________________  Date: _____________________
Field inspection handover status
[  ] Field observations recorded
[  ] Action / recheck outstanding
[  ] Temporary-works review required
This records the field inspection handover only. It is not design certification, authorization to pour, a Hold Point release, or permission to strip/load. Transfer the completed inspection and outstanding issues to the project-assigned temporary-works/project release process.
Handover roles and references
Field inspector name / role / date  ______________________________________________
Receiving temporary-works or project role / date  ______________________________________________
Open design query, NCR or change approval reference  ______________________________________________
Field inspector record
• Field inspector name/role/date  ______________________________________________
• Formwork zone/system and inspected configuration  ______________________________________________
• Observed condition, measurements and evidence refs  ______________________________________________
Design check record
• Temporary-works design and revision  ______________________________________________
• Designer and independent checker roles/identities  ______________________________________________
• Design assumptions and support evidence references  ______________________________________________
• Written change reassessment/approval reference  ______________________________________________
Project / contractual release record
• Project/temporary-works release role assigned by contract  ______________________________________________
• Decision scope and stage  ______________________________________________
• Decision status and conditions  ______________________________________________
• Date/time and ITP/control-point/notice reference  ______________________________________________
Role boundary: Field inspector records installed condition. Designer/checker owns design and required independent check; project role owns release. The checklist cannot certify capacity, alter design, release a Hold Point, or authorize placement, stripping or loading.
Signatures record the named person’s stated role and entry only. They do not by themselves approve design, certify compliance, release a contractual control point or authorize the next activity.


Source notes
These references explain topic and record design. They do not supply universal project acceptance values. Confirm the contract documents, applicable jurisdiction and approved product/system before use.
Cavoren cast-in-place concrete baseline
Role: Topic and sequence context only; not a project specification or independent technical authority.
Locator: Original proposed concrete baseline rows CON-01 to CON-08
Source URL: https://itp.cavoren.net/templates/concrete/
Queensland TMR MRTS70 Concrete, July 2022
Role: Topic guidance only for concrete/formwork interface. Queensland transport/infrastructure contract criteria are not universal building requirements.
Locator: Sections 15.5–15.9 (formwork/falsework, reinforcement, placement/compaction, early loading).
Source URL: https://www.tmr.qld.gov.au/_/media/busind/techstdpubs/specifications-and-drawings/specifications/2-bridges-and-structures/mrts70.pdf?extension=pdf&hash=BD4A48371C386F32622F6862572AA56A&rev=24517261eac44ddb86310c7980172050&sc_lang=en&size=1730809
Safe Work Australia, Guide to formwork, July 2014
Role: Safety interface guidance only. It does not replace temporary-works design, project acceptance criteria, jurisdiction-specific WHS advice or release.
Locator: PDF pages 1–4: formwork/falsework definitions, Design, formwork drawings, system components, erection/use safety and access prompts.
Source URL: https://www.safeworkaustralia.gov.au/system/files/documents/1703/guide-formwork.pdf
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