piping-plumbing-itp-template | Inspection and Test Plan
[Fill: project name] | Building Plumbing ITP — Water, Sanitary and Stormwater (Editable Baseline) — free editable baseline | [Fill: Australian state/territory] | Rev 00 | 2026-10-06 | For review
Contractor: [Fill: contractor]    Client: [Fill: client]
Scope: Original reusable baseline for conventional building cold/hot water, sanitary plumbing/drainage and stormwater where each is selected. Rows identify conditional services separately. Excludes gas, process/high-pressure pipework, fire services, HVAC/refrigerant, pools, onsite wastewater and industrial systems. Test regimes must be confirmed per jurisdiction, actual project-adopted standards and system; no default pressure/test duration is supplied. This is a free, editable, proposed baseline and is not tailored to a project, approved by a client, or evidence of completed inspection. Before use, complete the scope questions and bracketed fields, confirm every criterion and control against current project documents, and remove non-applicable rows.
Exclusions: Confirm exclusions for this project; use the scope notes above.
	ID
	Stage
	Inspection / test
	Method
	Acceptance requirement
	Reference
	Frequency
	Responsible role
	Point
	Approval / witness party
	Notice / release
	Record
	Remarks

	PL01
	Scope and service classification
	Proposed: baseline — Identify each system/medium, boundaries and excluded work.
	Proposed: baseline — Review plans, scope, schedules and design notes; classify water, sanitary, stormwater and heated-water systems separately.
	Proposed: baseline — Only specified systems [Fill: Included plumbing services] are included; process, gas, high-pressure, fire, HVAC/refrigerant, pool and on-site wastewater systems are excluded unless individually scoped.
	Guidance only; see Source Register: NCC22-V3, ABCB-PCA-INTRO
	Proposed: Once before work and when scope changes.
	Proposed: licensed plumbing contractor/design reviewer.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Plumbing scope and system register
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	PL02
	Regulatory basis and approvals
	Proposed: baseline — Confirm jurisdiction, applicable NCC Volume Three edition/state variations, licensing and inspection/notification pathway.
	Proposed: baseline — Review regulatory authority guidance, approvals, project specification and adopted document register.
	Proposed: baseline — Current applicable jurisdiction, approved pathway, inspection/notification roles and adopted editions are recorded; conflicts raised.
	Guidance only; see Source Register: NCC22-V3, ABCB-PCA-INTRO
	Proposed: Before work; update on regulatory/approved revision.
	Proposed: Plumbing contractor and builder/design reviewer.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Plumbing regulatory and approvals register
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	PL03
	Material and product approval
	Proposed: baseline — Check pipe/fitting material, class/type, joint system, potable water suitability and product certification where applicable.
	Proposed: baseline — Inspect labels/certificates and compare with approved submittal/specification and applicable WaterMark requirements.
	Proposed: baseline — Products match approved schedule [Fill: Pipe/fitting/product schedule] and required approvals/evidence for their intended service; drinking-water contact suitability is documented where required.
	Guidance only; see Source Register: NCC22-V3, NCC22-REFDOCS
	Proposed: Each delivery/product type and substitution.
	Proposed: licensed plumbing contractor submits; reviewer approves.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Plumbing products register
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	PL04
	Delivery and storage
	Proposed: baseline — Inspect received materials for identity, damage, cleanliness, contamination and storage protection.
	Proposed: baseline — Visual inspection and trace labels/batches against product submittal; maintain caps/protection as required.
	Proposed: baseline — Correct approved items are traceable, undamaged and kept clean/protected per manufacturer instructions [Fill: Pipe/fitting/product schedule].
	Guidance only; see Source Register: CQA-ITP
	Proposed: Each delivery/batch.
	Proposed: plumbing contractor.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Plumbing delivery and traceability log
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	PL05
	Set-out and service coordination
	Proposed: baseline — Check service route, levels, fixture/equipment connections, penetrations and clashes.
	Proposed: baseline — Compare marked-out installation to coordinated drawings and surveyed levels; resolve clashes before fixing/covering.
	Proposed: baseline — Routes, invert/connection levels and service points match approved drawings [Fill: Approved plumbing drawings]; unresolved clashes have approved resolution.
	Guidance only; see Source Register: NCC22-V3
	Proposed: Each zone/floor before installation.
	Proposed: plumbing contractor; builder coordinates.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Plumbing set-out and coordination check
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	PL06
	Trench, bedding and support
	Proposed: baseline — For buried runs, check trench condition, bedding, support, depth/cover and protection; for above-ground, check supports and movement provisions.
	Proposed: baseline — Inspect before laying and before cover; measure against approved details and the relevant adopted standard/project criteria.
	Proposed: baseline — Bedding/support, depth, cover, spacing and movement provisions meet approved detail [Fill: Approved plumbing drawings] and criteria [Fill: Specification and adopted standards]; no values assumed.
	Guidance only; see Source Register: NCC22-V3, NCC22-REFDOCS
	Proposed: Each run/section before pipe placement or concealment.
	Proposed: licensed plumbing contractor.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Trench and pipe support checklist
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	PL07
	Pipework installation and identification
	Proposed: baseline — Inspect pipe type/diameter, route, gradient where relevant, jointing, supports, isolation/access and identification.
	Proposed: baseline — Visual and measured checks against isometrics, schedule, manufacturer jointing instructions and adopted standard.
	Proposed: baseline — Installed pipework, gradient, joints, access and identification match approved documents [Fill: Approved plumbing drawings]/[Fill: Specification and adopted standards]; system is clearly identified by service.
	Guidance only; see Source Register: NCC22-V3, NCC22-REFDOCS
	Proposed: Each service run before concealment.
	Proposed: Licensed plumbing contractor.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Pipe installation checklist
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	PL08
	Jointing and workmanship
	Proposed: baseline — Check joint preparation, assembly, welding/brazing/solvent process only for the specified material/system.
	Proposed: baseline — Observe installer qualification where specified; check process parameters and joint records required by product/project instructions.
	Proposed: baseline — Joint type and workmanship follow approved method [Fill: Pipe/fitting/product schedule] and manufacturer/project criteria; required qualification/evidence is current.
	Guidance only; see Source Register: CQA-ITP
	Proposed: Each joint batch/lot and visual check along completed run.
	Proposed: Licensed plumbing contractor; qualified specialist if project requires.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Jointing and workmanship record
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	PL09
	Valves, fixtures and backflow interfaces
	Proposed: baseline — Verify valve type/location/access, fixture connections, backflow device and cross-connection protections if in scope.
	Proposed: baseline — Compare to approved schedules and NCC/project hazard assessment; record device identification and certificates where required.
	Proposed: baseline — Devices and interfaces match approved design [Fill: Approved plumbing drawings] and applicable project/jurisdictional requirements; missing hazard assessment is referred for resolution.
	Guidance only; see Source Register: NCC22-V3, NCC22-REFDOCS
	Proposed: Each device/fixture or assembly.
	Proposed: Licensed plumbing contractor; authorised tester for device tests if required.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Valve, fixture and backflow register
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	PL10
	Sanitary drainage alignment and falls
	Proposed: baseline — Inspect sanitary drain route, grade, connections, access openings and cleanouts before backfill.
	Proposed: baseline — Check against approved drainage plan and levels; use survey/measurement method specified by project.
	Proposed: baseline — Alignment, gradient, invert and access match approved design [Fill: Approved plumbing drawings] and adopted criteria [Fill: Specification and adopted standards]; record actual levels where required.
	Guidance only; see Source Register: NCC22-V3, WA-BULLETIN-133
	Proposed: Each drain run before testing/backfill.
	Proposed: Licensed plumber/drainer.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Sanitary drainage pre-cover checklist
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	PL11
	Sanitary pipe test before backfill
	Proposed: baseline — For sanitary plumbing/drainage, perform only the applicable jurisdiction/project test before concealment.
	Proposed: baseline — Licensed plumber/drainer confirms adopted standard edition, system boundaries, test medium, pressure/head and duration; record results.
	Proposed: baseline — Test meets confirmed project/jurisdiction criteria [Fill: Sanitary test method and criteria]; defects repaired and section retested before backfill. WA bulletin illustrates local methods, not national default criteria.
	Guidance only; see Source Register: WA-BULLETIN-133, NCC22-REFDOCS
	Proposed: Each defined test section before backfill/cover.
	Proposed: Licensed plumber/drainer; authority/client witness only where required.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Sanitary pipe test record
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	PL12
	Water service pressure/leak test
	Proposed: baseline — Test water services using the method and criteria approved for the project and jurisdiction.
	Proposed: baseline — Licensed plumber confirms isolated section, test medium, pressure/duration and acceptance source; record actual readings, instrument and observations.
	Proposed: baseline — No leakage or pressure change beyond confirmed applicable criterion [Fill: Water-service test method and criteria]; no preset national pressure/duration is assumed.
	Guidance only; see Source Register: NCC22-V3, NCC22-REFDOCS
	Proposed: Each defined water service section before concealment/commissioning.
	Proposed: Licensed plumbing contractor.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Water service pressure test record
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	PL13
	Stormwater drainage (conditional)
	Proposed: baseline — Where included, check stormwater pipe, pits, inlets, gradients, connections and discharge points.
	Proposed: baseline — Inspect route/levels and compare to approved stormwater plan, civil interface and applicable adopted requirements.
	Proposed: baseline — Installed system and discharge path match approved drawings [Fill: Approved plumbing drawings] and project criteria [Fill: Specification and adopted standards]; no sanitary test rule applied by assumption.
	Guidance only; see Source Register: NCC22-V3, NCC22-REFDOCS
	Proposed: Each run/pit/outfall before cover and at completion.
	Proposed: plumbing contractor/civil contractor per scope.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Stormwater installation checklist
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	PL14
	Heated water service (conditional)
	Proposed: baseline — Where included, check heater/system connections, relief/tempering components, discharge and access.
	Proposed: baseline — Inspect against approved design, equipment instructions and adopted heated-water requirements.
	Proposed: baseline — Equipment, safety components, connection/discharge and settings meet approved schedule [Fill: Approved plumbing drawings]/[Fill: Specification and adopted standards]; record settings only from approved source.
	Guidance only; see Source Register: NCC22-V3, NCC22-REFDOCS
	Proposed: Each heater/system before commissioning.
	Proposed: Licensed plumbing contractor; electrical trade interface separate.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Heated water installation checklist
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	PL15
	Flushing, cleaning and disinfection (conditional)
	Proposed: baseline — Where required for drinking water, confirm flushing, disinfection and any specified water quality evidence.
	Proposed: baseline — Follow project-approved procedure and applicable authority/manufacturer requirements; use competent authorised person.
	Proposed: baseline — Required flushing/disinfection steps and any specified sample results meet project/jurisdiction criteria [Fill: Flushing/disinfection requirements]; no unsupported universal chlorination value.
	Guidance only; see Source Register: NCC22-V3
	Proposed: Each system/zone where required before use.
	Proposed: Licensed plumbing contractor; laboratory/person as required.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Water service flushing/disinfection record
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	PL16
	Pre-cover inspection and backfill
	Proposed: baseline — Walk down installed services and confirm testing/photographs/authority inspections before covering.
	Proposed: baseline — Check inspection checklist, test evidence, utility/authority notices, service marking and approved backfill requirements.
	Proposed: baseline — All required pre-cover checks are complete; identified defects are closed and required authority release is documented [Fill: Concealment/backfill release].
	Guidance only; see Source Register: WA-BULLETIN-133, CQA-ITP
	Proposed: Each trench/shaft/ceiling area before concealment.
	Proposed: Licensed plumber/drainer; builder coordinates; authority as required.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Pre-cover and backfill release checklist
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	PL17
	Commissioning and operational checks
	Proposed: baseline — Verify specified flow, operation, fixture discharge, leaks and system interfaces.
	Proposed: baseline — Commission by licensed plumbing practitioner under approved procedure; record measured results and exceptions by system.
	Proposed: baseline — Specified operational criteria in [Fill: Specification and adopted standards] are satisfied; defects are corrected and retested; no generic flow/pressure figures assumed.
	Guidance only; see Source Register: NCC22-V3, ABCB-PCA-INTRO
	Proposed: Each system/zone at commissioning.
	Proposed: Licensed plumbing contractor; client/operator witness if required.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Plumbing commissioning record
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	PL18
	Defects and retest
	Proposed: baseline — Record leaks, blockages, incorrect levels, joint failures and corrective work.
	Proposed: baseline — Identify location/system, defect, repair method, retest evidence and closure.
	Proposed: baseline — Defects are corrected against approved method and failed tests repeated successfully before cover/use.
	Guidance only; see Source Register: CQA-ITP
	Proposed: Each defect/retest.
	Proposed: Licensed plumbing contractor; reviewer per project.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Plumbing defect and retest register
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	PL19
	As-built and handover
	Proposed: baseline — Verify certificates, inspection notices, test reports, product evidence, as-builts and operation/maintenance information.
	Proposed: baseline — Review contract/regulator handover index and match records to service IDs/locations.
	Proposed: baseline — Required certificates and records are complete for included systems and issued by properly authorised persons; as-builts reflect installed route.
	Guidance only; see Source Register: NCC22-V3, CQA-ITP
	Proposed: Once per package and after approved changes.
	Proposed: Licensed plumbing contractor submits; builder compiles.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Plumbing handover register
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.



Inspection point key
Inspection point key: H = Proposed Hold Point - use only if assigned in the contract | W = Proposed Witness Point - use only if assigned in the contract | R = Proposed Review | S = Proposed Surveillance | TBC = To be confirmed | N/A = Not applicable. External H/W rights and whether work may proceed are governed by the project contract and approved process; proposed points require agreement.


Blank Inspection Record Forms
[Fill: project name] | piping-plumbing-itp-template | Record actual observations during the work. No results or signatures are pre-filled.
	ITP ID / Stage
	Inspection / method / acceptance
	Location / lot
	Date and result
	Evidence / record ref.
	Performed by / signature
	Reviewed by / signature

	PL01 | Scope and service classification
	Proposed: baseline — Identify each system/medium, boundaries and excluded work.
Method: Proposed: baseline — Review plans, scope, schedules and design notes; classify water, sanitary, stormwater and heated-water systems separately.
Accept when: Proposed: baseline — Only specified systems [Fill: Included plumbing services] are included; process, gas, high-pressure, fire, HVAC/refrigerant, pool and on-site wastewater systems are excluded unless individually scoped.
Record: Plumbing scope and system register
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	PL02 | Regulatory basis and approvals
	Proposed: baseline — Confirm jurisdiction, applicable NCC Volume Three edition/state variations, licensing and inspection/notification pathway.
Method: Proposed: baseline — Review regulatory authority guidance, approvals, project specification and adopted document register.
Accept when: Proposed: baseline — Current applicable jurisdiction, approved pathway, inspection/notification roles and adopted editions are recorded; conflicts raised.
Record: Plumbing regulatory and approvals register
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	PL03 | Material and product approval
	Proposed: baseline — Check pipe/fitting material, class/type, joint system, potable water suitability and product certification where applicable.
Method: Proposed: baseline — Inspect labels/certificates and compare with approved submittal/specification and applicable WaterMark requirements.
Accept when: Proposed: baseline — Products match approved schedule [Fill: Pipe/fitting/product schedule] and required approvals/evidence for their intended service; drinking-water contact suitability is documented where required.
Record: Plumbing products register
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	PL04 | Delivery and storage
	Proposed: baseline — Inspect received materials for identity, damage, cleanliness, contamination and storage protection.
Method: Proposed: baseline — Visual inspection and trace labels/batches against product submittal; maintain caps/protection as required.
Accept when: Proposed: baseline — Correct approved items are traceable, undamaged and kept clean/protected per manufacturer instructions [Fill: Pipe/fitting/product schedule].
Record: Plumbing delivery and traceability log
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	PL05 | Set-out and service coordination
	Proposed: baseline — Check service route, levels, fixture/equipment connections, penetrations and clashes.
Method: Proposed: baseline — Compare marked-out installation to coordinated drawings and surveyed levels; resolve clashes before fixing/covering.
Accept when: Proposed: baseline — Routes, invert/connection levels and service points match approved drawings [Fill: Approved plumbing drawings]; unresolved clashes have approved resolution.
Record: Plumbing set-out and coordination check
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	PL06 | Trench, bedding and support
	Proposed: baseline — For buried runs, check trench condition, bedding, support, depth/cover and protection; for above-ground, check supports and movement provisions.
Method: Proposed: baseline — Inspect before laying and before cover; measure against approved details and the relevant adopted standard/project criteria.
Accept when: Proposed: baseline — Bedding/support, depth, cover, spacing and movement provisions meet approved detail [Fill: Approved plumbing drawings] and criteria [Fill: Specification and adopted standards]; no values assumed.
Record: Trench and pipe support checklist
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	PL07 | Pipework installation and identification
	Proposed: baseline — Inspect pipe type/diameter, route, gradient where relevant, jointing, supports, isolation/access and identification.
Method: Proposed: baseline — Visual and measured checks against isometrics, schedule, manufacturer jointing instructions and adopted standard.
Accept when: Proposed: baseline — Installed pipework, gradient, joints, access and identification match approved documents [Fill: Approved plumbing drawings]/[Fill: Specification and adopted standards]; system is clearly identified by service.
Record: Pipe installation checklist
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	PL08 | Jointing and workmanship
	Proposed: baseline — Check joint preparation, assembly, welding/brazing/solvent process only for the specified material/system.
Method: Proposed: baseline — Observe installer qualification where specified; check process parameters and joint records required by product/project instructions.
Accept when: Proposed: baseline — Joint type and workmanship follow approved method [Fill: Pipe/fitting/product schedule] and manufacturer/project criteria; required qualification/evidence is current.
Record: Jointing and workmanship record
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	PL09 | Valves, fixtures and backflow interfaces
	Proposed: baseline — Verify valve type/location/access, fixture connections, backflow device and cross-connection protections if in scope.
Method: Proposed: baseline — Compare to approved schedules and NCC/project hazard assessment; record device identification and certificates where required.
Accept when: Proposed: baseline — Devices and interfaces match approved design [Fill: Approved plumbing drawings] and applicable project/jurisdictional requirements; missing hazard assessment is referred for resolution.
Record: Valve, fixture and backflow register
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	PL10 | Sanitary drainage alignment and falls
	Proposed: baseline — Inspect sanitary drain route, grade, connections, access openings and cleanouts before backfill.
Method: Proposed: baseline — Check against approved drainage plan and levels; use survey/measurement method specified by project.
Accept when: Proposed: baseline — Alignment, gradient, invert and access match approved design [Fill: Approved plumbing drawings] and adopted criteria [Fill: Specification and adopted standards]; record actual levels where required.
Record: Sanitary drainage pre-cover checklist
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	PL11 | Sanitary pipe test before backfill
	Proposed: baseline — For sanitary plumbing/drainage, perform only the applicable jurisdiction/project test before concealment.
Method: Proposed: baseline — Licensed plumber/drainer confirms adopted standard edition, system boundaries, test medium, pressure/head and duration; record results.
Accept when: Proposed: baseline — Test meets confirmed project/jurisdiction criteria [Fill: Sanitary test method and criteria]; defects repaired and section retested before backfill. WA bulletin illustrates local methods, not national default criteria.
Record: Sanitary pipe test record
	
	Date: __________
System/section ID: __________
Hydrostatic/air/vacuum/other: __________
Test medium: __________
Head/pressure applied: __________
Unit: __________
Stabilisation time: __________
Test duration: __________
Start reading/time: __________
End reading/time: __________
Leak/pressure change observed: __________
Instrument ID/calibration: __________
Pass/fail/exception: __________
Repair/retest reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	PL12 | Water service pressure/leak test
	Proposed: baseline — Test water services using the method and criteria approved for the project and jurisdiction.
Method: Proposed: baseline — Licensed plumber confirms isolated section, test medium, pressure/duration and acceptance source; record actual readings, instrument and observations.
Accept when: Proposed: baseline — No leakage or pressure change beyond confirmed applicable criterion [Fill: Water-service test method and criteria]; no preset national pressure/duration is assumed.
Record: Water service pressure test record
	
	Date: __________
System/section ID: __________
Test method/reference: __________
Test medium: __________
Test pressure: __________
Unit: __________
Duration: __________
Start reading/time: __________
End reading/time: __________
Leak observation: __________
Instrument ID/calibration: __________
Pass/fail/exception: __________
Repair/retest reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	PL13 | Stormwater drainage (conditional)
	Proposed: baseline — Where included, check stormwater pipe, pits, inlets, gradients, connections and discharge points.
Method: Proposed: baseline — Inspect route/levels and compare to approved stormwater plan, civil interface and applicable adopted requirements.
Accept when: Proposed: baseline — Installed system and discharge path match approved drawings [Fill: Approved plumbing drawings] and project criteria [Fill: Specification and adopted standards]; no sanitary test rule applied by assumption.
Record: Stormwater installation checklist
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	PL14 | Heated water service (conditional)
	Proposed: baseline — Where included, check heater/system connections, relief/tempering components, discharge and access.
Method: Proposed: baseline — Inspect against approved design, equipment instructions and adopted heated-water requirements.
Accept when: Proposed: baseline — Equipment, safety components, connection/discharge and settings meet approved schedule [Fill: Approved plumbing drawings]/[Fill: Specification and adopted standards]; record settings only from approved source.
Record: Heated water installation checklist
	
	Date: __________
Heater make/model: __________
Serial number: __________
Recorded setting: __________
Unit: __________
Discharge check/reference: __________
Commissioning record: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	PL15 | Flushing, cleaning and disinfection (conditional)
	Proposed: baseline — Where required for drinking water, confirm flushing, disinfection and any specified water quality evidence.
Method: Proposed: baseline — Follow project-approved procedure and applicable authority/manufacturer requirements; use competent authorised person.
Accept when: Proposed: baseline — Required flushing/disinfection steps and any specified sample results meet project/jurisdiction criteria [Fill: Flushing/disinfection requirements]; no unsupported universal chlorination value.
Record: Water service flushing/disinfection record
	
	Date: __________
System/zone: __________
Procedure/reference: __________
Date/time: __________
Water source: __________
Sample ID: __________
Laboratory: __________
Result: __________
Criterion source/location: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	PL16 | Pre-cover inspection and backfill
	Proposed: baseline — Walk down installed services and confirm testing/photographs/authority inspections before covering.
Method: Proposed: baseline — Check inspection checklist, test evidence, utility/authority notices, service marking and approved backfill requirements.
Accept when: Proposed: baseline — All required pre-cover checks are complete; identified defects are closed and required authority release is documented [Fill: Concealment/backfill release].
Record: Pre-cover and backfill release checklist
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	PL17 | Commissioning and operational checks
	Proposed: baseline — Verify specified flow, operation, fixture discharge, leaks and system interfaces.
Method: Proposed: baseline — Commission by licensed plumbing practitioner under approved procedure; record measured results and exceptions by system.
Accept when: Proposed: baseline — Specified operational criteria in [Fill: Specification and adopted standards] are satisfied; defects are corrected and retested; no generic flow/pressure figures assumed.
Record: Plumbing commissioning record
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	PL18 | Defects and retest
	Proposed: baseline — Record leaks, blockages, incorrect levels, joint failures and corrective work.
Method: Proposed: baseline — Identify location/system, defect, repair method, retest evidence and closure.
Accept when: Proposed: baseline — Defects are corrected against approved method and failed tests repeated successfully before cover/use.
Record: Plumbing defect and retest register
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	PL19 | As-built and handover
	Proposed: baseline — Verify certificates, inspection notices, test reports, product evidence, as-builts and operation/maintenance information.
Method: Proposed: baseline — Review contract/regulator handover index and match records to service IDs/locations.
Accept when: Proposed: baseline — Required certificates and records are complete for included systems and issued by properly authorised persons; as-builts reflect installed route.
Record: Plumbing handover register
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	





Source Register
	Source ID
	Title / filename
	Revision
	Type
	Path / URL

	NCC22-V3
	ABCB, NCC 2022 Volume Three (Plumbing Code of Australia)
	See linked source; verify current edition and project adoption
	guidance
	https://ncc.abcb.gov.au/editions/ncc-2022/adopted/volume-three

	NCC22-REFDOCS
	ABCB, NCC 2022 Volume Three referenced documents
	See linked source; verify current edition and project adoption
	guidance
	https://ncc.abcb.gov.au/editions/ncc-2022/adopted/volume-three/2-referenced-documents/referenced-documents

	WA-BULLETIN-133
	WA DMIRS, Industry Bulletin 133: Sanitary plumbing and sanitary drainage installation testing
	See linked source; verify current edition and project adoption
	guidance
	https://www.wa.gov.au/system/files/2024-10/industry_bulletin_133_-_sanitary_plumbing_and_sanitary_drainage_installation.pdf

	ABCB-PCA-INTRO
	ABCB, NCC Tutor lesson: Using Volume Three
	See linked source; verify current edition and project adoption
	guidance
	https://ncc.abcb.gov.au/resources/videos/ncc-tutor-lesson-using-volume-three

	CQA-ITP
	Construction Quality Association, Guide: How to create an ITP
	See linked source; verify current edition and project adoption
	guidance
	https://www.cqa.org.au/post/guide-how-to-create-an-inspection-and-test-plan-itp



Open Confirmations
	Issue ID
	Priority
	ITP rows
	Open item
	Action needed

	CONF-001
	confirmation
	PL01
	PL01: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-002
	confirmation
	PL02
	PL02: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-003
	confirmation
	PL03
	PL03: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-004
	confirmation
	PL04
	PL04: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-005
	confirmation
	PL05
	PL05: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-006
	confirmation
	PL06
	PL06: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-007
	confirmation
	PL07
	PL07: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-008
	confirmation
	PL08
	PL08: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-009
	confirmation
	PL09
	PL09: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-010
	confirmation
	PL10
	PL10: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-011
	confirmation
	PL11
	PL11: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-012
	confirmation
	PL12
	PL12: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-013
	confirmation
	PL13
	PL13: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-014
	confirmation
	PL14
	PL14: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-015
	confirmation
	PL15
	PL15: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-016
	confirmation
	PL16
	PL16: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-017
	confirmation
	PL17
	PL17: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-018
	confirmation
	PL18
	PL18: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-019
	confirmation
	PL19
	PL19: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.







