CAVOREN  |  FIELD RECORD
Reinforcement Inspection Checklist
Blank project field record  |  Complete from current approved documents and site observations
Scope
Included: Steel reinforcement installed in cast-in-place reinforced slabs, pad footings and strip footings, from document/bar-mark check through pre-concealment inspection.
Excluded: Precast manufacture, post-tensioning/prestressing, piles, shotcrete, bridge/highway special provisions, welding/NDT acceptance, structural design/rebar design verification, concrete delivery/testing/placement, and whole-pour release.
Use and project setup
Project field: Project / contractor  ______________________________________________
Project field: Element / grid / inspection zone  ______________________________________________
Project field: Pour or lot reference  ______________________________________________
Project field: Inspection date  ______________________________________________
Project field: Structural drawing / revision  ______________________________________________
Project field: Bar schedule / revision  ______________________________________________
Before inspection: Element, grid and pour/lot IDs — Defines the physical steel package inspected and links results to the pour record.
Before inspection: Current structural drawings and bar schedule, including revisions — Provides actual marks, layout, details and dimensions.
Before inspection: Project reinforcement specification and adopted standard edition — Supplies contractual product, tolerance, records and installation criteria.
Before inspection: Approved steel/coupler submittals and delivery traceability records — Links installed marks/products to evidence.
Before inspection: Project inspection, substitution and NCR procedures — Defines assigned roles, control points and closeout process.
How to use
1. Confirm physical scope, controlled documents, measurement method, required records and assigned roles.
2. Inspect a defined zone/lot; cite criterion and actual document revision for each check.
3. Record actual measurements only where required; attach traceability and photo evidence by reference.
4. For deviations, identify affected steel, prevent concealment where required, obtain written disposition and record recheck.
5. Keep field observations separate from designer approval and project release.
Important: Blank field checklist for project adaptation. Use actual approved documents and project acceptance criteria. Record only observations made. This is not design approval, a temporary-works certificate, contractual Hold/Witness Point release, or permission to place, strip or load.


Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	RE-01  Inspection package and reinforcement documents


	What to observe
	Identify element, pour/lot boundaries, current structural drawings, bar schedule, revisions and project inspection/check requirements.

	How to check
	Review the controlled document register against the element and schedule marks at the workface; note superseded or conflicting copies.

	Acceptance basis
	Use current approved project drawings, bar schedule, specification and ITP; record unresolved conflict rather than choosing a revision.

	Reference to verify
	Controlled document register, approved structural drawings, bar schedule, reinforcement specification and project ITP.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	element / grid
	



	drawing / rev
	



	bar schedule / rev
	



	open item ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	RE-02  Delivery identity and traceability


	What to observe
	Inspect labels/tags, bundle or mesh marks and delivery documents for identity to scheduled bar marks, product description and source traceability required by the job.

	How to check
	Compare delivered bundles/mesh with schedule and dockets/certificates; link identity to storage location and element allocation.

	Acceptance basis
	Apply only project procurement/specification traceability requirements and scheduled marks; do not impose TMR registration unless adopted by contract.

	Reference to verify
	Approved bar schedule, material submittal, delivery docket and project traceability requirements.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	delivery docket
	



	bundle / bar mark
	



	certificate ref
	



	allocated location
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	RE-03  Storage and visible steel condition


	What to observe
	Observe stacking/separation, ground contact, physical damage, bends/kinks and visible contamination relevant to the specified product.

	How to check
	Walk stock before fixing; inspect representative bundles and suspect bars; photograph defects and identify affected marks.

	Acceptance basis
	Compare with project specification and approved material submittal; seek direction where condition may affect specified use.

	Reference to verify
	Project reinforcement specification, approved material submittal and written condition disposition.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	bar mark / bundle
	



	storage location
	



	condition / photo ref
	



	disposition ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	RE-04  Cut, bend and bar-mark conformity


	What to observe
	Compare installed cut/bent shapes, schedule marks and orientation with approved bending/bar schedule, including any project-controlled site re-bending.

	How to check
	Trace selected bars to bending schedule and inspect shape/orientation; review authorization and method for permitted field adjustment.

	Acceptance basis
	Use current approved schedule and project-approved fabrication/adjustment procedure; no generic bend radius, length or tolerance is supplied.

	Reference to verify
	Approved bar bending schedule and project-approved fabrication or field-adjustment procedure.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	bar mark / location
	



	schedule shape / rev
	



	observed shape
	



	approval / disposition ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	RE-05  Bar arrangement, spacing and layer position


	What to observe
	Observe installed bar marks, direction, layer, orientation and relative spacing against structural details, including congestion zones.

	How to check
	Check identified grids/sections using project measurement method; record actual readings where required by drawings/specification.

	Acceptance basis
	Use actual structural drawing, bar schedule and project tolerance; no universal spacing or tolerance applies.

	Reference to verify
	Approved structural drawings, bar schedule and project dimensional criteria.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	grid / section
	



	bar marks / layer
	



	criterion / drawing ref
	



	actual measurement
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	RE-06  Laps, anchorage, couplers and termination details


	What to observe
	Inspect shown splice locations/types, lap/anchorage arrangement, bar ends and coupler identity/engagement evidence specified for the element.

	How to check
	Compare critical locations with structural details; check product and installation records for specified mechanical splices.

	Acceptance basis
	Follow exact project drawings, adopted specification/standard and approved coupler submittal; do not infer lap lengths, embedment or coupler acceptance class.

	Reference to verify
	Structural splice/anchorage details, adopted project specification and approved coupler instructions.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	splice / location
	



	detail / drawing ref
	



	product / batch
	



	installation / disposition ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	RE-07  Supports, spacers and specified cover


	What to observe
	Observe chair/spacer product and placement, support contact/stability and reinforcement position relative to formed faces or substrate.

	How to check
	Inspect support type/locations; check project-identified cover points with suitable verified measuring method when required.

	Acceptance basis
	Use project cover schedule/details, accepted products and tolerances; record actual values where project calls for measurement.

	Reference to verify
	Project cover schedule, support/spacer details and approved products.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	support / location
	



	cover criterion / ref
	



	actual cover / unit / method
	



	recheck evidence
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	RE-08  Fixing, restraint and placement stability


	What to observe
	Observe ties/fixings, cage rigidity, support stability and displacement risk from planned worker access and documented placing method.

	How to check
	Review approved placing/access method; inspect congested, edge, opening and support zones; record project-required movement checks.

	Acceptance basis
	Use project-approved fixing details and construction/placement method; do not infer universal tie frequency or load resistance.

	Reference to verify
	Approved fixing details and concrete placement/access method.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	zone / bar IDs
	



	fixing observed
	



	placing method ref
	



	direction / recheck ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	RE-09  Surface, projection and reinforcement exceptions


	What to observe
	Observe contamination/coating or loose material that may affect specified performance, projecting bars at interfaces, and outstanding substitutions/NCRs.

	How to check
	Walk steel zone before concealment; cross-check substitution/NCR register and prior-pour interfaces; record condition and closeout reference.

	Acceptance basis
	Use project specification and written designer/project disposition; no blanket rust rejection threshold or cleaning rule is imposed.

	Reference to verify
	Project specification, approved substitutions and written NCR/designer dispositions.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	zone / interface
	



	condition observed
	



	NCR / substitution ref
	



	action / closeout ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Issues and corrective action
Project: _____________________  Location / room / element: _____________________  Inspection date: _____________________
	Item / date
	Issue and immediate action
	Disposition / corrective instruction
	Recheck evidence / date
	Responsible role / reference

	


	


	


	


	



	


	


	


	


	



	


	


	


	


	



	


	


	


	


	



	


	


	


	


	




Unresolved items: identify affected area, status, person notified, instruction / NCR reference and any condition before concealment or next work.


Reinforcement inspection handover
Project: _____________________  Location / room / element: _____________________  Date: _____________________
Inspection record status
[  ] Inspection record complete
[  ] Action / recheck outstanding
[  ] Design or project disposition required
This status records the steel inspection handover only. It does not mean ready to pour, approve reinforcement design, release a contractual control point, or authorize placement. Carry open items into the project ITP/pre-pour process.
Handover roles and references
Field inspector name / role / date  ______________________________________________
Receiving project role / date  ______________________________________________
Open NCR, RFI or disposition reference  ______________________________________________
Field inspector record
• Field inspector name/role/date  ______________________________________________
• Inspection lot, element and boundaries  ______________________________________________
• Observation and evidence references  ______________________________________________
Design check record
• Design document and revision  ______________________________________________
• Designer/checker identity and project-assigned role  ______________________________________________
• Design response/calculation/RFI reference  ______________________________________________
Project / contractual release record
• Release decision-maker role assigned by project/contract  ______________________________________________
• Decision status and conditions  ______________________________________________
• Basis: inspection/NCR references and control-point clause  ______________________________________________
• Date/time and notice/release record reference  ______________________________________________
Role boundary: Inspector records field observations; design author/checker and project release authority remain separate records/roles. This signature does not certify design, approve a substitution, release a Hold Point or authorize placement.
Signatures record the named person’s stated role and entry only. They do not by themselves approve design, certify compliance, release a contractual control point or authorize the next activity.


Source notes
These references explain topic and record design. They do not supply universal project acceptance values. Confirm the contract documents, applicable jurisdiction and approved product/system before use.
Cavoren cast-in-place concrete baseline
Role: Topic and sequence context only; not a project specification or independent technical authority.
Locator: Original proposed concrete baseline rows CON-01 to CON-08
Source URL: https://itp.cavoren.net/templates/concrete/
Queensland TMR Ancillary MRTS71 Reinforcing Steel / ATS 5310, July 2025
Role: Topic guidance from a Queensland transport/infrastructure specification only. Do not import its values, registrations, frequencies, roles or hold points into general building work.
Locator: Clauses 1.1–1.4; 4.1; 5.1–5.19; 6.1–6.9; 7.1–7.8; 8.1–8.5; 9.1–9.9; Sections 10–12; Appendix A. TMR listing says ancillary harmonised specifications are information only and not for use in contracts.
Source URL: https://www.tmr.qld.gov.au/_/media/busind/techstdpubs/specifications-and-drawings/specifications/2-bridges-and-structures/mrts71.pdf?extension=pdf&hash=436D56549EF2693B1E5CC9DAD5DCF1D6&rev=c09d0ebf1e8149bfbab395d06076d9d1&sc_lang=en&size=695385
Queensland TMR MRTS70 Concrete, July 2022
Role: Topic guidance only for concrete/formwork interface. Queensland transport/infrastructure contract criteria are not universal building requirements.
Locator: Sections 15.5–15.9 (formwork/falsework, reinforcement, placement/compaction, early loading).
Source URL: https://www.tmr.qld.gov.au/_/media/busind/techstdpubs/specifications-and-drawings/specifications/2-bridges-and-structures/mrts70.pdf?extension=pdf&hash=BD4A48371C386F32622F6862572AA56A&rev=24517261eac44ddb86310c7980172050&sc_lang=en&size=1730809
https://itp.cavoren.net/checklists/reinforcement/  |  Project: __________________________  |  Page 




