CAVOREN  |  FIELD RECORD
Sanitary Drainage Installation and Pre-Cover Record
Blank project field record  |  Complete from current approved documents and site observations
Scope
Included: Ordinary building sanitary plumbing/drainage installation records for defined pipe segments, connections and inspection before concealment/backfill where applicable.
Excluded: Design sizing or gradients, universal levels or test criteria, on-site wastewater treatment, trade waste systems, industrial/process piping, gas, fire and public utility networks unless separately scoped and sourced.
Use and project setup
Project field: Project / building / jurisdiction  ______________________________________________
Project field: Drainage drawing / revision  ______________________________________________
Project field: Segment / from–to node IDs  ______________________________________________
Project field: Pipe / joint system  ______________________________________________
Project field: Design levels / criterion ref  ______________________________________________
Project field: Test method / report ref  ______________________________________________
Project field: Pre-cover notice / witness ref  ______________________________________________
Project field: As-built / NCR / disposition refs  ______________________________________________
Before inspection: Approved sanitary drainage plans and schedules — Identify current segment layout, nodes, sizes, levels, interfaces and revision.
Before inspection: Project material and joint submittals — Defines approved components, joint systems and installation requirements.
Before inspection: Project test specification and adopted standard — Supplies local method, acceptance criteria and any required test record; the form has no universal test settings.
Before inspection: Inspection, backfill and notification schedule — Assigns pre-cover checks, notice periods, witness role and any external notification/release.
Before inspection: As-built and nonconformance workflow — Defines required marked-up drawings, photo evidence, repair records and disposition.
How to use
1. Use a separate record for each identifiable segment or project-defined inspection lot; keep different systems and criteria separate.
2. Check current drainage drawing and node-to-node identity, then record actual observed geometry and interfaces against project references.
3. Record test method, values and outcome only from the approved procedure and actual test report; attach the source evidence.
4. Before backfill/concealment, link required inspection/notice, test, repairs, photos and as-built markups.
5. Leave any unclear criterion, missing test or covered uninspected extent open for project disposition.
Important: No gradient, invert tolerance, test method, pressure/head, duration or witness/release rule is prefilled. Confirm the jurisdiction, current approved drawings, project-adopted standard and inspection notice before covering work. WA Bulletin 133 is WA-specific guidance only.


Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	SD-01  Drainage section identity and approved geometry


	What to observe
	Drain line/branch ID, upstream/downstream nodes, drawing revision, pipe material/size, design direction and segment limits.

	How to check
	Trace the installed segment between identified connection points against approved drainage layout and schedule; record design references for any checked levels/grade.

	Acceptance basis
	Each observation belongs to a defined segment and current drawing; geometry and any numerical criteria are assessed only against project-approved design documents.

	Reference to verify
	Current approved project drawings, specification, adopted service standard and inspection/test plan; record exact document, revision, clause/detail and affected segment.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Drain line / segment ID
	



	From–to nodes / pit refs
	



	Material / nominal size as scheduled
	



	Drawing / revision / detail
	



	Design levels / criterion source
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	SD-BED  Exposed trench, bedding and pipe support


	What to observe
	Record trench condition, installed bedding and pipe support before they are concealed, where below-ground work is included.

	How to check
	Compare exposed work with the approved trench, bedding and embedment detail and relevant product instructions. Identify unstable formation, voids, debris, pipe movement and civil-work interfaces for project disposition.

	Acceptance basis
	Observed trench support, bedding and embedment correspond to the approved project detail. Material, thickness, cover and compaction requirements come from the actual applicable sources; this record supplies no default value.

	Reference to verify
	Enter approved drawing/detail and revision, applicable civil or geotechnical specification, and product installation instruction.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Drain run / inspection location
	



	Drawing / bedding detail and revision
	



	Formation condition / groundwater observation
	



	Bedding material and evidence reference
	



	Actual bedding / support observation or measurement and unit
	



	Specified cover / surround criterion source
	



	Civil interface / unresolved defect / reinspection reference
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	SD-02  Pipe, joint and connection workmanship


	What to observe
	Pipe/fitting identity, joint type and visible condition, connection orientation, damage, contamination and transition to fixtures or other drains.

	How to check
	Inspect accessible work and compare joints/fittings with approved product submittal, installation details and method; capture photographs or location references where useful.

	Acceptance basis
	Installed components and observable joints correspond to the approved project system and are free of unresolved visible damage/defects; this blank form sets no dimensional or joint acceptance limit.

	Reference to verify
	Current approved project drawings, specification, adopted service standard and inspection/test plan; record exact document, revision, clause/detail and affected segment.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Pipe/fitting / product submittal ref
	



	Joint type / installation method ref
	



	Joint / connection location
	



	Observed condition / defect
	



	Photo / instruction ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	SD-03  Access, support and service separation


	What to observe
	Inspection/cleaning access, supports/restraints where visible, penetrations and separation from stormwater or other systems at interfaces.

	How to check
	Compare accessible installation with approved coordination/service drawings and manufacturer/project details; identify access points and cross-system interfaces.

	Acceptance basis
	Required access and interfaces are identifiable and installed to current project details; keep stormwater and sanitary service identities distinct; any proposed cross-system connection needs verified design and applicable authority approval.

	Reference to verify
	Current approved project drawings, specification, adopted service standard and inspection/test plan; record exact document, revision, clause/detail and affected segment.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Access opening / cleaning point IDs
	



	Support / penetration detail ref
	



	Sanitary–stormwater separation observation
	



	Interface / coordination drawing ref
	



	Issue / instruction reference
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	SD-04  Specified test, result and defect closeout


	What to observe
	Project-specified test method and exact source, section identity, actual test record/report, defects found, repairs and retest linkage.

	How to check
	Before testing, transcribe the locally applicable project method and criteria; after test, link the original report and any repair/retest in sequence. Record only the actual method and findings.

	Acceptance basis
	A required test is traceable to the defined section and project-approved criterion; any failure/repair/retest remains linked. WA Bulletin 133 details are not general project defaults.

	Reference to verify
	Current approved project drawings, specification, adopted service standard and inspection/test plan; record exact document, revision, clause/detail and affected segment.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Test required? / governing source
	



	Method / clause / edition
	



	Original report / actual result ref
	



	Observed defect / location
	



	Repair and retest IDs / date
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	SD-05  Pre-cover inspection and assigned release record


	What to observe
	Whether required inspection/witness occurred before backfill or concealment, notice record, outstanding issues, as-installed markups and assigned release decision.

	How to check
	Compare the actual work stage with project inspection/notification schedule; link inspection photos, test evidence, marked-up drawings and release or hold instruction.

	Acceptance basis
	Required pre-cover observations and contractual notice/release evidence are present before concealment; record the actual authority and status from project documents.

	Reference to verify
	Current approved project drawings, specification, adopted service standard and inspection/test plan; record exact document, revision, clause/detail and affected segment.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Pre-cover date / exposed extent
	



	Notice / witness / inspection record
	



	Open NCR / repair / retest ref
	



	As-built markup / photo refs
	



	Release authority / decision / date
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Sanitary drainage segment and test log
Use one line per segment, inspection or actual test event. Link the segment to the approved nodes/drawing, method, original test report, repair/retest and pre-cover evidence. No local or WA numeric test setting is supplied.
Project / contract: ______________________________    Element / pour / lot: ______________________________    Date / shift: ____________________
Location / area: ______________________________    Record reference / revision: ______________________________
	Date / stage
	Segment / node IDs
	Drawing / revision
	Joint / access / interface observation
	Test method / source ref
	Actual result / report ref
	Defect / repair / retest ref
	Pre-cover notice / release ref
	Recorder / status

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 




Issues and corrective action
Project: _____________________  Location / room / element: _____________________  Inspection date: _____________________
	Item / date
	Issue and immediate action
	Disposition / corrective instruction
	Recheck evidence / date
	Responsible role / reference

	


	


	


	


	



	


	


	


	


	



	


	


	


	


	



	


	


	


	


	



	


	


	


	


	




Unresolved items: identify affected area, status, person notified, instruction / NCR reference and any condition before concealment or next work.


Sanitary drainage pre-cover handover
Project: _____________________  Location / room / element: _____________________  Date: _____________________
Record inspection handover status
[  ] Record complete; source evidence linked
[  ] Issue, repair, retest or project decision remains open
[  ] Assigned project role review / disposition required
This record documents observations and links project evidence. It does not certify compliance, approve a design, create statutory notification or grant contractual release.
Handover roles and references
Installer / licensed role and date  ______________________________________________
Field inspector / role / date  ______________________________________________
Assigned authority / witness / release role and record ref  ______________________________________________
Open defect / repair / retest / as-built references  ______________________________________________
Signatures record the named person’s stated role and entry only. They do not by themselves approve design, certify compliance, release a contractual control point or authorize the next activity.


Source notes
These references explain topic and record design. They do not supply universal project acceptance values. Confirm the contract documents, applicable jurisdiction and approved product/system before use.
ABCB, NCC 2022 Volume Three — Plumbing Code of Australia
Role: Official scope and jurisdictional topic framework; does not provide project-specific field test acceptance values.
Locator: Section B water services and Section C sanitary plumbing and drainage; volume includes jurisdiction schedules.
Source URL: https://ncc.abcb.gov.au/editions/ncc-2022/adopted/volume-three
ABCB, NCC 2022 Volume Three Schedule 2 — Referenced documents
Role: Reference-edition pointer only; full Standards not inspected and project adoption must be checked.
Locator: AS/NZS 3500 Parts 1–4:2021 titles and NCC clause pointers by service type.
Source URL: https://ncc.abcb.gov.au/editions/ncc-2022/adopted/volume-three/2-referenced-documents/referenced-documents
ABCB, Editions of the National Construction Code
Role: Edition/adoption context; check actual jurisdiction, transition and project approvals.
Locator: NCC 2022 Amendment 2 adoption and edition transition notes.
Source URL: https://ncc.abcb.gov.au/editions-national-construction-code
Government of Western Australia, Building and Energy Industry Bulletin 133
Role: Topic guidance for sanitary test record linkage and pre-cover workflow in WA only. No test values or notification rules are generalized; check current local adoption and project criteria.
Locator: Two-page October 2020 bulletin: tests sanitary plumbing/drainage before trench fill, describes methods, repair and retesting; references AS/NZS 3500.2:2018.
Source URL: https://www.wa.gov.au/system/files/2024-10/industry_bulletin_133_-_sanitary_plumbing_and_sanitary_drainage_installation.pdf
https://itp.cavoren.net/checklists/sanitary-drainage/  |  Project: __________________________  |  Page 




