CAVOREN  |  FIELD RECORD
Building Stormwater Drainage Inspection Record
Blank project field record  |  Complete from current approved documents and site observations
Scope
Included: Ordinary building surface/subsurface stormwater drainage within the project boundary, including identified lines, pits, inlets, connections and approved outlet interface.
Excluded: Stormwater network design or sizing, universal levels/gradients/test requirements, public authority mains, major civil flood systems and on-site detention design; industrial/process, sanitary, gas or fire networks unless separately scoped and sourced.
Use and project setup
Project field: Project / building / jurisdiction  ______________________________________________
Project field: Stormwater drawing / revision  ______________________________________________
Project field: Line / pit / inlet IDs  ______________________________________________
Project field: Design datum / outlet detail  ______________________________________________
Project field: Survey / as-built ref  ______________________________________________
Project field: Pre-cover notice / inspector  ______________________________________________
Project field: Test requirement / source if any  ______________________________________________
Project field: Defect / disposition refs  ______________________________________________
Before inspection: Approved stormwater plans, pit schedules and outlet details — Define design nodes, levels, pits, flow route, destination and current revision.
Before inspection: Project survey/setout criteria and level datum — Allows actual levels to be recorded and compared on the correct datum and against stated tolerances.
Before inspection: Authority, consent and point-of-connection documents — Define approved network interface or on-site discharge arrangement where applicable.
Before inspection: Project test/inspection and pre-cover schedule — States whether functional testing, notice, witness or release is required; no generic requirement is assumed.
Before inspection: As-built and defect-closeout process — Defines required survey file, markup, photographs, repair records and handover evidence.
How to use
1. Use the approved drainage drawing to identify line, pit, inlet, connection and terminal outlet. Keep design and actual surveyed data distinct.
2. Record actual levels with unit and datum, linked to the survey/setout evidence and project acceptance source.
3. Inspect pit/access and pipe interfaces while visible; record exact connection identity and check separation from sanitary drainage.
4. Confirm and record the designated connection or approved disposal point from project/authority evidence.
5. Record a test only where required. Link method and source; if none is specified, state the basis for N/A.
6. Before cover or surface closure, link required inspection, photos, survey and as-built records and project-assigned disposition.
Important: Stormwater requirements and authority interfaces vary by jurisdiction and project. No default test is assumed: perform and record a test only where the approved project or authority documents require one. Capture actual surveyed levels with datum and the designated discharge destination.


Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	SW-01  Stormwater network identity and design setout


	What to observe
	Line, pit and inlet IDs, contributing area/reference where scheduled, drawing revision, flow direction, design levels and outlet destination.

	How to check
	Trace each installed line and pit to the current approved drainage plan, pit schedule and level details; record measured/as-installed values separately from design values.

	Acceptance basis
	Network elements and flow path are traceable to approved project drawings, with actual measurements compared only against project criteria and units.

	Reference to verify
	Current approved project drawings, specification, adopted service standard and inspection/test plan; record exact document, revision, clause/detail and affected segment.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Line / pit / inlet ID
	



	From–to node / outlet
	



	Drawing / pit schedule revision
	



	Design level / datum / source
	



	Actual level / unit / survey ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	SW-BED  Exposed trench, bedding and pipe support


	What to observe
	Record trench condition, installed bedding and pipe support before they are concealed, where below-ground work is included.

	How to check
	Compare exposed work with the approved trench, bedding and embedment detail and relevant product instructions. Identify unstable formation, voids, debris, pipe movement and civil-work interfaces for project disposition.

	Acceptance basis
	Observed trench support, bedding and embedment correspond to the approved project detail. Material, thickness, cover and compaction requirements come from the actual applicable sources; this record supplies no default value.

	Reference to verify
	Enter approved drawing/detail and revision, applicable civil or geotechnical specification, and product installation instruction.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Drain run / inspection location
	



	Drawing / bedding detail and revision
	



	Formation condition / groundwater observation
	



	Bedding material and evidence reference
	



	Actual bedding / support observation or measurement and unit
	



	Specified cover / surround criterion source
	



	Civil interface / unresolved defect / reinspection reference
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	SW-02  Pits, inlets, grates and access condition


	What to observe
	Pit type/mark, installed position and orientation, inlet/grate condition, cover level reference, access for maintenance and visible workmanship.

	How to check
	Compare installed pit and access arrangement with approved pit detail/schedule; record photo and level/survey references where required.

	Acceptance basis
	Pits, inlets and maintenance access match project-approved details; no size, level tolerance or grate load class is assumed by this record.

	Reference to verify
	Current approved project drawings, specification, adopted service standard and inspection/test plan; record exact document, revision, clause/detail and affected segment.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Pit / inlet mark
	



	Approved pit detail / revision
	



	Grate / cover identity
	



	Access and clearance observation
	



	Photo / level survey ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	SW-03  Pipe connections, transitions and separation


	What to observe
	Pipe material/joint identity, pit entry/exit, connection seating, changes of direction/level, sealed interfaces and separation from sanitary drainage.

	How to check
	Inspect accessible interfaces and compare to approved connection details and service coordination drawings; trace suspected cross-connections to source and destination before disposition.

	Acceptance basis
	Connections and transitions follow approved project details; keep stormwater and sanitary systems separate; any proposed cross-system connection needs verified design and applicable authority approval.

	Reference to verify
	Current approved project drawings, specification, adopted service standard and inspection/test plan; record exact document, revision, clause/detail and affected segment.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Pipe / joint system
	



	Pit entry / exit / connection IDs
	



	Transition / detail reference
	



	Sanitary separation observation
	



	Issue / photo / instruction ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	SW-04  Designated point of connection or on-site outlet


	What to observe
	Approved network connection, lawful/designated discharge point or approved on-site disposal arrangement, destination ID and any authority interface.

	How to check
	Trace installed discharge route to the approved project outlet and relevant consent/authority detail; record the actual terminal point, not an assumed discharge path.

	Acceptance basis
	The constructed route terminates at the project-designated point of connection or approved disposal system and required interface evidence is linked.

	Reference to verify
	Current approved project drawings, specification, adopted service standard and inspection/test plan; record exact document, revision, clause/detail and affected segment.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Outlet / point-of-connection ID
	



	Approved outlet drawing / consent ref
	



	Actual destination / receiving system
	



	Authority interface record if applicable
	



	Open issue / decision ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	SW-05  Specified test or functional evidence, conditional


	What to observe
	Whether a test/functional demonstration is required, its project source, defined extent, actual method and result; visible obstruction, defect, repair or retest if encountered.

	How to check
	Only where specified, follow the current approved project/authority method and retain actual test evidence. If no test is specified, record N/A with the controlling scope basis rather than inventing one.

	Acceptance basis
	Any required test is assessed against its stated project criteria and linked to actual segment/pit results; no universal stormwater test or acceptance value is imposed.

	Reference to verify
	Current approved project drawings, specification, adopted service standard and inspection/test plan; record exact document, revision, clause/detail and affected segment.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Test required? / source
	



	Test extent / method / revision
	



	Actual observation / result and unit
	



	Defect / blockage / repair ref
	



	Retest / disposition record
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	SW-06  Pre-cover, levels and as-built closeout


	What to observe
	Required exposed inspection, surveyed actual inverts/cover levels where required, pit and connection coordinates, photos, as-built markups, outstanding defects and release evidence.

	How to check
	Compare actual survey and installed network to current approved requirements; link inspection notice and project release decision before trench fill or surface closure where required.

	Acceptance basis
	Project-required pre-cover inspection, level records and as-built evidence are complete and traceable; this form does not create a universal hold point or level tolerance.

	Reference to verify
	Current approved project drawings, specification, adopted service standard and inspection/test plan; record exact document, revision, clause/detail and affected segment.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Pre-cover inspection / notice ref
	



	Actual invert / cover levels and datum
	



	Survey / setout file ref
	



	As-built markup / photo refs
	



	Release / outstanding disposition ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Stormwater segment, pit and outlet log
Use one line per identified segment, pit, inspection or project-required test event. Record design and measured levels with their datum/source. A test is conditional on actual project/authority requirements; leave entries blank until observed.
Project / contract: ______________________________    Element / pour / lot: ______________________________    Date / shift: ____________________
Location / area: ______________________________    Record reference / revision: ______________________________
	Date / stage
	Line / pit / inlet ID
	From–to / outlet
	Drawing / revision
	Design level / datum
	Actual level / unit / survey ref
	Connection / access observation
	Test / defect / as-built evidence ref
	Recorder / status

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 




Issues and corrective action
Project: _____________________  Location / room / element: _____________________  Inspection date: _____________________
	Item / date
	Issue and immediate action
	Disposition / corrective instruction
	Recheck evidence / date
	Responsible role / reference

	


	


	


	


	



	


	


	


	


	



	


	


	


	


	



	


	


	


	


	



	


	


	


	


	




Unresolved items: identify affected area, status, person notified, instruction / NCR reference and any condition before concealment or next work.


Stormwater drainage handover
Project: _____________________  Location / room / element: _____________________  Date: _____________________
Record inspection handover status
[  ] Record complete; source evidence linked
[  ] Issue, repair, retest or project decision remains open
[  ] Assigned project role review / disposition required
This record links observed installation and project evidence. It does not design drainage, establish lawful discharge, certify compliance or grant a contractual release.
Handover roles and references
Installer / assigned trade role and date  ______________________________________________
Field inspector / role / date  ______________________________________________
Surveyor / as-built evidence role and reference  ______________________________________________
Authority / project release role and decision ref if applicable  ______________________________________________
Signatures record the named person’s stated role and entry only. They do not by themselves approve design, certify compliance, release a contractual control point or authorize the next activity.


Source notes
These references explain topic and record design. They do not supply universal project acceptance values. Confirm the contract documents, applicable jurisdiction and approved product/system before use.
ABCB, NCC 2022 Volume Three — Plumbing Code of Australia
Role: Official scope and jurisdictional topic framework; does not provide project-specific field test acceptance values.
Locator: Section B water services and Section C sanitary plumbing and drainage; volume includes jurisdiction schedules.
Source URL: https://ncc.abcb.gov.au/editions/ncc-2022/adopted/volume-three
ABCB, NCC 2022 Volume Three Schedule 2 — Referenced documents
Role: Reference-edition pointer only; full Standards not inspected and project adoption must be checked.
Locator: AS/NZS 3500 Parts 1–4:2021 titles and NCC clause pointers by service type.
Source URL: https://ncc.abcb.gov.au/editions/ncc-2022/adopted/volume-three/2-referenced-documents/referenced-documents
ABCB, Editions of the National Construction Code
Role: Edition/adoption context; check actual jurisdiction, transition and project approvals.
Locator: NCC 2022 Amendment 2 adoption and edition transition notes.
Source URL: https://ncc.abcb.gov.au/editions-national-construction-code
ABCB, NCC 2022 Volume Three — Victoria Part E4 Stormwater, Surface and Sub-surface Drainage Systems
Role: Jurisdiction-specific topic support for access/outlet fields only; verify current local variation and project/authority criteria. No universal test is inferred.
Locator: Victoria-specific E4 includes maintenance access and transfer of stormwater to a point of connection; points to AS/NZS 3500.3 for covered systems.
Source URL: https://ncc.abcb.gov.au/editions/ncc-2022/adopted/volume-three/e-facilities-and-ancillary-additions/vic-part-e4-stormwater-surface-and-sub-surface-drainage-systems
Victoria Building and Plumbing Commission, DR 07 Bedding site stormwater drains
Role: Victoria-specific topic guidance. Overview inspected; project material and dimensional criteria are not derived from it. Verify applicable jurisdiction and adopted requirements.
Locator: Practice-note overview and version history: published 13 March 2024; bedding, embedment, backfill, grade and cover topics. Checked 7 October 2026.
Source URL: https://www.bpc.vic.gov.au/resource-hub/practice-notes/dr-07-bedding-site-stormwater-drains
https://itp.cavoren.net/checklists/stormwater/  |  Project: __________________________  |  Page 




