structural-steel-itp-template | Inspection and Test Plan
[Fill: project name] | Structural steel fabrication and erection inspection and test plan template — free editable baseline | [Fill: Australian state/territory] | Rev 00 | 2026-10-06 | For review
Contractor: [Fill: contractor]    Client: [Fill: client]
Scope: Reusable baseline for structural steelwork from material receipt and workshop fabrication through coating, delivery and site erection. Separate shop and site lots/roles where different. Excludes design certification, crane/lift engineering, fireproofing and specialist coatings unless included. This is a free, editable, proposed baseline and is not tailored to a project, approved by a client, or evidence of completed inspection. Before use, complete the scope questions and bracketed fields, confirm every criterion and control against current project documents, and remove non-applicable rows.
Exclusions: Confirm exclusions for this project; use the scope notes above.
	ID
	Stage
	Inspection / test
	Method
	Acceptance requirement
	Reference
	Frequency
	Responsible role
	Point
	Approval / witness party
	Notice / release
	Record
	Remarks

	STE-01
	Planning and submittals
	Proposed: baseline — Confirm package boundaries, design documents, construction category, inspection/testing plan and fabrication/erection interfaces.
	Proposed: baseline — Review approved drawings, specification, annexures and submittal register.
	Proposed: baseline — Current approved [Fill: Approved drawings and revisions], [Fill: Construction category], [Fill: Steel Criteria], [Fill: Approved weld procedure, acceptance and sampling criteria], [Fill: Specified NDT method, extent and acceptance criteria] and [Fill: Project coating system, preparation and inspection criteria] requirements are identified; resolve inconsistencies before fabrication.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS78, HUTCHIES-SUITE
	Proposed: Before procurement / fabrication.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Steelwork submittal and document register
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	STE-02
	Material certificates and traceability
	Proposed: baseline — Verify section, plate, bolt and consumable identity and link supplied steel to certificates/heat or batch evidence.
	Proposed: baseline — Check markings, tags, delivery dockets and certificates against material register and approved grade schedule.
	Proposed: baseline — Material type/grade matches [Fill: Material grades / certification criteria] and each item/lot is traceable to required certification; quarantine unidentified or discrepant material.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS78, HUTCHIES-SUITE
	Proposed: Each delivery and before traceability is lost through cutting/blasting.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Steel material register and certificates
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	STE-03
	Material condition and storage
	Proposed: baseline — Inspect received steel and consumables for damage, corrosion, distortion, contamination and protected storage.
	Proposed: baseline — Visual inspection on receipt and before use; check storage requirements for consumables.
	Proposed: baseline — Condition remains suitable for specified fabrication/coating; damage or consumable storage excursions are recorded and dispositioned.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS78
	Proposed: Every delivery and before use.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Incoming steel inspection
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	STE-04
	Fabrication set-out and cutting
	Proposed: baseline — Check member identity, cut lengths, hole positions, edge preparation and fabrication dimensions.
	Proposed: baseline — Measure against shop/approved drawings and fabrication schedule before assembly or welding.
	Proposed: baseline — Dimensions and preparation match [Fill: Fabrication dimensions / tolerances]; revisions and approved deviations are traceable.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS78, HUTCHIES-SUITE
	Proposed: Each member or defined fabrication lot before assembly.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Fabrication dimensional checklist
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	STE-05
	Welding documentation readiness
	Proposed: baseline — Verify approved welding procedures, weld map, consumables and personnel qualifications required by project.
	Proposed: baseline — Review WPS, procedure qualification evidence, welder qualifications/continuity and consumable records against weld schedule.
	Proposed: baseline — Applicable WPS and qualifications cover the specified joint/material/process under [Fill: Weld procedure/qualification requirements]; missing or mismatched coverage is resolved before welding.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS78, HUTCHIES-SUITE
	Proposed: Before first weld and when material, process, joint or personnel scope changes.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Welding document and qualification register
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	STE-06
	Fit-up and joint preparation
	Proposed: baseline — Inspect joint preparation, root gap, alignment, cleanliness, backing and fit-up before welding.
	Proposed: baseline — Visual and dimensional checks against approved joint detail and applicable WPS.
	Proposed: baseline — Fit-up satisfies [Fill: Joint fit-up acceptance] and WPS; defects, unapproved tacks or mismatch are corrected before welding.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS78, HUTCHIES-SUITE
	Proposed: Each joint category / weld lot before welding, at specified rate.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Weld fit-up inspection
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	STE-07
	Welding process controls
	Proposed: baseline — Check weld execution records include joint identity, WPS, welder, date and any specified environmental/process controls.
	Proposed: baseline — Observe/record welding and review production logs against approved WPS and project requirements.
	Proposed: baseline — Work is performed within the applicable approved WPS and [Fill: Welding process variables / controls]; interruptions, repairs and deviations are traceable.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS78, HUTCHIES-SUITE
	Proposed: During each welding shift / project-defined lot.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Welding production log
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	STE-08
	Completed weld visual inspection
	Proposed: baseline — Inspect completed welds for profile, visible defects, size and completion against weld map and acceptance criteria.
	Proposed: baseline — Visual inspection by project-designated competent inspector; use measuring gauges where required.
	Proposed: baseline — Weld identification and visual acceptance match [Fill: Visual acceptance and sampling]; repairs are recorded and reinspected.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS78, HUTCHIES-SUITE
	Proposed: Each weld or sampling rate defined in project requirements.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Weld visual inspection register
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	STE-09
	Specified NDT
	Proposed: baseline — Arrange and review only the NDT methods, extent and acceptance specified for the welds.
	Proposed: baseline — Match NDT request/report to joint IDs and weld map; verify method, operator, equipment and report disposition as required.
	Proposed: baseline — Reports cover [Fill: NDT method, extent and criteria] and report acceptance against the adopted project criteria; untested, rejected or repair-required welds are tracked to closure.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS78, HUTCHIES-SUITE
	Proposed: At specified welds/lots and before concealment or coating as required.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	NDT request and report register
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	STE-10
	Bolt and fastener receipt
	Proposed: baseline — Check bolt assemblies, grade, lot identity, coating/condition and required certificates.
	Proposed: baseline — Review packaging marks, certificates and delivery register against connection schedule and installation specification.
	Proposed: baseline — Fasteners match [Fill: Bolt system / certificate criteria] and remain identifiable by lot; mixed, damaged or undocumented items are isolated pending disposition.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS78, HUTCHIES-SUITE
	Proposed: Each delivery / lot before installation.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Fastener register and certificates
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	STE-11
	Bolt installation and verification
	Proposed: baseline — Inspect connection assembly, fit, washer/nut arrangement and the project-specified installation/verification evidence.
	Proposed: baseline — Observe installation method and examine calibrated tool records or verification tests only where required by project.
	Proposed: baseline — Installation and verification satisfy [Fill: Bolt installation / verification criteria]; record connection/member IDs, method and any retightening or replacement.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS78, HUTCHIES-SUITE
	Proposed: Each connection group at the project-defined stage and rate.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Bolt installation and verification log
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	STE-12
	Protective coating surface preparation
	Proposed: baseline — Check substrate preparation, cleanliness, profile and environmental conditions before coating.
	Proposed: baseline — Inspect surface against specified coating system and record preparation method/environment; verify traceability before blasting/galvanizing where required.
	Proposed: baseline — Surface preparation and conditions meet [Fill: Preparation class / environmental limits] and supplier instructions; contamination or unsuitable conditions are corrected before application.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS78, HUTCHIES-SUITE
	Proposed: Each coating lot / shift and before coating.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Coating surface-preparation report
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	STE-13
	Coating application and thickness
	Proposed: baseline — Inspect applied coating system, coverage, dry film thickness or galvanizing checks as specified.
	Proposed: baseline — Review batch records and use specified inspection method/instrument; record calibration and measurement locations.
	Proposed: baseline — System, coats, measured values and acceptance comply with [Fill: System, thickness and acceptance]; repair/recoat and reinspection are documented.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS78, HUTCHIES-SUITE
	Proposed: Each defined coating lot at specified stages.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Coating application and inspection report
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	STE-14
	Fabrication release and delivery
	Proposed: baseline — Compile material, dimensional, weld, NDT and coating records; inspect member markings and transport condition.
	Proposed: baseline — Review manufacturing data book against member register; inspect before dispatch and again on receipt.
	Proposed: baseline — Required manufacturing records are complete; member marks match erection drawings; transport damage is dispositioned before erection.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS78, HUTCHIES-SUITE
	Proposed: Each dispatch and receipt lot.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Fabrication release and delivery inspection
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	STE-15
	Erection and temporary stability
	Proposed: baseline — Check erection sequence, lifting/temporary bracing, member orientation, plumb/level and connection completion against approved erection documents.
	Proposed: baseline — Observe erection and survey critical geometry against approved drawings and temporary works/erection method.
	Proposed: baseline — Erection follows approved method and [Fill: Erection geometry and release criteria]; temporary stability and connections are confirmed before removing temporary supports.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS78, HUTCHIES-SUITE
	Proposed: Each erection sequence / level / frame before releasing temporary supports.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Erection inspection and survey record
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	STE-16
	Grout, final connections and closeout
	Proposed: baseline — Inspect specified baseplate grout and final connection completion; close out defects and as-built records.
	Proposed: baseline — Check grout product, preparation/application records where required; verify final bolt/weld completion, survey and NCR closure.
	Proposed: baseline — Grout and connections match approved details and [Fill: Grout / connection / closeout requirements]; outstanding deviations have written design/client disposition before package completion.
	Guidance only; see Source Register: NSW-QMG, TMR-MRTS78, HUTCHIES-SUITE
	Proposed: At completion and before concealment/load transfer where applicable.
	Proposed: [Fill: Person/role proposed to perform this check] performs and records; [Fill: Person/role proposed to review or release this check] reviews where the project assigns review.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Steelwork completion checklist and record pack
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.



Inspection point key
Inspection point key: H = Proposed Hold Point - use only if assigned in the contract | W = Proposed Witness Point - use only if assigned in the contract | R = Proposed Review | S = Proposed Surveillance | TBC = To be confirmed | N/A = Not applicable. External H/W rights and whether work may proceed are governed by the project contract and approved process; proposed points require agreement.


Blank Inspection Record Forms
[Fill: project name] | structural-steel-itp-template | Record actual observations during the work. No results or signatures are pre-filled.
	ITP ID / Stage
	Inspection / method / acceptance
	Location / lot
	Date and result
	Evidence / record ref.
	Performed by / signature
	Reviewed by / signature

	STE-01 | Planning and submittals
	Proposed: baseline — Confirm package boundaries, design documents, construction category, inspection/testing plan and fabrication/erection interfaces.
Method: Proposed: baseline — Review approved drawings, specification, annexures and submittal register.
Accept when: Proposed: baseline — Current approved [Fill: Approved drawings and revisions], [Fill: Construction category], [Fill: Steel Criteria], [Fill: Approved weld procedure, acceptance and sampling criteria], [Fill: Specified NDT method, extent and acceptance criteria] and [Fill: Project coating system, preparation and inspection criteria] requirements are identified; resolve inconsistencies before fabrication.
Record: Steelwork submittal and document register
	
	Date: __________
Document title / number: __________
Revision / issue date: __________
Conflict / unresolved interface: __________
Submittal register reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	STE-02 | Material certificates and traceability
	Proposed: baseline — Verify section, plate, bolt and consumable identity and link supplied steel to certificates/heat or batch evidence.
Method: Proposed: baseline — Check markings, tags, delivery dockets and certificates against material register and approved grade schedule.
Accept when: Proposed: baseline — Material type/grade matches [Fill: Material grades / certification criteria] and each item/lot is traceable to required certification; quarantine unidentified or discrepant material.
Record: Steel material register and certificates
	
	Date: __________
Member / heat ID: __________
Specified grade: __________
Section / plate size (mm): __________
Certificate reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	STE-03 | Material condition and storage
	Proposed: baseline — Inspect received steel and consumables for damage, corrosion, distortion, contamination and protected storage.
Method: Proposed: baseline — Visual inspection on receipt and before use; check storage requirements for consumables.
Accept when: Proposed: baseline — Condition remains suitable for specified fabrication/coating; damage or consumable storage excursions are recorded and dispositioned.
Record: Incoming steel inspection
	
	Date: __________
Item / member: __________
Condition / damage: __________
Disposition ref: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	STE-04 | Fabrication set-out and cutting
	Proposed: baseline — Check member identity, cut lengths, hole positions, edge preparation and fabrication dimensions.
Method: Proposed: baseline — Measure against shop/approved drawings and fabrication schedule before assembly or welding.
Accept when: Proposed: baseline — Dimensions and preparation match [Fill: Fabrication dimensions / tolerances]; revisions and approved deviations are traceable.
Record: Fabrication dimensional checklist
	
	Date: __________
Member mark: __________
Length (mm): __________
Hole / feature position (mm): __________
Edge prep / detail: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	STE-05 | Welding documentation readiness
	Proposed: baseline — Verify approved welding procedures, weld map, consumables and personnel qualifications required by project.
Method: Proposed: baseline — Review WPS, procedure qualification evidence, welder qualifications/continuity and consumable records against weld schedule.
Accept when: Proposed: baseline — Applicable WPS and qualifications cover the specified joint/material/process under [Fill: Weld procedure/qualification requirements]; missing or mismatched coverage is resolved before welding.
Record: Welding document and qualification register
	
	Date: __________
WPS ID/revision: __________
Welder ID: __________
Qualification record ref: __________
Consumable batch: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	STE-06 | Fit-up and joint preparation
	Proposed: baseline — Inspect joint preparation, root gap, alignment, cleanliness, backing and fit-up before welding.
Method: Proposed: baseline — Visual and dimensional checks against approved joint detail and applicable WPS.
Accept when: Proposed: baseline — Fit-up satisfies [Fill: Joint fit-up acceptance] and WPS; defects, unapproved tacks or mismatch are corrected before welding.
Record: Weld fit-up inspection
	
	Date: __________
Joint ID: __________
Root gap (mm): __________
Mismatch / alignment (mm): __________
WPS ID: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	STE-07 | Welding process controls
	Proposed: baseline — Check weld execution records include joint identity, WPS, welder, date and any specified environmental/process controls.
Method: Proposed: baseline — Observe/record welding and review production logs against approved WPS and project requirements.
Accept when: Proposed: baseline — Work is performed within the applicable approved WPS and [Fill: Welding process variables / controls]; interruptions, repairs and deviations are traceable.
Record: Welding production log
	
	Date: __________
Joint ID: __________
WPS ID: __________
Welder ID: __________
Weld date: __________
Repair cycle ref: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	STE-08 | Completed weld visual inspection
	Proposed: baseline — Inspect completed welds for profile, visible defects, size and completion against weld map and acceptance criteria.
Method: Proposed: baseline — Visual inspection by project-designated competent inspector; use measuring gauges where required.
Accept when: Proposed: baseline — Weld identification and visual acceptance match [Fill: Visual acceptance and sampling]; repairs are recorded and reinspected.
Record: Weld visual inspection register
	
	Date: __________
Joint ID: __________
Measured weld size (mm): __________
Visual result: __________
Repair / reinspection ref: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	STE-09 | Specified NDT
	Proposed: baseline — Arrange and review only the NDT methods, extent and acceptance specified for the welds.
Method: Proposed: baseline — Match NDT request/report to joint IDs and weld map; verify method, operator, equipment and report disposition as required.
Accept when: Proposed: baseline — Reports cover [Fill: NDT method, extent and criteria] and report acceptance against the adopted project criteria; untested, rejected or repair-required welds are tracked to closure.
Record: NDT request and report register
	
	Date: __________
Joint ID: __________
NDT method: __________
Extent / coverage: __________
Report ref: __________
Result / disposition: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	STE-10 | Bolt and fastener receipt
	Proposed: baseline — Check bolt assemblies, grade, lot identity, coating/condition and required certificates.
Method: Proposed: baseline — Review packaging marks, certificates and delivery register against connection schedule and installation specification.
Accept when: Proposed: baseline — Fasteners match [Fill: Bolt system / certificate criteria] and remain identifiable by lot; mixed, damaged or undocumented items are isolated pending disposition.
Record: Fastener register and certificates
	
	Date: __________
Lot / batch: __________
Nominal diameter (mm): __________
Specified grade: __________
Certificate ref: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	STE-11 | Bolt installation and verification
	Proposed: baseline — Inspect connection assembly, fit, washer/nut arrangement and the project-specified installation/verification evidence.
Method: Proposed: baseline — Observe installation method and examine calibrated tool records or verification tests only where required by project.
Accept when: Proposed: baseline — Installation and verification satisfy [Fill: Bolt installation / verification criteria]; record connection/member IDs, method and any retightening or replacement.
Record: Bolt installation and verification log
	
	Date: __________
Connection ID: __________
Bolt lot: __________
Installation method: __________
Verification reading/result: __________
Tool ID / calibration: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	STE-12 | Protective coating surface preparation
	Proposed: baseline — Check substrate preparation, cleanliness, profile and environmental conditions before coating.
Method: Proposed: baseline — Inspect surface against specified coating system and record preparation method/environment; verify traceability before blasting/galvanizing where required.
Accept when: Proposed: baseline — Surface preparation and conditions meet [Fill: Preparation class / environmental limits] and supplier instructions; contamination or unsuitable conditions are corrected before application.
Record: Coating surface-preparation report
	
	Date: __________
Member / lot: __________
Specified / observed prep grade: __________
Profile result: __________
Conditions / dew point if required: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	STE-13 | Coating application and thickness
	Proposed: baseline — Inspect applied coating system, coverage, dry film thickness or galvanizing checks as specified.
Method: Proposed: baseline — Review batch records and use specified inspection method/instrument; record calibration and measurement locations.
Accept when: Proposed: baseline — System, coats, measured values and acceptance comply with [Fill: System, thickness and acceptance]; repair/recoat and reinspection are documented.
Record: Coating application and inspection report
	
	Date: __________
Member / location: __________
Coat / system: __________
Measured thickness (µm): __________
Instrument ID: __________
Repair / recheck ref: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	STE-14 | Fabrication release and delivery
	Proposed: baseline — Compile material, dimensional, weld, NDT and coating records; inspect member markings and transport condition.
Method: Proposed: baseline — Review manufacturing data book against member register; inspect before dispatch and again on receipt.
Accept when: Proposed: baseline — Required manufacturing records are complete; member marks match erection drawings; transport damage is dispositioned before erection.
Record: Fabrication release and delivery inspection
	
	Date: __________
Member mark: __________
Dispatch docket: __________
Damage / disposition: __________
Dossier ref: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	STE-15 | Erection and temporary stability
	Proposed: baseline — Check erection sequence, lifting/temporary bracing, member orientation, plumb/level and connection completion against approved erection documents.
Method: Proposed: baseline — Observe erection and survey critical geometry against approved drawings and temporary works/erection method.
Accept when: Proposed: baseline — Erection follows approved method and [Fill: Erection geometry and release criteria]; temporary stability and connections are confirmed before removing temporary supports.
Record: Erection inspection and survey record
	
	Date: __________
Grid / level: __________
Member mark: __________
Plumb / alignment (mm): __________
Survey ref: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	STE-16 | Grout, final connections and closeout
	Proposed: baseline — Inspect specified baseplate grout and final connection completion; close out defects and as-built records.
Method: Proposed: baseline — Check grout product, preparation/application records where required; verify final bolt/weld completion, survey and NCR closure.
Accept when: Proposed: baseline — Grout and connections match approved details and [Fill: Grout / connection / closeout requirements]; outstanding deviations have written design/client disposition before package completion.
Record: Steelwork completion checklist and record pack
	
	Date: __________
Baseplate / location: __________
Grout batch: __________
Release evidence: __________
NCR / disposition ref: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	





Source Register
	Source ID
	Title / filename
	Revision
	Type
	Path / URL

	NSW-QMG
	NSW Government Quality Management Guidelines for Construction, Appendix D (ITP guidance)
	See linked source; verify current edition and project adoption
	guidance
	https://www.info.buy.nsw.gov.au/resources/construction/quality-management-guidelines-for-construction

	TMR-MRTS78
	Queensland TMR MRTS78 Fabrication of Structural Steelwork (November 2020)
	See linked source; verify current edition and project adoption
	guidance
	https://www.tmr.qld.gov.au/_/media/busind/techstdpubs/specifications-and-drawings/specifications/2-bridges-and-structures/mrts78.pdf?extension=pdf&hash=50EAAB111B231F1443975ABF3F281175&rev=13c320fd75b648a5b31908b182c84091&sc_lang=en&size=1765061

	HUTCHIES-SUITE
	Hutchinson Builders, Construction ITPs and Reports suite (downloadable Word examples)
	See linked source; verify current edition and project adoption
	guidance
	https://subbies.hutchies.com.au/resources/videos/safety-and-quality-planning



Open Confirmations
	Issue ID
	Priority
	ITP rows
	Open item
	Action needed

	CONF-001
	confirmation
	STE-01
	STE-01: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-002
	confirmation
	STE-02
	STE-02: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-003
	confirmation
	STE-03
	STE-03: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-004
	confirmation
	STE-04
	STE-04: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-005
	confirmation
	STE-05
	STE-05: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-006
	confirmation
	STE-06
	STE-06: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-007
	confirmation
	STE-07
	STE-07: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-008
	confirmation
	STE-08
	STE-08: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-009
	confirmation
	STE-09
	STE-09: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-010
	confirmation
	STE-10
	STE-10: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-011
	confirmation
	STE-11
	STE-11: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-012
	confirmation
	STE-12
	STE-12: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-013
	confirmation
	STE-13
	STE-13: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-014
	confirmation
	STE-14
	STE-14: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-015
	confirmation
	STE-15
	STE-15: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-016
	confirmation
	STE-16
	STE-16: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.







