waterproofing-itp-template | Inspection and Test Plan
[Fill: project name] | Internal Wet Area Waterproofing ITP — Editable Baseline — free editable baseline | [Fill: Australian state/territory] | Rev 00 | 2026-10-06 | For review
Contractor: [Fill: contractor]    Client: [Fill: client]
Scope: Original reusable baseline for membrane waterproofing to internal bathrooms, showers, laundries and similar wet areas in Australian building work. It is a planning aid, not a design or compliance certificate. Exterior/below-ground/roof/facade waterproofing, swimming pools, tanking and proprietary specialist systems are excluded. Confirm NCC edition/state variation, building class, approved compliance pathway, contract and manufacturer system before use. This is a free, editable, proposed baseline and is not tailored to a project, approved by a client, or evidence of completed inspection. Before use, complete the scope questions and bracketed fields, confirm every criterion and control against current project documents, and remove non-applicable rows.
Exclusions: Confirm exclusions for this project; use the scope notes above.
	ID
	Stage
	Inspection / test
	Method
	Acceptance requirement
	Reference
	Frequency
	Responsible role
	Point
	Approval / witness party
	Notice / release
	Record
	Remarks

	WP01
	Scope and compliance basis
	Proposed: baseline — Confirm rooms, wet-area types, system limits and interfaces included.
	Proposed: baseline — Review approved scope, room schedule, drawings and jurisdiction/compliance pathway.
	Proposed: baseline — Included locations and waterproofing extents match the approved scope [Fill: Wet-area drawings/schedule] and pathway [Fill: Compliance pathway]; exclusions are listed.
	Guidance only; see Source Register: NCC22-HOUSE, ABCB-WETAREAS
	Proposed: Once before work; update on approved scope revision.
	Proposed: waterproofing subcontractor; builder/design reviewer to confirm.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Scope and compliance basis register
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	WP02
	Product/system approval
	Proposed: baseline — Check specified membrane, primer, bond breaker, reinforcement and accessories are the approved compatible system.
	Proposed: baseline — Compare submittals, product labels and current manufacturer data to approved product schedule.
	Proposed: baseline — Product/system and components match approved submittal [Fill: Waterproofing system/product]; compatibility and permitted substrate/use are documented.
	Guidance only; see Source Register: NCC22-HOUSE, SIKA-1K-PDS
	Proposed: Each system/product and each substitution.
	Proposed: subcontractor submits; builder/design reviewer approves.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Waterproofing product submittal register
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	WP03
	Delivery and storage
	Proposed: baseline — Check delivered product identity, batch, shelf life and storage condition.
	Proposed: baseline — Inspect packaging/labels and compare to approved submittal and current manufacturer storage instructions.
	Proposed: baseline — Product identity and batch are traceable; packaging is intact and within manufacturer shelf-life/storage limits [Fill: Waterproofing system/product].
	Guidance only; see Source Register: SIKA-1K-PDS
	Proposed: Each delivery/batch.
	Proposed: waterproofing subcontractor.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Waterproofing delivery and batch register
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	WP04
	Substrate readiness
	Proposed: baseline — Inspect substrate type, soundness, cleanliness, dryness/condition and surface preparation before priming.
	Proposed: baseline — Visual inspection; check moisture/condition using method and limit in project/manufacturer documents; record defects and remedial preparation.
	Proposed: baseline — Substrate is the approved type [Fill: Substrate type], prepared to [Fill: Waterproofing system/product] instructions, free of specified contaminants/defects, and within any stated moisture/condition limits. Specific project/system condition: [Fill: Specified substrate preparation limits].
	Guidance only; see Source Register: NCC22-HOUSE, SIKA-1K-PDS
	Proposed: Each room/area before primer.
	Proposed: applicator; builder reviewer if specified.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Substrate readiness checklist
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	WP05
	Falls and drainage
	Proposed: baseline — Check floor falls, floor waste position, drainage path and any step-down/threshold details before membrane.
	Proposed: baseline — Measure levels/falls against approved drawings and jurisdiction/code pathway; confirm waste is secure and interface detail identified.
	Proposed: baseline — Falls, waste position and threshold/step details match approved detail [Fill: Falls/drain details] and applicable compliance pathway [Fill: Compliance pathway]; missing design criteria are flagged.
	Guidance only; see Source Register: NCC22-HOUSE
	Proposed: Each wet room before membrane.
	Proposed: subcontractor measures; builder/surveyor where specified.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Falls and drainage check
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	WP06
	Junctions and movement joints
	Proposed: baseline — Inspect wall-floor junctions, internal corners, changes of plane, construction/movement joints and bond-breaker detail.
	Proposed: baseline — Visual check against approved detail and system instructions; record each junction type and treatment.
	Proposed: baseline — Each junction treatment is continuous and matches approved detail [Fill: Penetrations/junction details] and the compatible system instructions [Fill: Waterproofing system/product].
	Guidance only; see Source Register: NCC22-HOUSE, SIKA-1K-PDS
	Proposed: Each room and each junction type before covering.
	Proposed: waterproofing subcontractor.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Junction and bond-breaker checklist
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	WP07
	Penetrations and outlets
	Proposed: baseline — Check pipe penetrations, floor wastes, puddle flanges and fixtures interfaces are stable and treated.
	Proposed: baseline — Visual inspection and compare dimensions/details to approved drawings and system instructions.
	Proposed: baseline — Penetrations/outlets are correctly located and sealed using the specified compatible detail [Fill: Penetrations/junction details]; no untreated opening remains.
	Guidance only; see Source Register: NCC22-HOUSE, SIKA-1K-PDS
	Proposed: Each penetration/outlet before membrane.
	Proposed: waterproofing subcontractor; plumbing interface role to confirm.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Penetration and outlet checklist
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	WP08
	Primer and preparation coat
	Proposed: baseline — Verify primer selection, mixing (if applicable), application and drying/overcoat readiness.
	Proposed: baseline — Observe product/batch and application; record ambient/substrate conditions where required by data sheet.
	Proposed: baseline — Primer and preparation follow current instructions for [Fill: Waterproofing system/product] on substrate [Fill: Substrate type], including stated coverage and recoat conditions. Specific project/system condition: [Fill: Primer application and readiness criteria].
	Guidance only; see Source Register: SIKA-1K-PDS
	Proposed: Each room/application batch.
	Proposed: applicator.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Primer/application log
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	WP09
	Membrane first coat
	Proposed: baseline — Inspect coverage, continuity, corners, upturns and specified reinforcement at first application.
	Proposed: baseline — Visual inspection while accessible; measure wet/dry thickness or consumption only by manufacturer/project-prescribed method.
	Proposed: baseline — Coverage, coat build-up, reinforcement and extent meet project detail [Fill: Wet-area drawings/schedule] and system instructions [Fill: Waterproofing system/product]; record actual measurements where required. Specific project/system condition: [Fill: First-coat coverage and build-up criteria].
	Guidance only; see Source Register: NCC22-HOUSE, SIKA-1K-PDS
	Proposed: Each room and coat before next coat.
	Proposed: waterproofing subcontractor; reviewer per contract.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Membrane coat application log
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	WP10
	Membrane subsequent coat(s)
	Proposed: baseline — Check subsequent coats, direction/overlap and cure/recoat interval.
	Proposed: baseline — Visual check; record coat time and conditions against product instructions.
	Proposed: baseline — Number/order of coats, continuity and recoat interval comply with approved system [Fill: Waterproofing system/product] and project detail [Fill: Wet-area drawings/schedule]. Specific project/system condition: [Fill: Subsequent-coat and recoat criteria].
	Guidance only; see Source Register: SIKA-1K-PDS
	Proposed: Every coat/room.
	Proposed: applicator.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Membrane coat and cure log
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	WP11
	Upturns and terminations
	Proposed: baseline — Inspect membrane height/extents, edges, doorway/threshold termination, hob and bath/shower details.
	Proposed: baseline — Measure only against project detail and applicable pathway; visually inspect terminations and continuity.
	Proposed: baseline — Extents and terminations match approved detail [Fill: Wet-area drawings/schedule] and applicable NCC/standard pathway [Fill: Compliance pathway]; no generic height substituted. Specific project/system condition: [Fill: Membrane extent and termination criteria].
	Guidance only; see Source Register: NCC22-HOUSE
	Proposed: Each room/termination before covering.
	Proposed: subcontractor; design reviewer where needed.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Upturn and termination checklist
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	WP12
	Curing and protection
	Proposed: baseline — Confirm cure before traffic, flood test or follow-on trade; inspect protection method.
	Proposed: baseline — Check elapsed time and conditions against manufacturer instructions; inspect protection and trade interface.
	Proposed: baseline — Membrane has reached the system-specified cure condition before test/cover; protection is compatible and does not damage membrane [Fill: Waterproofing system/product]. Specific project/system condition: [Fill: Cure and protection criteria].
	Guidance only; see Source Register: SIKA-1K-PDS
	Proposed: Each area before access, test or covering.
	Proposed: waterproofing subcontractor and builder.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Cure and protection log
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	WP13
	Specified water test
	Proposed: baseline — Where required, inspect test setup and result before finishes/concealment.
	Proposed: baseline — Use only project-approved test method, boundaries, duration and limits; document start/end, observed leakage and result.
	Proposed: baseline — Result meets the specified test criteria [Fill: Specified water test]; defects are repaired and retested before release. If no criterion is supplied, raise confirmation and do not invent a test.
	Guidance only; see Source Register: NCC22-HOUSE, CQA-ITP
	Proposed: Only where required; each test area.
	Proposed: subcontractor performs; builder/client witnesses only if contract says.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Wet-area water test record
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	WP14
	Pre-cover inspection
	Proposed: baseline — Final inspection before screed, tile, lining or other concealment.
	Proposed: baseline — Walk down complete system; verify all prior issues closed and photograph critical concealed interfaces.
	Proposed: baseline — Installed waterproofing is complete to approved drawings/system; penetrations, junctions, upturns and defects are recorded and resolved before concealment.
	Guidance only; see Source Register: NCC22-HOUSE, CQA-ITP
	Proposed: Each room/area before concealment.
	Proposed: subcontractor; builder/client reviewer if contract requires.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Pre-cover release checklist
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	WP15
	Tiling/screed interface
	Proposed: baseline — Check membrane protection and any screed/adhesive interface details before finishes.
	Proposed: baseline — Review approved detail and manufacturer compatibility; inspect that membrane is not damaged and required protection/separation is installed.
	Proposed: baseline — Interface materials and sequence match approved system [Fill: Waterproofing system/product] and detail [Fill: Wet-area drawings/schedule]; any damage is repaired by approved method before covering.
	Guidance only; see Source Register: NCC22-HOUSE, SIKA-1K-PDS
	Proposed: Each area before finishes.
	Proposed: waterproofing and tiling subcontractors; builder coordinates.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Membrane interface checklist
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	WP16
	Defects, repairs and retest
	Proposed: baseline — Track damage, pinholes, delamination or failed test; inspect repair.
	Proposed: baseline — Record defect location, approved repair method, product/batch, reinspection and retest where required.
	Proposed: baseline — Defects are closed using manufacturer-approved repair and any specified retest passes [Fill: Specified water test]; no undocumented patch accepted.
	Guidance only; see Source Register: SIKA-1K-PDS
	Proposed: Each defect/repair.
	Proposed: waterproofing subcontractor; reviewer per contract.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Waterproofing defect and repair register
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.

	WP17
	Completion and handover
	Proposed: baseline — Check required certificates, warranties, product/batch traceability, photos and maintenance information.
	Proposed: baseline — Review handover schedule and project-required documents.
	Proposed: baseline — Required handover evidence in [Fill: Compliance pathway] and contract is complete, traceable to rooms/areas, and consistent with installed system.
	Guidance only; see Source Register: CQA-ITP
	Proposed: Once per package at completion.
	Proposed: subcontractor submits; builder compiles.
	TBC
	Proposed: [Fill: reviewing role / authority assigned by project]
	Proposed: Confirm required notice period, who receives notice, release authority and whether a contractual hold/witness point applies.
	Waterproofing handover register
	Proposed: Check this baseline row against project documents; edit or remove it if it does not apply.



Inspection point key
Inspection point key: H = Proposed Hold Point - use only if assigned in the contract | W = Proposed Witness Point - use only if assigned in the contract | R = Proposed Review | S = Proposed Surveillance | TBC = To be confirmed | N/A = Not applicable. External H/W rights and whether work may proceed are governed by the project contract and approved process; proposed points require agreement.


Blank Inspection Record Forms
[Fill: project name] | waterproofing-itp-template | Record actual observations during the work. No results or signatures are pre-filled.
	ITP ID / Stage
	Inspection / method / acceptance
	Location / lot
	Date and result
	Evidence / record ref.
	Performed by / signature
	Reviewed by / signature

	WP01 | Scope and compliance basis
	Proposed: baseline — Confirm rooms, wet-area types, system limits and interfaces included.
Method: Proposed: baseline — Review approved scope, room schedule, drawings and jurisdiction/compliance pathway.
Accept when: Proposed: baseline — Included locations and waterproofing extents match the approved scope [Fill: Wet-area drawings/schedule] and pathway [Fill: Compliance pathway]; exclusions are listed.
Record: Scope and compliance basis register
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	WP02 | Product/system approval
	Proposed: baseline — Check specified membrane, primer, bond breaker, reinforcement and accessories are the approved compatible system.
Method: Proposed: baseline — Compare submittals, product labels and current manufacturer data to approved product schedule.
Accept when: Proposed: baseline — Product/system and components match approved submittal [Fill: Waterproofing system/product]; compatibility and permitted substrate/use are documented.
Record: Waterproofing product submittal register
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	WP03 | Delivery and storage
	Proposed: baseline — Check delivered product identity, batch, shelf life and storage condition.
Method: Proposed: baseline — Inspect packaging/labels and compare to approved submittal and current manufacturer storage instructions.
Accept when: Proposed: baseline — Product identity and batch are traceable; packaging is intact and within manufacturer shelf-life/storage limits [Fill: Waterproofing system/product].
Record: Waterproofing delivery and batch register
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	WP04 | Substrate readiness
	Proposed: baseline — Inspect substrate type, soundness, cleanliness, dryness/condition and surface preparation before priming.
Method: Proposed: baseline — Visual inspection; check moisture/condition using method and limit in project/manufacturer documents; record defects and remedial preparation.
Accept when: Proposed: baseline — Substrate is the approved type [Fill: Substrate type], prepared to [Fill: Waterproofing system/product] instructions, free of specified contaminants/defects, and within any stated moisture/condition limits. Specific project/system condition: [Fill: Specified substrate preparation limits].
Record: Substrate readiness checklist
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	WP05 | Falls and drainage
	Proposed: baseline — Check floor falls, floor waste position, drainage path and any step-down/threshold details before membrane.
Method: Proposed: baseline — Measure levels/falls against approved drawings and jurisdiction/code pathway; confirm waste is secure and interface detail identified.
Accept when: Proposed: baseline — Falls, waste position and threshold/step details match approved detail [Fill: Falls/drain details] and applicable compliance pathway [Fill: Compliance pathway]; missing design criteria are flagged.
Record: Falls and drainage check
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	WP06 | Junctions and movement joints
	Proposed: baseline — Inspect wall-floor junctions, internal corners, changes of plane, construction/movement joints and bond-breaker detail.
Method: Proposed: baseline — Visual check against approved detail and system instructions; record each junction type and treatment.
Accept when: Proposed: baseline — Each junction treatment is continuous and matches approved detail [Fill: Penetrations/junction details] and the compatible system instructions [Fill: Waterproofing system/product].
Record: Junction and bond-breaker checklist
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	WP07 | Penetrations and outlets
	Proposed: baseline — Check pipe penetrations, floor wastes, puddle flanges and fixtures interfaces are stable and treated.
Method: Proposed: baseline — Visual inspection and compare dimensions/details to approved drawings and system instructions.
Accept when: Proposed: baseline — Penetrations/outlets are correctly located and sealed using the specified compatible detail [Fill: Penetrations/junction details]; no untreated opening remains.
Record: Penetration and outlet checklist
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	WP08 | Primer and preparation coat
	Proposed: baseline — Verify primer selection, mixing (if applicable), application and drying/overcoat readiness.
Method: Proposed: baseline — Observe product/batch and application; record ambient/substrate conditions where required by data sheet.
Accept when: Proposed: baseline — Primer and preparation follow current instructions for [Fill: Waterproofing system/product] on substrate [Fill: Substrate type], including stated coverage and recoat conditions. Specific project/system condition: [Fill: Primer application and readiness criteria].
Record: Primer/application log
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	WP09 | Membrane first coat
	Proposed: baseline — Inspect coverage, continuity, corners, upturns and specified reinforcement at first application.
Method: Proposed: baseline — Visual inspection while accessible; measure wet/dry thickness or consumption only by manufacturer/project-prescribed method.
Accept when: Proposed: baseline — Coverage, coat build-up, reinforcement and extent meet project detail [Fill: Wet-area drawings/schedule] and system instructions [Fill: Waterproofing system/product]; record actual measurements where required. Specific project/system condition: [Fill: First-coat coverage and build-up criteria].
Record: Membrane coat application log
	
	Date: __________
Product/system: __________
Batch/lot: __________
Area/room: __________
Coat number: __________
Measured wet thickness (mm): __________
Product consumption: __________
Substrate temperature (°C): __________
Ambient temperature (°C): __________
Relative humidity (%): __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	WP10 | Membrane subsequent coat(s)
	Proposed: baseline — Check subsequent coats, direction/overlap and cure/recoat interval.
Method: Proposed: baseline — Visual check; record coat time and conditions against product instructions.
Accept when: Proposed: baseline — Number/order of coats, continuity and recoat interval comply with approved system [Fill: Waterproofing system/product] and project detail [Fill: Wet-area drawings/schedule]. Specific project/system condition: [Fill: Subsequent-coat and recoat criteria].
Record: Membrane coat and cure log
	
	Date: __________
Product/system: __________
Batch/lot: __________
Area/room: __________
Coat number: __________
Application start: __________
Application finish: __________
Ambient temperature (°C): __________
Relative humidity (%): __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	WP11 | Upturns and terminations
	Proposed: baseline — Inspect membrane height/extents, edges, doorway/threshold termination, hob and bath/shower details.
Method: Proposed: baseline — Measure only against project detail and applicable pathway; visually inspect terminations and continuity.
Accept when: Proposed: baseline — Extents and terminations match approved detail [Fill: Wet-area drawings/schedule] and applicable NCC/standard pathway [Fill: Compliance pathway]; no generic height substituted. Specific project/system condition: [Fill: Membrane extent and termination criteria].
Record: Upturn and termination checklist
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	WP12 | Curing and protection
	Proposed: baseline — Confirm cure before traffic, flood test or follow-on trade; inspect protection method.
Method: Proposed: baseline — Check elapsed time and conditions against manufacturer instructions; inspect protection and trade interface.
Accept when: Proposed: baseline — Membrane has reached the system-specified cure condition before test/cover; protection is compatible and does not damage membrane [Fill: Waterproofing system/product]. Specific project/system condition: [Fill: Cure and protection criteria].
Record: Cure and protection log
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	WP13 | Specified water test
	Proposed: baseline — Where required, inspect test setup and result before finishes/concealment.
Method: Proposed: baseline — Use only project-approved test method, boundaries, duration and limits; document start/end, observed leakage and result.
Accept when: Proposed: baseline — Result meets the specified test criteria [Fill: Specified water test]; defects are repaired and retested before release. If no criterion is supplied, raise confirmation and do not invent a test.
Record: Wet-area water test record
	
	Date: __________
Room/area: __________
Test method: __________
Start date/time: __________
End date/time: __________
Water level at start: __________
Water level at end: __________
Leakage/observations: __________
Repair/retest reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	WP14 | Pre-cover inspection
	Proposed: baseline — Final inspection before screed, tile, lining or other concealment.
Method: Proposed: baseline — Walk down complete system; verify all prior issues closed and photograph critical concealed interfaces.
Accept when: Proposed: baseline — Installed waterproofing is complete to approved drawings/system; penetrations, junctions, upturns and defects are recorded and resolved before concealment.
Record: Pre-cover release checklist
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	WP15 | Tiling/screed interface
	Proposed: baseline — Check membrane protection and any screed/adhesive interface details before finishes.
Method: Proposed: baseline — Review approved detail and manufacturer compatibility; inspect that membrane is not damaged and required protection/separation is installed.
Accept when: Proposed: baseline — Interface materials and sequence match approved system [Fill: Waterproofing system/product] and detail [Fill: Wet-area drawings/schedule]; any damage is repaired by approved method before covering.
Record: Membrane interface checklist
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	WP16 | Defects, repairs and retest
	Proposed: baseline — Track damage, pinholes, delamination or failed test; inspect repair.
Method: Proposed: baseline — Record defect location, approved repair method, product/batch, reinspection and retest where required.
Accept when: Proposed: baseline — Defects are closed using manufacturer-approved repair and any specified retest passes [Fill: Specified water test]; no undocumented patch accepted.
Record: Waterproofing defect and repair register
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	

	WP17 | Completion and handover
	Proposed: baseline — Check required certificates, warranties, product/batch traceability, photos and maintenance information.
Method: Proposed: baseline — Review handover schedule and project-required documents.
Accept when: Proposed: baseline — Required handover evidence in [Fill: Compliance pathway] and contract is complete, traceable to rooms/areas, and consistent with installed system.
Record: Waterproofing handover register
	
	Date: __________
Actual result/observation: __________
Evidence/photo/report reference: __________
Result / disposition: __________
Corrective action / retest ref.: __________
	
	
	





Source Register
	Source ID
	Title / filename
	Revision
	Type
	Path / URL

	NCC22-HOUSE
	ABCB, NCC 2022 Housing Provisions, Part 10.2 Wet area waterproofing
	See linked source; verify current edition and project adoption
	guidance
	https://ncc.abcb.gov.au/editions/ncc-2022/adopted/housing-provisions/10-health-and-amenity/part-102-wet-area-waterproofing

	NCC22-REFDOCS
	ABCB, NCC 2022 referenced documents
	See linked source; verify current edition and project adoption
	guidance
	https://ncc.abcb.gov.au/editions/ncc-2022/adopted/volume-three/2-referenced-documents/referenced-documents

	ABCB-WETAREAS
	ABCB, Waterproofing in houses
	See linked source; verify current edition and project adoption
	guidance
	https://ncc.abcb.gov.au/ncc-navigator/waterproofing-houses

	CQA-ITP
	Construction Quality Association, Guide: How to create an ITP
	See linked source; verify current edition and project adoption
	guidance
	https://www.cqa.org.au/post/guide-how-to-create-an-inspection-and-test-plan-itp

	SIKA-1K-PDS
	Sika Australia, Sikalastic-1K Product Data Sheet
	See linked source; verify current edition and project adoption
	guidance
	https://aus.sika.com/dms/getdocument.get/37ce9696-c23c-444d-9df2-02f76226b157/sikalastic_-1k.pdf



Open Confirmations
	Issue ID
	Priority
	ITP rows
	Open item
	Action needed

	CONF-001
	confirmation
	WP01
	WP01: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-002
	confirmation
	WP02
	WP02: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-003
	confirmation
	WP03
	WP03: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-004
	confirmation
	WP04
	WP04: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-005
	confirmation
	WP05
	WP05: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-006
	confirmation
	WP06
	WP06: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-007
	confirmation
	WP07
	WP07: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-008
	confirmation
	WP08
	WP08: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-009
	confirmation
	WP09
	WP09: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-010
	confirmation
	WP10
	WP10: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-011
	confirmation
	WP11
	WP11: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-012
	confirmation
	WP12
	WP12: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-013
	confirmation
	WP13
	WP13: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-014
	confirmation
	WP14
	WP14: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-015
	confirmation
	WP15
	WP15: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-016
	confirmation
	WP16
	WP16: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.

	CONF-017
	confirmation
	WP17
	WP17: verify scope and project-specific requirements for this proposed baseline row.
	Check current contract, drawings, specification, approved method, adopted standards and assigned roles; edit or delete this row as needed.







