CAVOREN  |  FIELD RECORD
Waterproofing Repair and Recheck Record
Blank project field record  |  Complete from current approved documents and site observations
Scope
Included: Internal wet-area waterproofing repair and recheck records where the project has defined a repair disposition and retained system compatibility. Tracks defect location, source evidence, approved instruction, repair materials and actual application, cure evidence as instructed, independent recheck and closure.
Excluded: Diagnosing structural movement or the cause of water ingress, designing a repair, approving substitutions, specifying product compatibility or cure values, certifying waterproofing, or authorizing concealment. Roofs, facades, tanks, below-ground work, pools and other specialist systems need a separate project-specific record.
Use and project setup
Project field: Project / contractor  ______________________________________________
Project field: Building / room / zone  ______________________________________________
Project field: Issue / NCR / defect reference  ______________________________________________
Project field: Membrane system / batch / application record  ______________________________________________
Project field: Approved repair instruction / revision  ______________________________________________
Project field: Recheck / release reference  ______________________________________________
Before inspection: Original defect and affected work extent — Map the actual room, detail, product/batch, installation history and source record; do not infer cause from appearance alone.
Before inspection: Authorized written repair disposition — The responsible designer/project authority states approved repair materials, method, extent, acceptance and any required review.
Before inspection: Compatible current system documents — Exact membrane/accessory manufacturer instructions and approved project submittal control compatibility, preparation and any cure/recoat requirements.
Before inspection: Recheck and test requirement — Specify what must be reinspected, who performs it and whether any separately authorized project test/retest is needed; no universal test is assumed.
Before inspection: Closure and release authority — Identify installer, verifier, certifier only if appointed, contractual release role and actual notice obligations.
How to use
1. Create one traceable entry per defect or linked repair location. Map room/zone, drawing/photo, affected detail and original inspection or test record.
2. Hold the affected work until an authorized written disposition identifies the repair scope, compatible system and required evidence. Do not substitute products or create cure values on this form.
3. Record actual surface preparation, product/batch, person, date/time, conditions, application evidence and any system-defined cure/recoat records against the instruction.
4. Reinspect the same mapped area after the instruction’s stated conditions are met; record findings, photos, result and any new issue. A test/retest is entered only if separately specified and authorized.
5. Keep installer completion, independent verifier findings and formal project/certifier release attributed to the person and authority that actually acted.
Important: Blank record. A project-authorized person supplies the repair disposition and acceptance criteria, checked against the exact compatible system and current local instructions. Actual repair, cure evidence, recheck result, dates and signatures remain blank until performed. Installer self-check, independent inspection and formal release are separate records.


Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	WPR-01  Defect identity and location


	What to observe
	Register the original issue, affected waterproofing system and precisely mapped area/detail.

	How to check
	Link the source inspection/test/NCR record; map room, surface, junction or penetration on approved drawing/photo; record product and batch only where evidenced.

	Acceptance basis
	Issue extent and history are traceable; the record does not assign cause or expand repair limits without authorized review.

	Reference to verify
	Original ITP/checklist/test/NCR, approved area detail and product/batch records.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Issue / NCR ID
	



	Room / surface / detail
	



	Observed extent / map ref
	



	Product / batch / application ref
	



	Original finding / photo ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	WPR-02  Authorized repair disposition


	What to observe
	Confirm the responsible authority has issued a written repair instruction for the identified defect and scope.

	How to check
	Record issuer, role, date, instruction revision, preparation/method, accepted materials, extent, criteria and required inspection/test/notice points; refer missing elements.

	Acceptance basis
	Repair starts only to a current authorized disposition that controls the identified location, method, compatible materials and closure evidence.

	Reference to verify
	Approved repair instruction/design disposition, project specification/ITP and approved product submittal.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Disposition / revision
	



	Author / role / date
	



	Approved repair scope
	



	Approved repair products
	



	Acceptance / recheck criteria
	



	Required notice / witness ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	WPR-03  System compatibility and preparation


	What to observe
	Record confirmation that repair materials and surface preparation follow the approved compatible system and exact current instructions.

	How to check
	Compare selected products, primers/accessories and substrate condition with current manufacturer documentation and project submittal; identify revision, area and any written exception approval.

	Acceptance basis
	Compatibility and preparation are supported by the exact approved source and disposition; no generic compatibility or preparation value is supplied.

	Reference to verify
	Current local TDS/instructions for the actual membrane, primer and accessories; approved repair disposition.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Membrane system / revision
	



	Repair material / batch
	



	Preparation / method ref
	



	TDS / revision / clause
	



	Exception / approval ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	WPR-04  Actual repair application and traceability


	What to observe
	Document the repair as actually performed and link it to each mapped affected location.

	How to check
	Record applicator, date/time, location, batch/expiry where stated, method, observed conditions, layers/accessories and contemporaneous photo or log refs per the approved instruction.

	Acceptance basis
	Actual work and materials are traceable to the authorized disposition; blank record fields are not evidence of completed work.

	Reference to verify
	Approved repair disposition, product labels/batch records, current TDS and dated site evidence.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Repair location / detail
	



	Actual method / layer
	



	Product / batch / expiry
	



	Actual conditions / measurement
	



	Installer / role / date/time
	



	Photo / application log ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	WPR-05  Cure / recoat / protection conditions


	What to observe
	Record any system-specific cure, recoat, protection or covering condition required for the repair before reinspection or follow-on work.

	How to check
	Use the exact current local system instructions and authorized project direction; enter actual timing and required conditions with units and evidence only where specified.

	Acceptance basis
	Readiness follows the controlling current system and project documents; this record supplies no cure time, environmental limit or permission to cover.

	Reference to verify
	Exact approved system TDS revision, actual repair log and project disposition.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Repair completion date/time
	



	Actual condition / units
	



	Source-defined condition / reference
	



	Protection / access note
	



	Reviewer / role / date
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	WPR-06  Reinspection and specified retest


	What to observe
	Recheck the same mapped repair and record actual observation, test/retest evidence only when specifically required, and unresolved defects.

	How to check
	Use project-defined visual/instrument method and acceptance; map photos to original defect; conduct no flood/performance test without explicit approved requirement, feasible setup and responsible-party method.

	Acceptance basis
	Repair status is compared with the authorized disposition. A test occurs only if explicitly required and separately authorized; no generic test or automatic Pass is implied.

	Reference to verify
	Repair disposition, current product instructions and project reinspection/test procedure if specified.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Rechecked location
	



	Recheck method / criteria ref
	



	Actual observation / measurement
	



	Specified test / N/A basis
	



	Actual result / Pending / Failed
	



	Photo / report ref
	



	Inspector / role / date
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	WPR-07  Issue closure and formal release


	What to observe
	Record installer completion, verifier decision, unresolved NCRs and any project or certifier release separately.

	How to check
	Trace each decision to actual person, role, date, scope and document; confirm the next work/concealment status against contract and ITP.

	Acceptance basis
	Issue is closed only by the designated authority under documented project rules; repair completion or a visual observation does not itself certify compliance or release the area.

	Reference to verify
	Project ITP/contract, appointment/authority documents, repair/recheck report and written release.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Installer statement / role / date
	



	Verifier finding / role / date
	



	Open issue / disposition ref
	



	Formal decision / authority / date
	



	Certificate / release / dossier ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Issues and corrective action
Project: _____________________  Location / room / element: _____________________  Inspection date: _____________________
	Item / date
	Issue and immediate action
	Disposition / corrective instruction
	Recheck evidence / date
	Responsible role / reference

	


	


	


	


	



	


	


	


	


	



	


	


	


	


	



	


	


	


	


	



	


	


	


	


	




Unresolved items: identify affected area, status, person notified, instruction / NCR reference and any condition before concealment or next work.


Repair / recheck status
Project: _____________________  Location / room / element: _____________________  Date: _____________________
Repair closure status
[  ] Repair rechecked — formal release evidenced
[  ] Hold — further repair or recheck required
[  ] Disposition / verifier / release pending
Mark complete only when the authorized instruction, actual repair evidence, any required recheck and separate release decision are linked. Installer completion alone does not certify or release the area.
Handover roles and references
Repair installer / role / date  ______________________________________________
Independent/site verifier / role / date  ______________________________________________
Certifier only if appointed/required / reference  ______________________________________________
Contract release authority / decision reference  ______________________________________________
Signatures record the named person’s stated role and entry only. They do not by themselves approve design, certify compliance, release a contractual control point or authorize the next activity.


Source notes
These references explain topic and record design. They do not supply universal project acceptance values. Confirm the contract documents, applicable jurisdiction and approved product/system before use.
ABCB, NCC 2022 Housing Provisions, Part 10.2 Wet area waterproofing
Role: Official topic reference from NCC 2022 Housing Provisions, including the variations shown on that page. Confirm the project building class, compliance pathway, adopted edition and relevant state/territory variations before using any provision. This reference does not set universal acceptance criteria.
Locator: Clauses 10.2.1–10.2.32; especially 10.2.6–10.2.13, 10.2.22–10.2.30
Source URL: https://ncc.abcb.gov.au/editions/ncc-2022/adopted/housing-provisions/10-health-and-amenity/part-102-wet-area-waterproofing
ABCB, Waterproofing in houses
Role: Official introduction for Class 1 houses. Its national overview omits state/territory variations and does not establish requirements for other building classes or compliance pathways.
Locator: Scope/target audience and sections on NCC 2022 Volume Two H4, Housing Provisions Part 10.2 and AS 3740 options
Source URL: https://ncc.abcb.gov.au/ncc-navigator/waterproofing-houses
ABCB, Editions of the National Construction Code
Role: Official NCC edition index. Use it with the project documents and jurisdictional adoption/transition rules to identify the governing edition. Publication of a code edition does not by itself establish which edition applies to a particular project.
Locator: Edition and amendment listings; then consult the project jurisdiction for adoption and transition provisions
Source URL: https://ncc.abcb.gov.au/editions-national-construction-code
ARDEX Australia, WPM 155 Rapid Plus Technical Data Sheet
Role: First-party example of one internal/external under-tile system. Supports prompts to record substrate preparation, selected primer, junction/detail method, application coats, product-specific coverage/film build, curing and pre-cover inspection. Any manufacturer values apply only when this exact product/system is approved and the current local data sheet is verified; none are prefilled as generic acceptance criteria.
Locator: January 2025 issue, pp. 1–3: substrate preparation, primer, detailing, application, curing, flood testing and tiling; manufacturer warns newer revision may exist
Source URL: https://ardexaustralia.com/pdf/products/datasheets/waterproofing/ARDEX%20WPM%20155%20Rapid%20Plus%20Datasheet.pdf
Sika Australia, Sika SealTape F Product Data Sheet
Role: First-party accessory example for compatible Sika systems; supports documenting substrate cleanliness/priming, embedding, tape continuity/overlaps and membrane coat interface. Requirements are accessory/system specific and only apply after checking the selected membrane TDS and approval.
Locator: December 2025 version 05.01, pp. 1–2, substrate preparation and application instructions
Source URL: https://aus.sika.com/dms/getdocument.get/51447514-2e04-49ff-83cc-a4274d6f5191/sika-sealtape-f.pdf
Construction Quality Association, Guide: How to create an ITP
Role: ITP record design guidance only: identify what is checked, how, against what source, who records it, and what evidence follows. It supplies no waterproofing technical acceptance criteria.
Locator: Whole article; ITP requirement/inspection/evidence structure
Source URL: https://www.cqa.org.au/post/guide-how-to-create-an-inspection-and-test-plan-itp
https://itp.cavoren.net/checklists/waterproofing-repair-recheck/  |  Project: __________________________  |  Page 




