CAVOREN  |  FIELD RECORD
Wet Area Flood Test Record
Blank project field record  |  Complete from current approved documents and site observations
Scope
Included: Record only a water test that the project explicitly requires, the responsible project authority has confirmed is feasible for the actual membrane, substrate, room, drain system, structure and programme, and that a competent responsible party has provided an approved method for. Supports internal wet-area membrane work only.
Excluded: Does not prescribe or authorize a flood test; does not set test depth, duration, isolation method, allowable leakage, acceptance, safety controls or responsibility. Does not replace manufacturer instructions, a project test procedure, design review, building/certifier approval or project release. If no explicit approved requirement and method exist, do not perform a test using this form.
Use and project setup
Project field: Project / contractor  ______________________________________________
Project field: Building / room / zone  ______________________________________________
Project field: Membrane system and application record  ______________________________________________
Project field: Approved test procedure / revision  ______________________________________________
Project field: Test request / approval reference  ______________________________________________
Project field: Test area / isolation boundary  ______________________________________________
Before inspection: Explicit project requirement and authority — Record the exact specification/ITP requirement and person authorized to direct the test; an assumed practice is insufficient.
Before inspection: Written feasibility review for this installation — Confirm the actual membrane/product, substrate, drains, penetrations, adjacent construction, structural loading and site constraints are suitable under the project decision.
Before inspection: Approved test method and acceptance criteria — The responsible project party supplies area, isolation, setup, medium, any level or duration, observations, acceptance, stop rules and witness roles; this blank form invents none.
Before inspection: Current membrane system instructions and cure evidence — The selected compatible system documentation controls cure and any test suitability or restriction.
Before inspection: Notice, witness and release responsibilities — Identify installer, competent test operator, verifier, certifier only if appointed, and formal release authority separately.
How to use
1. Before any setup, attach the explicit project requirement, written feasibility decision and approved procedure. If any is absent or conflicts with current product instructions, mark Hold / Refer and do not test.
2. Use the responsible party’s procedure verbatim for area, isolation, setup, test medium, values, duration, observation and stop conditions. This record supplies no defaults.
3. Record actual setup and baseline condition before commencement; link each observation to room/zone and time. Stop and report unexpected leakage, movement or damage under the approved procedure.
4. Record actual result and any defect, repair instruction and recheck separately. A repair does not inherit the original test result; follow the approved repair and retest decision.
5. Record installer, test operator, verifier, witness and release authority with actual role, date and reference. A passed record does not by itself certify compliance or authorize concealment.
Important: Blank record only. A test is undertaken only where the actual project documents explicitly require it and the responsible authority has confirmed feasibility and provided the approved method and acceptance criteria. Complete conditions, readings, dates, witnesses and signatures from actual records only; keep blank until performed. This record does not grant authority to test or certify the membrane.


Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	WFT-01  Requirement and authorization


	What to observe
	Verify an explicit project requirement, responsible direction and approved procedure exist before test setup.

	How to check
	Review the controlled specification/ITP, written test instruction and procedure revision; record any conflict or missing authorization.

	Acceptance basis
	Proceed only when the identified project authority has explicitly required and authorized the test and an approved method is available; otherwise status remains Pending / Hold.

	Reference to verify
	Project specification / ITP, written instruction and approved test procedure (exact reference required).

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Requirement / clause / revision
	



	Directing person / role
	



	Procedure / revision
	



	Authorization status
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	WFT-02  Installation suitability and feasibility


	What to observe
	Record the project’s written feasibility decision for this actual installed system and proposed test area.

	How to check
	Link membrane/system and cure records, substrate and drain details, structural/design review where applicable, adjacent work constraints and product-supplier information to the responsible authority’s decision.

	Acceptance basis
	Suitability is accepted only by the assigned responsible authority using project evidence; the blank checklist makes no universal flood-test claim and does not establish feasibility itself.

	Reference to verify
	Written project/design feasibility review, current exact product instructions and approved area details.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Membrane / batch / system ref
	



	Cure/application record ref
	



	Area / drain / boundary
	



	Feasibility decision / author / date
	



	Conditions / restrictions
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	WFT-03  Method, limits and setup plan


	What to observe
	Confirm the responsible party’s method fully defines the proposed setup, measurements, acceptance, monitoring, stop criteria and witnesses.

	How to check
	Transcribe references to the approved procedure; do not create a test level, hold period, isolation approach, allowable change or acceptance rule on this form.

	Acceptance basis
	Every test criterion and method is traceable to the approved procedure and current compatible system; any missing or conflicting item means do not test and remain Pending.

	Reference to verify
	Approved project test procedure and current product-system instructions (exact revision and clauses).

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Method / procedure clause
	



	Setup / isolation reference
	



	Acceptance criteria reference
	



	Stop / contingency criteria ref
	



	Required witness / notice ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	WFT-04  Pre-test area and baseline condition


	What to observe
	Document the actual test boundary and visible condition before filling or otherwise commencing the approved test.

	How to check
	Walk the approved area and record room/zone, isolation boundaries, drain/penetration condition, adjacent surfaces, existing defects, photo references and actual starting observations using the approved procedure.

	Acceptance basis
	The area and baseline are traceable to the procedure; pre-existing damage, inaccessible interfaces or unapproved changes are resolved before test commencement.

	Reference to verify
	Approved test procedure, room drawing, membrane application and pre-cover inspection records.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Room / zone / test boundary
	



	Baseline condition / observation
	



	Pre-existing defect / location
	



	Photo / plan refs
	



	Inspector role / date
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	WFT-05  Approved test setup and actual observations


	What to observe
	Record actual setup and observations at the times and locations specified by the responsible party’s procedure.

	How to check
	A competent designated operator follows the approved method; enter actual readings with units, equipment IDs, times and witness initials in attached contemporaneous records. Stop or escalate per method if conditions deviate.

	Acceptance basis
	Observed values and conditions are attributable to actual records and compared only with the specified criteria; no assumed test duration, water depth, leakage threshold or automatic pass is provided.

	Reference to verify
	Approved procedure, original field log, calibrated/identified equipment record where required.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Actual setup / medium
	



	Actual start date/time
	



	Actual reading / unit / time
	



	Equipment ID / calibration ref
	



	Operator / role
	



	Witness / role / observation
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	WFT-06  Completion, result and anomalies


	What to observe
	Record actual completion status, observed condition and responsible reviewer’s result against the approved criteria.

	How to check
	Reinspect the test area and adjacent accessible spaces as directed; attach original log/photos and identify any departure, interruption, leakage, unexplained level change or damage.

	Acceptance basis
	Result is reported against the approved method and criterion by the assigned reviewer; interruption, anomaly or missing evidence is not represented as Pass.

	Reference to verify
	Approved procedure, attached original observations and project acceptance/review authority.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Actual finish date/time
	



	Final observed condition
	



	Actual result / Pending / Failed
	



	Anomaly / interruption ref
	



	Reviewer / role / date
	



	Report / photo refs
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	WFT-07  Repair, retest and formal release


	What to observe
	Link any repair and separately required re-test, then record the actual project decision for concealment or next work.

	How to check
	Use an approved repair disposition and current compatible system instructions; obtain a new method/direction for retesting and keep original and later results distinct. Record contractual/certifier releases only when issued.

	Acceptance basis
	Repair, recheck and formal release are separately evidenced by their actual authorities; test completion alone does not certify compliance or authorize covering.

	Reference to verify
	Approved repair instruction, repair record, any new test procedure, project ITP/contract and written release.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Repair / NCR / disposition ref
	



	Recheck / retest report ref
	



	Installer / role / date
	



	Verifier / role / date
	



	Release decision / authority / ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Issues and corrective action
Project: _____________________  Location / room / element: _____________________  Inspection date: _____________________
	Item / date
	Issue and immediate action
	Disposition / corrective instruction
	Recheck evidence / date
	Responsible role / reference

	


	


	


	


	



	


	


	


	


	



	


	


	


	


	



	


	


	


	


	



	


	


	


	


	




Unresolved items: identify affected area, status, person notified, instruction / NCR reference and any condition before concealment or next work.


Test / cover status
Project: _____________________  Location / room / element: _____________________  Date: _____________________
Test and next-work status
[  ] Test recorded — separate project release evidenced
[  ] Hold — anomaly, repair or retest required
[  ] No approved test basis / formal release pending
Select a test-complete state only when its actual approved procedure and observations are attached. Test completion does not itself certify compliance or authorize covering; record the separately appointed authority’s decision.
Handover roles and references
Test operator / role / date  ______________________________________________
Installer / role / date  ______________________________________________
Verifier / witness / role / date  ______________________________________________
Formal release authority / decision reference  ______________________________________________
Signatures record the named person’s stated role and entry only. They do not by themselves approve design, certify compliance, release a contractual control point or authorize the next activity.


Source notes
These references explain topic and record design. They do not supply universal project acceptance values. Confirm the contract documents, applicable jurisdiction and approved product/system before use.
ABCB, NCC 2022 Housing Provisions, Part 10.2 Wet area waterproofing
Role: Official topic reference from NCC 2022 Housing Provisions, including the variations shown on that page. Confirm the project building class, compliance pathway, adopted edition and relevant state/territory variations before using any provision. This reference does not set universal acceptance criteria.
Locator: Clauses 10.2.1–10.2.32; especially 10.2.6–10.2.13, 10.2.22–10.2.30
Source URL: https://ncc.abcb.gov.au/editions/ncc-2022/adopted/housing-provisions/10-health-and-amenity/part-102-wet-area-waterproofing
ABCB, Waterproofing in houses
Role: Official introduction for Class 1 houses. Its national overview omits state/territory variations and does not establish requirements for other building classes or compliance pathways.
Locator: Scope/target audience and sections on NCC 2022 Volume Two H4, Housing Provisions Part 10.2 and AS 3740 options
Source URL: https://ncc.abcb.gov.au/ncc-navigator/waterproofing-houses
ABCB, Editions of the National Construction Code
Role: Official NCC edition index. Use it with the project documents and jurisdictional adoption/transition rules to identify the governing edition. Publication of a code edition does not by itself establish which edition applies to a particular project.
Locator: Edition and amendment listings; then consult the project jurisdiction for adoption and transition provisions
Source URL: https://ncc.abcb.gov.au/editions-national-construction-code
ARDEX Australia, WPM 155 Rapid Plus Technical Data Sheet
Role: First-party example of one internal/external under-tile system. Supports prompts to record substrate preparation, selected primer, junction/detail method, application coats, product-specific coverage/film build, curing and pre-cover inspection. Any manufacturer values apply only when this exact product/system is approved and the current local data sheet is verified; none are prefilled as generic acceptance criteria.
Locator: January 2025 issue, pp. 1–3: substrate preparation, primer, detailing, application, curing, flood testing and tiling; manufacturer warns newer revision may exist
Source URL: https://ardexaustralia.com/pdf/products/datasheets/waterproofing/ARDEX%20WPM%20155%20Rapid%20Plus%20Datasheet.pdf
Sika Australia, Sika SealTape F Product Data Sheet
Role: First-party accessory example for compatible Sika systems; supports documenting substrate cleanliness/priming, embedding, tape continuity/overlaps and membrane coat interface. Requirements are accessory/system specific and only apply after checking the selected membrane TDS and approval.
Locator: December 2025 version 05.01, pp. 1–2, substrate preparation and application instructions
Source URL: https://aus.sika.com/dms/getdocument.get/51447514-2e04-49ff-83cc-a4274d6f5191/sika-sealtape-f.pdf
Construction Quality Association, Guide: How to create an ITP
Role: ITP record design guidance only: identify what is checked, how, against what source, who records it, and what evidence follows. It supplies no waterproofing technical acceptance criteria.
Locator: Whole article; ITP requirement/inspection/evidence structure
Source URL: https://www.cqa.org.au/post/guide-how-to-create-an-inspection-and-test-plan-itp
https://itp.cavoren.net/checklists/wet-area-flood-test/  |  Project: __________________________  |  Page 




