CAVOREN  |  FIELD RECORD
Concrete Curing and Protection Record
Blank project field record  |  Complete from current approved documents and site observations
Scope
Included: Curing/protection observation for ordinary cast-in-place concrete after placement/finishing through the project-defined closeout, including traceability if an approved product is used.
Excluded: Setting universal duration/environment limits; approving a method or product; prescribing application technique; testing concrete strength; certification; permission to strip, load or proceed.
Use and project setup
Project field: Project / contractor  ______________________________________________
Project field: Element / grid / curing-zone map  ______________________________________________
Project field: Pour / lot / placement record  ______________________________________________
Project field: Approved method / procedure rev  ______________________________________________
Project field: Product / batch / TDS rev if used  ______________________________________________
Project field: Start / monitoring log refs  ______________________________________________
Project field: Interruption / repair / NCR ref  ______________________________________________
Project field: Recorder / reviewer roles  ______________________________________________
Before inspection: Approved project curing method/procedure and concrete specification — Defines method, start trigger, duration, environmental checks and record requirements.
Before inspection: Element/zone map and placement/finish log — Connects curing area to the actual concrete lot and start event.
Before inspection: Exact approved product/TDS/submittal if used — Product compatibility and use conditions depend on current specific system.
Before inspection: Project monitoring and interruption response — Supplies actual readings, evidence intervals and corrective action path.
Before inspection: Protection and separate stripping/loading release criteria — Keeps curing observation distinct from design or contractual permission for later work.
How to use
1. Identify exact area/element, approved method, project-specific time/monitoring criteria and product evidence if applicable.
2. Record actual finishing/placement handover and observed curing start with source log.
3. Log only actual conditions and project-required measurements with time, unit, method/instrument and evidence.
4. Map interruption, exposure, damage, repair and recheck; do not infer continuity from appearance alone.
5. Close the curing record only against project criteria and keep any separate structural/contractual release with its assigned role.
6. Use the curing log for repeat entries; continue on another blank copy when needed and retain the linked original evidence.
Important: Blank field record. Use actual project method and product instructions, record observed events/measurements only, and obtain separate release where required. Curing records do not establish strength or loading permission.


Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	CC-01  Element, area and approved curing basis


	What to observe
	Concrete lot and mapped zone, placement/finish record, current curing procedure/revision, specified duration/monitoring basis and assigned role.

	How to check
	Reconcile actual area to pour map; review controlled project documents and note which conditions apply to each zone.

	Acceptance basis
	The actual zone and pour can be matched to the approved curing basis and required monitoring/closeout criteria. Missing method, duration or zone applicability is identified for direction; no generic curing period is assumed.

	Reference to verify
	Approved project curing procedure and concrete specification clauses, element/zone map, placement/finish record and assigned monitoring roles.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Element / grid / zone map
	



	Pour lot / placement ref
	



	Curing procedure / revision
	



	Duration / monitoring clause
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	CC-02  Method and product traceability


	What to observe
	Actual method observed; where compound/proprietary product is used, product name, batch, current data sheet and approval/submittal.

	How to check
	Compare label and actual application to approved project submittal; link batch and application evidence.

	Acceptance basis
	Observed method and any product identity/batch are consistent with the approved submittal and exact applicable instructions, with discrepancies recorded. Suitability or compatibility is confirmed by the project evidence rather than this form.

	Reference to verify
	Approved curing method/product submittal, exact product data sheet and revision if used, product label/batch and actual application record.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Method observed / date
	



	Product / batch if used
	



	Current TDS / approval ref
	



	Application evidence / discrepancy
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	CC-03  Observed curing start and initial application


	What to observe
	Actual finishing/placement handover, observed curing start time, initial protected condition and installer/observer.

	How to check
	Use contemporaneous site record; distinguish actual event from planned schedule. Attach dated observation evidence.

	Acceptance basis
	The recorded start event and initial condition are traceable to contemporaneous evidence and checked against the project-defined trigger/instructions. An unknown or late start is identified for assigned disposition, without a default time window.

	Reference to verify
	Project procedure defining the curing start trigger, applicable approved product instructions and contemporaneous placement/finish/curing-start log.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Finish / placement handover time
	



	Actual start time / date
	



	Area / initial condition
	



	Observer role / evidence ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	CC-04  Continuity and project-defined duration


	What to observe
	Dated monitoring entries, observed coverage/condition by mapped area, project-required intervals and interruptions/inaccessible area.

	How to check
	Use the actual monitoring plan and dated log; map any gap and connect it to the instruction and evidence.

	Acceptance basis
	Dated observations cover the required zones and monitoring basis, with continuity, gaps and end evidence checked against the actual project criteria. Interruption or inaccessible areas remain identified; a planned duration is not proof of completion.

	Reference to verify
	Project monitoring plan and duration/condition clause, area map, dated curing log and any interruption/inaccessible-area disposition.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Monitoring times / observers
	



	Zone / condition observed
	



	Project interval / duration clause
	



	Interruption period / affected area
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	CC-05  Environmental evidence required by project


	What to observe
	Actual weather/ambient/element observation and measured readings only where project requires; units, times, instrument/method and source.

	How to check
	Record actual readings with instrument ID and evidence; if no measurement required, state factual observation rather than estimate.

	Acceptance basis
	Any required reading has a recorded parameter, unit, time/location, method/instrument and evidence source, and is assessed only against the project criterion. Estimated or unavailable measurements are not presented as actual readings.

	Reference to verify
	Project procedure requiring the specific environmental parameter, measurement method and frequency, plus actual instrument/log/weather evidence.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Required parameter / exact clause
	



	Actual value / unit if measured
	



	Time / location / instrument
	



	Log / photo / weather source ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	CC-06  Protection, disruption, repair and recheck


	What to observe
	Protection/access condition, interruption or exposure, damage/contamination, affected area/time, approved action and reinspection.

	How to check
	Walk the defined zone; map observations and link photos, instruction, repair and recheck evidence.

	Acceptance basis
	Protection condition, disruption and damage are recorded by affected zone/time, with corrective instruction and recheck evidence linked. Outstanding issues are carried forward; protection observations do not establish in-place strength.

	Reference to verify
	Project protection/access method, mapped observation/photo, written corrective instruction or repair/NCR and recheck record.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Protection / affected area
	



	Interruption / damage and time
	



	Instruction / NCR / repair ref
	



	Recheck evidence / date
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	CC-07  Curing closeout and separate project release


	What to observe
	Project-required log completion evidence, open exceptions, contractor closeout, reviewer record and any separate stripping/loading/follow-on release.

	How to check
	Check dated log against exact project criteria; keep contractor completion, technical review and contractual release separate.

	Acceptance basis
	The project-required curing logs and closure evidence have been reviewed by the assigned role, with open conditions recorded. Any separate structural/contractual release remains separately evidenced; this log cannot authorise stripping or loading.

	Reference to verify
	Project curing-closeout criteria and evidence register, assigned review arrangements and separate stripping/loading release documents where required.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Completion criterion / clause
	



	Evidence pack / log ref
	



	Open issue disposition ref
	



	Recorder / assigned reviewer roles and dates
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Curing log
Use one row per actual area monitoring event. Enter the project method, criteria and required monitoring basis in the check pages first. Record actual observed conditions/readings and interruption actions, not an inferred continuous history. Continue on another copy as needed.
Project / contract: ______________________________    Element / pour / lot: ______________________________    Date / shift: ____________________
Location / area: ______________________________    Record reference / revision: ______________________________
	Observation date / time
	Element / zone / pour
	Method / procedure ref
	Start / event log ref
	Actual condition observed
	Reading / unit / method if required
	Interruption / affected area ref
	Action / recheck ref
	Observer / evidence ref

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 




Issues and corrective action
Project: _____________________  Location / room / element: _____________________  Inspection date: _____________________
	Item / date
	Issue and immediate action
	Disposition / corrective instruction
	Recheck evidence / date
	Responsible role / reference

	


	


	


	


	



	


	


	


	


	



	


	


	


	


	



	


	


	


	


	



	


	


	


	


	




Unresolved items: identify affected area, status, person notified, instruction / NCR reference and any condition before concealment or next work.


Concrete curing and protection handover
Project: _____________________  Location / room / element: _____________________  Date: _____________________
Record handover status
[  ] Record completed; evidence filed
[  ] Action or recheck remains open
[  ] Project / technical disposition required
This status reports curing evidence and open actions only. It does not establish in-place strength, certify compliance, release a contractual point or authorize stripping, loading or follow-on work.
Handover roles and references
Curing recorder / installer role / date  ______________________________________________
Assigned curing reviewer role / date  ______________________________________________
Separate project release role / reference if required  ______________________________________________
Open NCR / repair / disposition ref  ______________________________________________
Signatures record the named person’s stated role and entry only. They do not by themselves approve design, certify compliance, release a contractual control point or authorize the next activity.


Source notes
These references explain topic and record design. They do not supply universal project acceptance values. Confirm the contract documents, applicable jurisdiction and approved product/system before use.
Cavoren cast-in-place concrete baseline
Role: Scope context only; not independent technical authority or project acceptance criteria.
Locator: Original proposed curing/protection topic CON-13 and closeout interface CON-15.
Source URL: https://itp.cavoren.net/templates/concrete/
Queensland Department of Transport and Main Roads, MRTS70 Concrete (July 2022)
Role: Topic guidance only. MRTS70 is for Queensland road/bridge infrastructure contracts (or other specified elements). Its values, timing limits, test frequencies, qualifications, H/W points, project roles and release rules are not generalized into these records.
Locator: July 2022, 17.15 (normal-class concrete curing topics), 15.11 (in-situ curing) and 14 (defects/rectification). Verify the applicable project method and adopted provisions; no duration is transferred.
Source URL: https://www.tmr.qld.gov.au/-/media/busind/techstdpubs/Specifications-and-drawings/Specifications/2-Bridges-and-Structures/MRTS70.pdf
Hutchies 040 Concrete Place Report (public Word report template)
Role: Contractor-specific example of report layout and handover, not universal criteria. No Hutchies text is reproduced.
Locator: Public 040 Concrete Place Report: header and closeout fields, rows 6–13 on discharge, placement, protection, curing and final records review. Contractor example only; no technical acceptance conditions are adopted.
Source URL: https://toolbox.hutchies.com.au/uploads/040-Concrete-Place-Report.docx
https://itp.cavoren.net/checklists/concrete-curing/  |  Project: __________________________  |  Page 




