Pre-Pour Inspection Checklist
Cavoren ITP  |  Pre-pour field record  |  Blank form for project completion
Pre-placement checks for ordinary cast-in-place concrete slabs, pad footings and strip footings: document readiness, set-out and founding, formwork, reinforcement, cast-in items and joints, cleanliness/access, and recording the project release decision.
Scope: Does not cover concrete delivery or testing, placement, compaction, finishing, curing, post-pour inspection, precast, prestressing, shotcrete, piles, specialist repair, or project-specific design/engineering approval. Add separate records where those scopes apply. Blank generic record for project adaptation. Complete each acceptance requirement and reference from current approved project documents before use. No standard engineering values, inspection results, release, certification or approval are supplied. A checklist entry is not a contractual Hold or Witness Point unless the project assigns it.
	Project / contractor / client
	

	Element / pour number
	


	Location / grid
	

	Inspection date / drawing revision
	




	Check
	Project requirement and document reference
	Site record

	PP-01 Project documents and pour identification
Confirm this checklist identifies the correct project, element and pour; check current approved drawings, specification, mix approval and required test arrangements are available.
	Project acceptance / values:
________________________
Drawing / spec ref and revision:
________________________
	Result: Pass / Fail / N/A / Pending
Observation / measurement: __________
Issue / evidence ref: ________________
Inspector initials / date: ____________
Recheck ref / date: _________________

	PP-02 Set-out and dimensions
Check element location, grid references, dimensions and levels against the approved drawings.
	Project acceptance / values:
________________________
Drawing / spec ref and revision:
________________________
	Result: Pass / Fail / N/A / Pending
Observation / measurement: __________
Issue / evidence ref: ________________
Inspector initials / date: ____________
Recheck ref / date: _________________

	PP-03 Founding or substrate
Check exposed founding surface or substrate type, level and condition; confirm any required geotechnical or design release is recorded.
	Project acceptance / values:
________________________
Drawing / spec ref and revision:
________________________
	Result: Pass / Fail / N/A / Pending
Observation / measurement: __________
Issue / evidence ref: ________________
Inspector initials / date: ____________
Recheck ref / date: _________________

	PP-04 Formwork and temporary works
Check formwork line, level, dimensions, support/bracing, tightness, cleanliness, release-agent condition and access for placement.
	Project acceptance / values:
________________________
Drawing / spec ref and revision:
________________________
	Result: Pass / Fail / N/A / Pending
Observation / measurement: __________
Issue / evidence ref: ________________
Inspector initials / date: ____________
Recheck ref / date: _________________


Record one result per applicable check. Enter criteria and references from current approved project documents; mark N/A with a reason. Use page 3 for detailed corrective action, rechecks and the release record.


Pre-pour checks continued
Project: ______________________________   Element / pour: ______________________________   Location / grid: ______________________________
	Check
	Project requirement and document reference
	Site record

	PP-05 Reinforcement identification and traceability
Check reinforcement type, size and identification against the approved bar schedule; confirm project-required certificates or traceability records are available.
	Project acceptance / values:
________________________
Drawing / spec ref and revision:
________________________
	Result: Pass / Fail / N/A / Pending
Observation / measurement: __________
Issue / evidence ref: ________________
Inspector initials / date: ____________
Recheck ref / date: _________________

	PP-06 Reinforcement placement and cover
Check bar arrangement, spacing, laps, anchorage, supports, specified cover and congestion against structural details.
	Project acceptance / values:
________________________
Drawing / spec ref and revision:
________________________
	Result: Pass / Fail / N/A / Pending
Observation / measurement: __________
Issue / evidence ref: ________________
Inspector initials / date: ____________
Recheck ref / date: _________________

	PP-07 Cast-in items, services and joints
Check applicable cast-in plates, bolts, sleeves, conduits, waterstops, construction/isolation joints and other embedded items for type, location, level and secure fixing.
	Project acceptance / values:
________________________
Drawing / spec ref and revision:
________________________
	Result: Pass / Fail / N/A / Pending
Observation / measurement: __________
Issue / evidence ref: ________________
Inspector initials / date: ____________
Recheck ref / date: _________________

	PP-08 Pre-pour area readiness and release
Confirm preceding checks are complete, debris and standing water are addressed as required by project documents, access is ready, open issues are dispositioned, and the required project release decision is recorded.
	Project acceptance / values:
________________________
Drawing / spec ref and revision:
________________________
	Result: Pass / Fail / N/A / Pending
Observation / measurement: __________
Issue / evidence ref: ________________
Inspector initials / date: ____________
Recheck ref / date: _________________




Issues, rechecks and pour release
Project: ______________________________   Element / pour: ______________________________   Location / grid: ______________________________
	Item / date
	Issue / corrective action
	Disposition / recheck
	Evidence reference
	Responsible person / sign / date

	


	


	


	


	



	


	


	


	


	



	


	


	


	


	



	


	


	


	


	



	


	


	


	


	




Release decision:   ☐ Ready to pour   ☐ Not released   ☐ Pending conditions   Date / time: ____________________
Open conditions / release basis / required client notice: ________________________________________________________________
Contractor representative name / signature: __________________________________________   Date / time: __________________
Client / reviewer name / signature (only if required by project): _________________________   Date / time: __________________
Do not treat this record as a contractual Hold / Witness Point unless the project documents assign that status. Release authority and notice follow the contract.
Source note: Cavoren concrete baseline CON-01 to CON-08; Queensland TMR MRTS70 Concrete (July 2022) is transport-specific topic evidence only; Hutchies public examples corroborate broad sequencing. None supplies universal project acceptance values.
Cavoren ITP  |  Public checklist page: https://itp.cavoren.net/checklists/pre-pour/




