CAVOREN  |  FIELD RECORD
Building Water Service Pressure Test Record
Blank project field record  |  Complete from current approved documents and site observations
Scope
Included: Blank site record for ordinary building cold, heated or other specifically identified water-service sections only where a project-approved pressure test applies.
Excluded: Designing or prescribing a test; universal pressure, duration, medium, test sequence or acceptance limits; industrial/process/high-pressure pipework, gas, fire networks or utility/authority mains unless separately scoped and supported by applicable project sources.
Use and project setup
Project field: Project / package  ______________________________________________
Project field: State / territory and building class  ______________________________________________
Project field: Service type / material  ______________________________________________
Project field: Section from–to / drawing revision  ______________________________________________
Project field: Approved method / criterion ref  ______________________________________________
Project field: Instrument / serial / evidence  ______________________________________________
Project field: Test date / recorder / assigned witness  ______________________________________________
Project field: Repair / retest / closeout refs  ______________________________________________
Before inspection: Approved service drawings and section boundaries — Identify service type, material, endpoints, branches and current revisions.
Before inspection: Project-adopted test procedure and acceptance criteria — Supplies actual medium, pressure/time, readings, tolerances, preparation and test controls; none are invented here.
Before inspection: Project instrument and witness requirements — Assign instrument evidence, responsible roles, notification and any contractual release.
Before inspection: Service restoration/commissioning requirements — Defines whether flushing, disinfection, reinstatement or other closeout records apply.
How to use
1. Create one record per defined test section; do not combine sections with different materials, boundaries or approved methods.
2. Transcribe the governing procedure and exact criterion before testing, including units and reference. If absent, mark the criterion unresolved.
3. Identify actual isolation boundaries and setup from the approved method. The form does not direct how to pressurize or isolate a system.
4. Enter readings, times, instrument and observed leaks as they occur. Keep the original test result linked when repairs or retests follow.
5. Record project-assigned review, restoration and release evidence separately; signature alone is not a technical approval.
Important: No pressure, time, acceptance limit, test medium or safety step is prefilled. Use the current approved project procedure for the identified service and section, including its isolation and execution controls. Record actual values and any repair/retest without overwriting the original entry.


Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	WPT-01  Test section and approved test basis


	What to observe
	Service type and material, unique section boundaries, endpoints, branch/isolation points, drawing revision and test procedure/acceptance source.

	How to check
	Identify and mark the test section against current approved drawings and the project test schedule; confirm the assigned procedure and revision apply to this service/material.

	Acceptance basis
	Section limits, service identity, procedure and acceptance source are traceable and agreed before recording a test. No test value is supplied by this form.

	Reference to verify
	Current approved project drawings, specification, adopted service standard and inspection/test plan; record exact document, revision, clause/detail and affected segment.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Water service / material
	



	From–to / boundary IDs
	



	Drawing / isometric revision
	



	Procedure and criterion clause
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	WPT-02  Test medium, isolation and setup evidence


	What to observe
	Approved medium, isolation/boundary arrangement, connected components excluded or included, temporary caps/plugs, and any project-required preparation or notice.

	How to check
	Record the actual setup and link to the approved method; identify any exclusions, temporary arrangements and project-authorized witness/notification evidence.

	Acceptance basis
	Recorded setup matches the approved procedure for the defined section and identifies isolation boundaries and required parties. This record does not prescribe a test or safety procedure.

	Reference to verify
	Current approved project drawings, specification, adopted service standard and inspection/test plan; record exact document, revision, clause/detail and affected segment.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Actual test medium
	



	Isolation points / boundary sketch ref
	



	Included / excluded fixtures or components
	



	Notice / witness record ref
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	WPT-03  Instrument identity and pre-test reference


	What to observe
	Instrument type/ID/serial, range/unit, current project-required calibration or verification evidence, and any reference reading required by method.

	How to check
	Transcribe from instrument label and controlled equipment record; link the certificate/check record and note the date applicable to the test.

	Acceptance basis
	The instrument used is uniquely identified and any project/method-required equipment evidence is traceable; this template supplies no calibration interval or accuracy class.

	Reference to verify
	Current approved project drawings, specification, adopted service standard and inspection/test plan; record exact document, revision, clause/detail and affected segment.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Instrument type / serial
	



	Range and displayed unit
	



	Calibration / verification ref and date
	



	Pre-test check / reference reading
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	WPT-04  Actual readings, leakage observation and test interval


	What to observe
	Actual start/end readings with units and recorded times, intermediate readings required by procedure, visible leakage/pressure change observations, and criterion comparison source.

	How to check
	Enter contemporaneous actual readings and observations exactly as obtained; record the method-defined elapsed interval and compare only with the stated approved criterion.

	Acceptance basis
	Actual results, units, times and observations are complete and attributable to the identified section and instrument; conformity is assessed only against the entered project criterion.

	Reference to verify
	Current approved project drawings, specification, adopted service standard and inspection/test plan; record exact document, revision, clause/detail and affected segment.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Start reading / unit / time
	



	Intermediate reading(s) / unit / time
	



	End reading / unit / time
	



	Observed leakage / location
	



	Elapsed interval per approved method
	



	Criterion / clause / actual comparison
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Inspection record
Project: _____________________  Location / room / element: _____________________  Lot / area: _____________________
	WPT-05  Leak repair, retest and return-to-service evidence


	What to observe
	Leak/issue location, repair instruction and materials/reference, retest section/method, actual retest record and reinstatement/flush/commissioning evidence where required.

	How to check
	Link original test and each repair/retest in sequence. Record post-test restoration and any required project handover evidence without assuming it is always applicable.

	Acceptance basis
	Repairs and retests are traceable to the original section and disposition; required reinstatement and closeout documents are filed under the project process.

	Reference to verify
	Current approved project drawings, specification, adopted service standard and inspection/test plan; record exact document, revision, clause/detail and affected segment.

	Project criterion / actual approved document and revision
	
______________________________________________________________


	Record field
	Actual value / reference

	Issue / leak location
	



	Repair instruction / work ref
	



	Retest record ID / section
	



	Restoration evidence required / ref
	



	Disposition / closeout role and date
	



	Result / status (Pass / Fail / N/A / Pending)
	

	Inspector name / role / date
	

	Evidence / photo / report ref
	

	Issue / disposition / recheck evidence and date
	





Water service test reading and event log
Use one line per actual reading or event for the same identified test section. Preserve the initial result; record repairs and each retest under a linked record ID. Leave all actual entries blank until the event occurs.
Project / contract: ______________________________    Element / pour / lot: ______________________________    Date / shift: ____________________
Location / area: ______________________________    Record reference / revision: ______________________________
	Date / time
	Section / location
	Stage / event
	Procedure / criterion ref
	Instrument ID
	Actual reading / unit
	Observed leak / condition
	Repair / retest ref
	Recorder / status

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 
	 




Issues and corrective action
Project: _____________________  Location / room / element: _____________________  Inspection date: _____________________
	Item / date
	Issue and immediate action
	Disposition / corrective instruction
	Recheck evidence / date
	Responsible role / reference

	


	


	


	


	



	


	


	


	


	



	


	


	


	


	



	


	


	


	


	



	


	


	


	


	




Unresolved items: identify affected area, status, person notified, instruction / NCR reference and any condition before concealment or next work.


Water service test handover
Project: _____________________  Location / room / element: _____________________  Date: _____________________
Record inspection handover status
[  ] Record complete; source evidence linked
[  ] Issue, repair, retest or project decision remains open
[  ] Assigned project role review / disposition required
This record indexes the section test and evidence only; it does not design the service, define test conditions, certify compliance or grant contractual release.
Handover roles and references
Test recorder / role / date  ______________________________________________
Assigned plumbing reviewer / role / date  ______________________________________________
Contractual witness / release role and reference if applicable  ______________________________________________
Repair / NCR / retest / restoration evidence ref  ______________________________________________
Signatures record the named person’s stated role and entry only. They do not by themselves approve design, certify compliance, release a contractual control point or authorize the next activity.


Source notes
These references explain topic and record design. They do not supply universal project acceptance values. Confirm the contract documents, applicable jurisdiction and approved product/system before use.
ABCB, NCC 2022 Volume Three — Plumbing Code of Australia
Role: Official scope and jurisdictional topic framework; does not provide project-specific field test acceptance values.
Locator: Section B water services and Section C sanitary plumbing and drainage; volume includes jurisdiction schedules.
Source URL: https://ncc.abcb.gov.au/editions/ncc-2022/adopted/volume-three
ABCB, NCC 2022 Volume Three Schedule 2 — Referenced documents
Role: Reference-edition pointer only; full Standards not inspected and project adoption must be checked.
Locator: AS/NZS 3500 Parts 1–4:2021 titles and NCC clause pointers by service type.
Source URL: https://ncc.abcb.gov.au/editions/ncc-2022/adopted/volume-three/2-referenced-documents/referenced-documents
ABCB, Editions of the National Construction Code
Role: Edition/adoption context; check actual jurisdiction, transition and project approvals.
Locator: NCC 2022 Amendment 2 adoption and edition transition notes.
Source URL: https://ncc.abcb.gov.au/editions-national-construction-code
WA Plumbers Licensing Board, Pipe sizing and commissioning
Role: WA-specific topic support for section isolation, pressure-test readings, leakage repair and retest. No numeric settings or procedure are transferred to this general record; verify current applicable project and jurisdiction requirements.
Locator: Version 4, May 2023: page 4 Testing and commissioning of water services; page 5 WA scope notes
Source URL: https://www.wa.gov.au/media/54256/download
https://itp.cavoren.net/checklists/water-pressure-test/  |  Project: __________________________  |  Page 




