Water Services Installation ITP Template
Original editable baseline for ordinary building cold-water, heated-water and non-drinking water service pipework where selected. Covers product evidence, service routing, jointing, project-specified testing, conditional flushing/disinfection, operational checks and handover. Excludes fire-fighting, gas, process/high-pressure, HVAC, pools, off-site utility mains and specialist treatment plant. System selection and all numeric criteria must come from applicable authority, approved design and contract.
	Project
	[Enter project / state / parties]

	Package
	water-services

	Document / revision
	[Enter controlled number and revision]

	Issue purpose
	For review - proposed editable baseline

	Boundary
	Complete against project documents; remove out-of-scope activities.


Read before use
This is a reusable proposed baseline, not an approved project plan or completed inspection record.
Enter actual acceptance criteria, source revisions/locators, lot basis, frequency, roles and contractual control points from the project. No numeric limit, test result, qualification, signature or client release has been supplied.
Confirm scope and remove or mark conditional rows that do not apply. Resolve missing or conflicting decisions with the assigned project authority.
Complete the matching blank Record Prompts only when actual work occurs; retain source certificates and original specialist reports.
Project inputs to resolve
Jurisdiction and authority basis: [Enter project source / decision] State/territory, local plumbing regulator and applicable adoption/variations. Confirm current legal requirements.
Approved service drawings and revisions: [Enter project source / decision] Identify plans, risers/isometrics, schedules, details and any approved design revisions.
Project specification and adopted standards: [Enter project source / decision] Record exact contract sources, revisions and adopted editions; do not assume the current edition is the contract edition.
Approved product and material schedule: [Enter project source / decision] Identify approved pipe, fittings, joints, valves and product evidence applicable to this service.
Licensed roles, inspections and release authority: [Enter project source / decision] Identify performing/reviewing roles, regulatory inspections, notification, contractual H/W points and release authority.
Project records and handover requirements: [Enter project source / decision] Identify required test sheets, as-builts, certificates, commissioning and dossier index.
Project-specific test method and acceptance: [Enter project source / decision] Enter method, test medium, limits, duration, section/lot and source from applicable standard/specification/authority.
Service boundaries and connection interfaces: [Enter project source / decision] Identify property connection, downstream/upstream party, utility/network owner and excluded systems.
Flushing, disinfection and water quality requirements: [Enter project source / decision] Confirm whether required for this system and identify approved procedure, limits, sampling and disposal.


Inspection and Test Plan
Proposed baseline. Replace prompts with controlled project criteria and references before project review.
WTR-01 · Service boundary and design release
	Inspection / test
	Confirm the included cold, heated and non-drinking water systems, tie-in points and work boundaries before installation.

	Method
	Compare approved service drawings, schedules, scope and interface register; distinguish potable/non-potable, cold/heated services, utility work and excluded fire/process systems.

	Acceptance condition
	Only identified services and current approved drawings are released; unresolved design, cross-connection or point-of-connection decisions are recorded for the responsible designer/authority. Project basis: [Enter Approved service drawings and revisions]; [Enter Service boundaries and connection interfaces]; [Enter Jurisdiction and authority basis].

	Reference / locator
	Topic guidance only; see Source Register. Enter the actual project document, revision and locator.

	Trigger / frequency
	Proposed: At the identified item / lot before the next step that would obscure or change the evidence; confirm project-defined coverage and timing.

	Responsibility
	Proposed: Assigned licensed plumbing contractor performs and records; reviewer / regulator acts only within documented authority. Project role basis: [Enter Licensed roles, inspections and release authority]

	Point / external party
	TBC; Proposed: [Enter project-assigned reviewing / release authority]

	Notice / release
	Proposed: Confirm project notice recipient, evidence, timing and release authority; no external control point is assigned.

	Record
	Water service scope and interface register

	Applicability / remarks
	Core for water-service package. Proposed baseline. Confirm applicability and replace with controlled project requirement.





WTR-02 · Product approval and delivery check
	Inspection / test
	Check pipe, fittings, valves and devices against the approved service schedule and applicable evidence-of-suitability requirements.

	Method
	Match product identity, size/material, pressure/service designation and required certification/document references to approved submittals; segregate mismatched or damaged products.

	Acceptance condition
	Products match approved project schedule and required evidence is available for the intended service and jurisdiction. No product approval is inferred from this template. Project basis: [Enter Approved product and material schedule]; [Enter Project specification and adopted standards].

	Reference / locator
	Topic guidance only; see Source Register. Enter the actual project document, revision and locator.

	Trigger / frequency
	Proposed: At the identified item / lot before the next step that would obscure or change the evidence; confirm project-defined coverage and timing.

	Responsibility
	Proposed: Assigned licensed plumbing contractor performs and records; reviewer / regulator acts only within documented authority. Project role basis: [Enter Licensed roles, inspections and release authority]

	Point / external party
	TBC; Proposed: [Enter project-assigned reviewing / release authority]

	Notice / release
	Proposed: Confirm project notice recipient, evidence, timing and release authority; no external control point is assigned.

	Record
	Water product receipt and approval register

	Applicability / remarks
	When water-service products are supplied for installation. Proposed baseline. Confirm applicability and replace with controlled project requirement.





WTR-03 · Set-out, support and service separation
	Inspection / test
	Verify installed route, identification and supports against approved drawings and service coordination before concealment.

	Method
	Walk the installed section; compare route, levels/clearances, support details, sleeves and service identification to controlled drawings and coordination requirements; record deviations.

	Acceptance condition
	Installed route and support/interface details agree with approved documents; separation, access and identification requirements are resolved from project sources. Project basis: [Enter Approved service drawings and revisions]; [Enter Project specification and adopted standards].

	Reference / locator
	Topic guidance only; see Source Register. Enter the actual project document, revision and locator.

	Trigger / frequency
	Proposed: At the identified item / lot before the next step that would obscure or change the evidence; confirm project-defined coverage and timing.

	Responsibility
	Proposed: Assigned licensed plumbing contractor performs and records; reviewer / regulator acts only within documented authority. Project role basis: [Enter Licensed roles, inspections and release authority]

	Point / external party
	TBC; Proposed: [Enter project-assigned reviewing / release authority]

	Notice / release
	Proposed: Confirm project notice recipient, evidence, timing and release authority; no external control point is assigned.

	Record
	Water service installation and pre-cover record

	Applicability / remarks
	Where concealed or supported water pipework is installed. Proposed baseline. Confirm applicability and replace with controlled project requirement.





WTR-04 · Jointing and concealed workmanship
	Inspection / test
	Inspect completed joints and fittings while accessible, before insulation or enclosure.

	Method
	Verify joint type and installer/process evidence against manufacturer instructions and approved method; visually inspect accessible joints and record defects and repair references.

	Acceptance condition
	Jointing method and workmanship meet approved product instructions and project criteria; all identified defects are dispositioned before concealment. Project basis: [Enter Approved product and material schedule]; [Enter Project specification and adopted standards].

	Reference / locator
	Topic guidance only; see Source Register. Enter the actual project document, revision and locator.

	Trigger / frequency
	Proposed: At the identified item / lot before the next step that would obscure or change the evidence; confirm project-defined coverage and timing.

	Responsibility
	Proposed: Assigned licensed plumbing contractor performs and records; reviewer / regulator acts only within documented authority. Project role basis: [Enter Licensed roles, inspections and release authority]

	Point / external party
	TBC; Proposed: [Enter project-assigned reviewing / release authority]

	Notice / release
	Proposed: Confirm project notice recipient, evidence, timing and release authority; no external control point is assigned.

	Record
	Water joint and pre-concealment inspection log

	Applicability / remarks
	For installed joints that will become inaccessible. Proposed baseline. Confirm applicability and replace with controlled project requirement.





WTR-05 · Pressure test readiness and isolation
	Inspection / test
	Confirm each test section, boundaries, compatible test setup and protection of connected components before testing.

	Method
	Review approved test procedure; verify section limits, gauge/instrument identification and calibration status if required, isolated appliances, test medium and safety controls.

	Acceptance condition
	Test section and procedure match project-approved test plan and applicable service requirements; vulnerable components are protected and setup is recorded before pressurisation. Project basis: [Enter Project-specific test method and acceptance]; [Enter Project specification and adopted standards].

	Reference / locator
	Topic guidance only; see Source Register. Enter the actual project document, revision and locator.

	Trigger / frequency
	Proposed: At the identified item / lot before the next step that would obscure or change the evidence; confirm project-defined coverage and timing.

	Responsibility
	Proposed: Assigned licensed plumbing contractor performs and records; reviewer / regulator acts only within documented authority. Project role basis: [Enter Licensed roles, inspections and release authority]

	Point / external party
	TBC; Proposed: [Enter project-assigned reviewing / release authority]

	Notice / release
	Proposed: Confirm project notice recipient, evidence, timing and release authority; no external control point is assigned.

	Record
	Water pressure test setup record

	Applicability / remarks
	When a pressure test is specified for the installed service. Proposed baseline. Confirm applicability and replace with controlled project requirement.





WTR-06 · Pressure test and defect closeout
	Inspection / test
	Record the specified water-service test result and verify repair/retest evidence where required.

	Method
	Perform the approved test for the defined section; record actual medium, set conditions, start/end readings, times, observed leakage and test instrument; repair and repeat per approved procedure.

	Acceptance condition
	Actual results satisfy only the project-approved acceptance criteria and authority pathway; failed tests remain open until documented repair and accepted retest. Do not apply WA example values unless expressly adopted. Project basis: [Enter Project-specific test method and acceptance]; [Enter Jurisdiction and authority basis].

	Reference / locator
	Topic guidance only; see Source Register. Enter the actual project document, revision and locator.

	Trigger / frequency
	Proposed: At the identified item / lot before the next step that would obscure or change the evidence; confirm project-defined coverage and timing.

	Responsibility
	Proposed: Assigned licensed plumbing contractor performs and records; reviewer / regulator acts only within documented authority. Project role basis: [Enter Licensed roles, inspections and release authority]

	Point / external party
	TBC; Proposed: [Enter project-assigned reviewing / release authority]

	Notice / release
	Proposed: Confirm project notice recipient, evidence, timing and release authority; no external control point is assigned.

	Record
	Water service test and retest certificate

	Applicability / remarks
	When the specified test is applicable. Proposed baseline. Confirm applicability and replace with controlled project requirement.





WTR-07 · Flushing and disinfection, where required
	Inspection / test
	Determine and complete project-required flushing, disinfection and water-quality checks before service use.

	Method
	Confirm system type, scope and written procedure; flush/disinfect only where required and by approved method; record water quality samples/results, disposal and clearance where specified.

	Acceptance condition
	Applicable flushing/disinfection and water-quality evidence meets authority and project requirements; where not required, the basis is recorded. No universal disinfection trigger, dose or residual is supplied. Project basis: [Enter Flushing, disinfection and water quality requirements]; [Enter Jurisdiction and authority basis].

	Reference / locator
	Topic guidance only; see Source Register. Enter the actual project document, revision and locator.

	Trigger / frequency
	Proposed: At the identified item / lot before the next step that would obscure or change the evidence; confirm project-defined coverage and timing.

	Responsibility
	Proposed: Assigned licensed plumbing contractor performs and records; reviewer / regulator acts only within documented authority. Project role basis: [Enter Licensed roles, inspections and release authority]

	Point / external party
	TBC; Proposed: [Enter project-assigned reviewing / release authority]

	Notice / release
	Proposed: Confirm project notice recipient, evidence, timing and release authority; no external control point is assigned.

	Record
	Water flushing, disinfection and sampling record

	Applicability / remarks
	Conditional on service type, jurisdiction and project procedure. Proposed baseline. Confirm applicability and replace with controlled project requirement.





WTR-08 · Operational checks and service identification
	Inspection / test
	Check completed valves, outlets, controls, labels and access against approved schedules and operation requirements.

	Method
	Operate each scheduled item; verify intended service identification, access/isolation, flow direction and documented function; record exceptions and closeout actions.

	Acceptance condition
	Installed items match approved schedule and perform as specified; access and service identification are maintained and defects are closed. Project basis: [Enter Approved service drawings and revisions]; [Enter Project specification and adopted standards].

	Reference / locator
	Topic guidance only; see Source Register. Enter the actual project document, revision and locator.

	Trigger / frequency
	Proposed: At the identified item / lot before the next step that would obscure or change the evidence; confirm project-defined coverage and timing.

	Responsibility
	Proposed: Assigned licensed plumbing contractor performs and records; reviewer / regulator acts only within documented authority. Project role basis: [Enter Licensed roles, inspections and release authority]

	Point / external party
	TBC; Proposed: [Enter project-assigned reviewing / release authority]

	Notice / release
	Proposed: Confirm project notice recipient, evidence, timing and release authority; no external control point is assigned.

	Record
	Water service functional check and asset register

	Applicability / remarks
	At completion for included water services. Proposed baseline. Confirm applicability and replace with controlled project requirement.





WTR-09 · Regulatory inspection and handover
	Inspection / test
	Confirm required authority notifications, inspection outcomes and service records are complete for handover.

	Method
	Reconcile regulator/utility approvals, certificates, approved deviations, test/flush results, marked-up drawings and operation information against the project dossier index.

	Acceptance condition
	All required project and jurisdiction records are indexed; outstanding authority conditions, defects or exclusions are visible and not represented as accepted. Project basis: [Enter Licensed roles, inspections and release authority]; [Enter Project records and handover requirements].

	Reference / locator
	Topic guidance only; see Source Register. Enter the actual project document, revision and locator.

	Trigger / frequency
	Proposed: At the identified item / lot before the next step that would obscure or change the evidence; confirm project-defined coverage and timing.

	Responsibility
	Proposed: Assigned licensed plumbing contractor performs and records; reviewer / regulator acts only within documented authority. Project role basis: [Enter Licensed roles, inspections and release authority]

	Point / external party
	TBC; Proposed: [Enter project-assigned reviewing / release authority]

	Notice / release
	Proposed: Confirm project notice recipient, evidence, timing and release authority; no external control point is assigned.

	Record
	Water services commissioning and handover dossier index

	Applicability / remarks
	Core where required by contract or authority. Proposed baseline. Confirm applicability and replace with controlled project requirement.





Blank matching record prompts
Complete the actual date, observation, result and responsible roles during the work. Blank cells are intentional; this template contains no completed inspection or approval.
WTR-01 · Service boundary and design release
	Field
	Actual entry / evidence

	Service/system ID
	

	Drawing and revision
	

	Tie-in / work boundary
	

	Open decision reference
	

	Date / location / lot
	

	Actual observation / result / unit
	

	Original evidence / report reference
	

	Disposition / corrective action / recheck
	

	Performed by / date
	

	Reviewed / decision reference
	





WTR-02 · Product approval and delivery check
	Field
	Actual entry / evidence

	Product / component
	

	Service and location
	

	Approval / certification reference
	

	Condition / disposition
	

	Date / location / lot
	

	Actual observation / result / unit
	

	Original evidence / report reference
	

	Disposition / corrective action / recheck
	

	Performed by / date
	

	Reviewed / decision reference
	





WTR-03 · Set-out, support and service separation
	Field
	Actual entry / evidence

	Section / location
	

	Drawing and revision
	

	Support / restraint reference
	

	Deviation / RFI reference
	

	Date / location / lot
	

	Actual observation / result / unit
	

	Original evidence / report reference
	

	Disposition / corrective action / recheck
	

	Performed by / date
	

	Reviewed / decision reference
	





WTR-04 · Jointing and concealed workmanship
	Field
	Actual entry / evidence

	Section / location
	

	Joint type / installer
	

	Observation / defect
	

	Repair / reinspection reference
	

	Date / location / lot
	

	Actual observation / result / unit
	

	Original evidence / report reference
	

	Disposition / corrective action / recheck
	

	Performed by / date
	

	Reviewed / decision reference
	





WTR-05 · Pressure test readiness and isolation
	Field
	Actual entry / evidence

	Test section
	

	Procedure / revision
	

	Gauge ID / calibration reference
	

	Isolation and protection check
	

	Date / location / lot
	

	Actual observation / result / unit
	

	Original evidence / report reference
	

	Disposition / corrective action / recheck
	

	Performed by / date
	

	Reviewed / decision reference
	





WTR-06 · Pressure test and defect closeout
	Field
	Actual entry / evidence

	Test section
	

	Actual readings / result
	

	Actual start/end time
	

	Defect / repair / retest ref.
	

	Date / location / lot
	

	Actual observation / result / unit
	

	Original evidence / report reference
	

	Disposition / corrective action / recheck
	

	Performed by / date
	

	Reviewed / decision reference
	





WTR-07 · Flushing and disinfection, where required
	Field
	Actual entry / evidence

	System / section
	

	Approved procedure reference
	

	Sample point / lab result
	

	Clearance / disposition
	

	Date / location / lot
	

	Actual observation / result / unit
	

	Original evidence / report reference
	

	Disposition / corrective action / recheck
	

	Performed by / date
	

	Reviewed / decision reference
	





WTR-08 · Operational checks and service identification
	Field
	Actual entry / evidence

	Valve / outlet / control ID
	

	Location / service
	

	Observed function
	

	Defect / closeout reference
	

	Date / location / lot
	

	Actual observation / result / unit
	

	Original evidence / report reference
	

	Disposition / corrective action / recheck
	

	Performed by / date
	

	Reviewed / decision reference
	





WTR-09 · Regulatory inspection and handover
	Field
	Actual entry / evidence

	Record / certificate
	

	Document number / revision
	

	Status / authority
	

	Open condition / owner
	

	Date / location / lot
	

	Actual observation / result / unit
	

	Original evidence / report reference
	

	Disposition / corrective action / recheck
	

	Performed by / date
	

	Reviewed / decision reference
	





Topic guidance sources and limitations
Australian Building Codes Board, NCC 2022 Volume Three — Plumbing Code of Australia
Accessed 2026-10-07; Volume Three index: Section B Water services, Section C Sanitary plumbing and drainage systems, state/territory schedules and Schedule 2 referenced documents.
https://ncc.abcb.gov.au/editions/ncc-2022/adopted/volume-three
Official national framework and source locator. State adoption, variations, application and project compliance pathway must be confirmed; NCC edition is not assumed to be the contract edition.
Australian Building Codes Board, NCC 2022 Volume Three — Schedule 2 Referenced documents
Accessed 2026-10-07; entries AS/NZS 3500 Part 1:2021 (B1D3 etc.), Part 2:2021 (C1/C2 provisions) and Part 3:2021 (F1D3, H2D2/H2D6 and 7.4.3).
https://ncc.abcb.gov.au/editions/ncc-2022/adopted/volume-three/2-referenced-documents/referenced-documents
Confirms NCC 2022 referenced-document editions and provision cross-references only. Verify the edition actually adopted by the project jurisdiction and contract; full standards text was not used.
Australian Building Codes Board, NCC 2022 Volume Three — Section B Water services
Accessed 2026-10-07; index entries Part B1 Cold water services, B2 Heated water services, B3 Non-drinking water services, B5 Cross-connection control, B6 Rainwater services and B7 Rainwater storage.
https://ncc.abcb.gov.au/editions/ncc-2022/adopted/volume-three/b-water-services
Defines service group coverage and compliance topic routing; it does not set project-specific test methods, design values, hold points or blanket disinfection requirements.
WA Plumbers Licensing Board, Pipe sizing and commissioning
Version 4, May 2023: page 4 Testing and commissioning of water services flowchart; page 5 WA scope and adopted-code notes. Checked 7 October 2026.
https://www.wa.gov.au/media/54256/download
WA-specific technical example only. Its stated pressure/time and disinfection triggers are intentionally not reproduced as generic criteria; use only if confirmed applicable by jurisdiction, contract and service design.
ABCB WaterMark, What requires WaterMark?
Transcript: schedules of products/excluded products and matching certificate/product identity. Checked 7 October 2026.
https://watermark.abcb.gov.au/resources/videos/what-requires-watermark
Topic support for checking certification applicability and product identity; not every plumbing product requires WaterMark. No individual product or installation is certified by this template.
Topic guidance is provided for orientation only. Confirm applicable jurisdictional adoption, approved design and contract requirements. No cited source substitutes for the complete controlled project documents or licensed standards.
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